
diff -r 65e91466a14b -r b7e5ed8c1342 srsfenginestub/recognitionhwdevice/bwins/asrsrecognitionhwdeviceu.def
--- /dev/null	Thu Jan 01 00:00:00 1970 +0000
+++ b/srsfenginestub/recognitionhwdevice/bwins/asrsrecognitionhwdeviceu.def	Tue Sep 07 08:19:48 2010 +0300
@@ -0,0 +1,20 @@
+EXPORTS
+	??1CASRSHwDevice@@UAE@XZ @ 1 NONAME ; CASRSHwDevice::~CASRSHwDevice(void)
+	??1CASRSRecognitionHwDevice@@UAE@XZ @ 2 NONAME ; CASRSRecognitionHwDevice::~CASRSRecognitionHwDevice(void)
+	?Clear@CASRSHwDevice@@UAEXXZ @ 3 NONAME ; void CASRSHwDevice::Clear(void)
+	?Clear@CASRSRecognitionHwDevice@@UAEXXZ @ 4 NONAME ; void CASRSRecognitionHwDevice::Clear(void)
+	?CustomInterface@CASRSHwDevice@@UAEPAXVTUid@@@Z @ 5 NONAME ; void * CASRSHwDevice::CustomInterface(class TUid)
+	?CustomInterface@CASRSRecognitionHwDevice@@UAEPAXVTUid@@@Z @ 6 NONAME ; void * CASRSRecognitionHwDevice::CustomInterface(class TUid)
+	?GetRejection@CASRSRecognitionHwDevice@@QAEKXZ @ 7 NONAME ; unsigned long CASRSRecognitionHwDevice::GetRejection(void)
+	?InitRecognizerBEL@CASRSRecognitionHwDevice@@QAEXABVTDesC8@@ABVCSIModelBank@@@Z @ 8 NONAME ; void CASRSRecognitionHwDevice::InitRecognizerBEL(class TDesC8 const &, class CSIModelBank const &)
+	?InitRecognizerFEL@CASRSRecognitionHwDevice@@QAEXH@Z @ 9 NONAME ; void CASRSRecognitionHwDevice::InitRecognizerFEL(int)
+	?InitializeL@CASRSHwDevice@@UAEXXZ @ 10 NONAME ; void CASRSHwDevice::InitializeL(void)
+	?InitializeL@CASRSRecognitionHwDevice@@UAEXXZ @ 11 NONAME ; void CASRSRecognitionHwDevice::InitializeL(void)
+	?NewL@CASRSHwDevice@@SAPAV1@XZ @ 12 NONAME ; class CASRSHwDevice * CASRSHwDevice::NewL(void)
+	?NewL@CASRSRecognitionHwDevice@@SAPAV1@AAVMASRSRecognitionHwDeviceObserver@@@Z @ 13 NONAME ; class CASRSRecognitionHwDevice * CASRSRecognitionHwDevice::NewL(class MASRSRecognitionHwDeviceObserver &)
+	?SendSpeechData@CASRSRecognitionHwDevice@@QAEXAAVTPtrC8@@H@Z @ 14 NONAME ; void CASRSRecognitionHwDevice::SendSpeechData(class TPtrC8 &, int)
+	?SetNBest@CASRSRecognitionHwDevice@@QAEXK@Z @ 15 NONAME ; void CASRSRecognitionHwDevice::SetNBest(unsigned long)
+	?SetRejection@CASRSRecognitionHwDevice@@QAEXK@Z @ 16 NONAME ; void CASRSRecognitionHwDevice::SetRejection(unsigned long)
+	?StartRecognitionL@CASRSRecognitionHwDevice@@QAEXAAV?$RArray@I@@AAV?$RArray@H@@@Z @ 17 NONAME ; void CASRSRecognitionHwDevice::StartRecognitionL(class RArray<unsigned int> &, class RArray<int> &)
+	?StopRecognition@CASRSRecognitionHwDevice@@QAEXXZ @ 18 NONAME ; void CASRSRecognitionHwDevice::StopRecognition(void)
+




