
diff -r b7e5ed8c1342 -r e71858845f73 srsfenginestub/recognitionhwdevice/bwins/asrsrecognitionhwdeviceu.def
--- a/srsfenginestub/recognitionhwdevice/bwins/asrsrecognitionhwdeviceu.def	Tue Sep 07 08:19:48 2010 +0300
+++ /dev/null	Thu Jan 01 00:00:00 1970 +0000
@@ -1,20 +0,0 @@
-EXPORTS
-	??1CASRSHwDevice@@UAE@XZ @ 1 NONAME ; CASRSHwDevice::~CASRSHwDevice(void)
-	??1CASRSRecognitionHwDevice@@UAE@XZ @ 2 NONAME ; CASRSRecognitionHwDevice::~CASRSRecognitionHwDevice(void)
-	?Clear@CASRSHwDevice@@UAEXXZ @ 3 NONAME ; void CASRSHwDevice::Clear(void)
-	?Clear@CASRSRecognitionHwDevice@@UAEXXZ @ 4 NONAME ; void CASRSRecognitionHwDevice::Clear(void)
-	?CustomInterface@CASRSHwDevice@@UAEPAXVTUid@@@Z @ 5 NONAME ; void * CASRSHwDevice::CustomInterface(class TUid)
-	?CustomInterface@CASRSRecognitionHwDevice@@UAEPAXVTUid@@@Z @ 6 NONAME ; void * CASRSRecognitionHwDevice::CustomInterface(class TUid)
-	?GetRejection@CASRSRecognitionHwDevice@@QAEKXZ @ 7 NONAME ; unsigned long CASRSRecognitionHwDevice::GetRejection(void)
-	?InitRecognizerBEL@CASRSRecognitionHwDevice@@QAEXABVTDesC8@@ABVCSIModelBank@@@Z @ 8 NONAME ; void CASRSRecognitionHwDevice::InitRecognizerBEL(class TDesC8 const &, class CSIModelBank const &)
-	?InitRecognizerFEL@CASRSRecognitionHwDevice@@QAEXH@Z @ 9 NONAME ; void CASRSRecognitionHwDevice::InitRecognizerFEL(int)
-	?InitializeL@CASRSHwDevice@@UAEXXZ @ 10 NONAME ; void CASRSHwDevice::InitializeL(void)
-	?InitializeL@CASRSRecognitionHwDevice@@UAEXXZ @ 11 NONAME ; void CASRSRecognitionHwDevice::InitializeL(void)
-	?NewL@CASRSHwDevice@@SAPAV1@XZ @ 12 NONAME ; class CASRSHwDevice * CASRSHwDevice::NewL(void)
-	?NewL@CASRSRecognitionHwDevice@@SAPAV1@AAVMASRSRecognitionHwDeviceObserver@@@Z @ 13 NONAME ; class CASRSRecognitionHwDevice * CASRSRecognitionHwDevice::NewL(class MASRSRecognitionHwDeviceObserver &)
-	?SendSpeechData@CASRSRecognitionHwDevice@@QAEXAAVTPtrC8@@H@Z @ 14 NONAME ; void CASRSRecognitionHwDevice::SendSpeechData(class TPtrC8 &, int)
-	?SetNBest@CASRSRecognitionHwDevice@@QAEXK@Z @ 15 NONAME ; void CASRSRecognitionHwDevice::SetNBest(unsigned long)
-	?SetRejection@CASRSRecognitionHwDevice@@QAEXK@Z @ 16 NONAME ; void CASRSRecognitionHwDevice::SetRejection(unsigned long)
-	?StartRecognitionL@CASRSRecognitionHwDevice@@QAEXAAV?$RArray@I@@AAV?$RArray@H@@@Z @ 17 NONAME ; void CASRSRecognitionHwDevice::StartRecognitionL(class RArray<unsigned int> &, class RArray<int> &)
-	?StopRecognition@CASRSRecognitionHwDevice@@QAEXXZ @ 18 NONAME ; void CASRSRecognitionHwDevice::StopRecognition(void)
-




