{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Main","Key values"],"not_rendered":{"macros":1,"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Main","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"flags":["formulas_cached_only"]}
[{"$nulls":5},"DO NOT DELETE THIS SHEET. THE FUTURE CONVERSION SCRIPTS NEED THE TEMPLATE VERSION INFORMATION"]
[null,"Template version","2.0"]
[null,"Purpose"]
[null,"CenRep keys "]
[]
[null,"Entity"]
[null,"Owner"]
[null,"Version",{"v":2,"d":"2.00"}]
[]
[null,"Version History"]
[null,"Date","Version","Type","Author","Comments"]
[null,"2005-06-01",{"v":0.1,"d":"0.10"},null,null,"Local variation key added"]
[null,"2005-06-09",{"v":0.2,"d":"0.20"},null,null,"KVTLocalVariationFlags value changed. HideNumberEntryInVideoTelephonyUi feature enabled (bit mask 0x400)."]
[null,"2005-09-19",{"v":0.3,"d":"0.30"},null,null,"KVTLocalVariationFlags value changed to 1332 (dec). KVTLVFlagViewFinderMirroring feature enabled (bit mask 0x0020)."]
[null,"2005-10-06",{"v":0.4,"d":"0.40"},null,null,"KVTLocalVariationFlags value changed to 1908 (dec). KVTLVFlagDisableFrameWatcher and KVTLVFlagLargeViewfinder features enabled. Same values applited to S60 3.1"]
[null,"2005-12-07",{"v":0.5,"d":"0.50"},null,null,"Added KCRUidVTConfiguration UID and KVTVideoFrameRates key for video frame rate control in encoder. \nKVTLocalVariationFlags key default value in 3.1 is 3956 (KVTLVFlagVideoQualityControl is set on)."]
[null,"2006-04-07",{"v":0.6,"d":"0.60"},null,null,"Added KVTCameraLayout key"]
[null,"2006-04-10",{"v":0.7,"d":"0.70"},null,null,"Added Central Repository keys for VT codec configurations"]
[null,"2006-06-13",{"v":0.8,"d":"0.80"},null,"Mikko Bertin","New default values for KVTLocalVariationFlags is 20340  (KVTLVFlagRemoteFrameSkipping is set on).\nAdded S60 3.2 key values"]
[null,"2006-08-10",{"v":0.9,"d":"0.90"},null,"Mikko Bertin","Added KVTToolbarCommands key"]
[null,"2006-09-21",{"v":1,"d":"1.00"},null,"Mikko Bertin","KVTLocalVariationFlags key default value in 3.1/3.2 is 24436 (KVTLVFlagWNSRP is set on)."]
[null,"2006-10-04",{"v":1.1,"d":"1.10"},null,"Antti Turunen","Removed KVTLVFlagEnablePacketVideoProxy flag"]
[null,"2006-11-15",{"v":1.2,"d":"1.20"},null,"Mikko Bertin","KVTLocalVariationFlags key default value in 3.1/3.2 is 24438/24182 (KVTLVFlagCameraOptionsInMenu is set on)."]
[null,"2006-11-16",{"v":1.3,"d":"1.30"},null,"Pasi Rantenen","Removed KVTLVFlagSwapVideoCallWindows flag"]
[null,"2006-12-19",{"v":1.4,"d":"1.40"},null,"Mikko Bertin","Removed KVTLVFlagCameraOptionsInMenu flag, KVTLocalVariationFlags key default value in 3.2 changed to 7792"]
[null,"2007-03-05",{"v":1.5,"d":"1.50"},null,"Pasi Rantanen","Defined CDSP audio encoder to be used in 3.2."]
[null,"2007-03-13",{"v":1.6,"d":"1.60"},null,"Mikko Bertin","Updated video codec UIDs for S60 3.2 and added S60 5.0 values"]
[null,"2007-03-29",{"v":1.7,"d":"1.70"},null,"Mikko Bertin","Corrected video KVTVideoEncoderUIDs key values for 3.2 and 5.0"]
[null,"2007-05-07",{"v":1.8,"d":"1.80"},null,"Mikko Bertin","Codec processing delay control keys added from 3.1 onwards"]
[null,"2007-05-08",{"v":1.9,"d":"1.90"},null,"Mikko Bertin","Removed KVTToolbarCommands key and adjusted affected key values accordingly"]
[null,"                     16.05.2007",{"v":2,"d":"2.00"},null,"Lauri Lehti","KVTToolbarCommands key modified"]
[null,"2007-05-24",{"v":2.1,"d":"2.10"},null,"Mikko Bertin","Removed KVTLVFlagWNSRP local variation flag in 3.2 (always enabled). KVTLocalVariationFlags key value changed to 3696"]
[null,"                     18.06.2007",{"v":2.2,"d":"2.20"},null,"Lauri Lehti","KVTToolbarCommands' default value changed"]
[null,"2007-09-26",{"v":2.3,"d":"2.30"},null,"Mikko Bertin","Update 5.0 local variation key KVTLocalVariationFlags value due to flag removals"]
[null,"2007-10-23",{"v":2.4,"d":"2.40"},null,"Mikko Bertin","Updated 5.0 local variation key value due to flag re-ordering."]
[null,"2008-04-01",{"v":2.5,"d":"2.50"},null,"Mikko Bertin","Updated local variation key value to correspond to actual flag amount"]
[null,"2008-06-04",{"v":2.6,"d":"2.60"},null,"Mikko Bertin","Changed camera oriantation key valut to \"C1:PR C2:PR\" (always in portrait regardless of selected camera)"]
[null,"2008-06-10",{"v":2.7,"d":"2.70"},null,"Miia Onkalo","KVTLocalVariationFlags 5.0 default value changed to 2."]

{"sheet":"Key values","index":1,"n_rows":62,"n_cols":59,"rows_kept":62,"flags":["formulas_cached_only"]}
["Uid Name","Uid Value","Range From","Range To","Key Name","Key Int","Shared Data Name","Purpose","Removed","Platform Release","Variant Name","Def Value","Read  Only","Key Type","Backup","RFS","Cust Config","Owner","Related Features","AlwaysPass","NetworkServices","LocalServices","ReadUserData","WriteUserData","Location","ReadDeviceData","WriteDeviceData","ProtServ","DRM","SwEvent","PowerMgmt","AllFiles","DiskAdmin","NetworkControl","MultiMediaDD","CommDD","TCB","TrustedUI","UserEnvironment","SurroundingsDD","SID Read","SID Write","Yes","No","Must","Int","Real","Str","Bin","R","W","RW","elaf","apac","thai","japan","gsm","low_cost","Do not delete AN1 -> BC1, since they are used in the multichoise column validation"]
["KCRUidVTVariation","0x102072D0"]
[{"$nulls":9},"S60 3.0",{"$nulls":4},"No","No",null,"0x101F8681",null,"R"]
[{"$nulls":4},"KVTLocalVariationFlags","0x00000001",null,"Bitmask for Video Telephony local variation.",{"$nulls":4},"Yes","Int"]
[{"$nulls":9},"S60 3.0",null,1908,null,null,"No","No","Must",null,null,"R"]
[{"$nulls":9},"S60 3.1",null,8054,null,null,"No","No","Must",null,null,"R"]
[{"$nulls":9},"S60 3.2",null,3696,null,null,"No","No","Must",null,null,"R"]
[{"$nulls":9},"S60 5.0",null,2,null,null,"No","No","Must",null,null,"R"]
[]
["KCRUidVTConfiguration","0x10281872"]
[{"$nulls":9},"S60 3.1",{"$nulls":4},"No","No",null,"0x101F8681",null,"R"]
[{"$nulls":4},"KVTVideoFrameRates","0x00000001",null,"Values that control minimum, normal and maximum frames for video encoder. Values are in range 0 and 31 and separated by space. Example for key value is \"5 10 15\".",{"$nulls":4},"Yes","Str"]
[{"$nulls":9},"S60 3.1",null,"5 10 15",null,null,"No","No","Yes",null,null,"R"]
[{"$nulls":9},"S60 3.2",null,"5 10 15",null,null,"No","No","Yes",null,null,"R"]
[{"$nulls":9},"S60 5.0",null,"5 10 15",null,null,"No","No","Yes",null,null,"R"]
[]
[{"$nulls":4},"KVTCameraLayout","0x00000002",null,"Defines layout (screen orientation) used by Video Telephone application per active camera.\nEach camera has one of the following values:\n1) \"LS\" = Landscape\n2) \"PR\" = Portrait\n3) \"OL\" = Obey layout in specific device mode (normal operation)\nCamera values are:\n1) \"C1\" = VT primary camera (inwards)\n2) \"C2\" = VT secondary camera (outwards)\nExample value (portrait for cam1, landscape for cam2):\nC1:PR C2:LS",{"$nulls":4},"Yes","Str"]
[{"$nulls":9},"S60 3.1",null,"C1:OL C2:OL",null,null,"No","No","Yes",null,null,"R"]
[{"$nulls":9},"S60 3.2",null,"C1:OL C2:OL",null,null,"No","No","Yes",null,null,"R"]
[{"$nulls":9},"S60 5.0",null,"C1:PR C2:PR",null,null,"No","No","Yes",null,null,"R"]
[]
[{"$nulls":4},"KVTVideoEncoderUIDs","0x00000003",null,"Lists implementation UIDs for MPEG4, H.263 and H.264 encoders for video telephony in hexadecimal separated by space",{"$nulls":4},"Yes","Str"]
[{"$nulls":9},"S60 3.1",null,"00000000 00000000 00000000",null,null,"No","No","Must",null,null,"R"]
[{"$nulls":9},"S60 3.2",null,"101f86d5 101f850a 20001c13",null,null,"No","No","Must",null,null,"R"]
[{"$nulls":9},"S60 5.0",null,"101f86d5 101f850a 20001c13",null,null,"No","No","Must",null,null,"R"]
[{"$nulls":4},"KVTVideoDecoderUIDs","0x00000004",null,"Lists implementation UIDs for MPEG4, H.263 and H.264 decoders for video telephony in hexadecimal separated by space",{"$nulls":4},"Yes","Str"]
[{"$nulls":9},"S60 3.1",null,"00000000 00000000 00000000",null,null,"No","No","Must",null,null,"R"]
[{"$nulls":9},"S60 3.2",null,"00000000 00000000 102073ef",null,null,"No","No","Must",null,null,"R"]
[{"$nulls":9},"S60 5.0",null,"00000000 00000000 102073ef",null,null,"No","No","Must",null,null,"R"]
[]
[{"$nulls":4},"KVTAudioEncoderUIDs","0x00000005",null,"Lists implementation UIDs for AMR-NB and future audio encoders for video telephony (in hex, separated by space)",{"$nulls":4},"Yes","Str"]
[{"$nulls":9},"S60 3.1",null,"00000000 00000000",null,null,"No","No","Must",null,null,"R"]
[{"$nulls":9},"S60 3.2",null,"1020659E 00000000",null,null,"No","No","Must",null,null,"R"]
[{"$nulls":9},"S60 5.0",null,"1020659E 00000000",null,null,"No","No","Must",null,null,"R"]
[]
[{"$nulls":4},"KVTAudioDecoderUIDs","0x00000006",null,"Lists implementation UIDs for AMR-NB and future audio decoders for video telephony (in hex, separated by space)",{"$nulls":4},"Yes","Str"]
[{"$nulls":9},"S60 3.1",null,"00000000 00000000",null,null,"No","No","Must",null,null,"R"]
[{"$nulls":9},"S60 3.2",null,"00000000 00000000",null,null,"No","No","Must",null,null,"R"]
[{"$nulls":9},"S60 5.0",null,"00000000 00000000",null,null,"No","No","Must",null,null,"R"]
[]
[{"$nulls":4},"KVTVideoEncoderDelay","0x00000007",null,"Lists processing delay for MPEG4, H.263 and H.264 encoders for video telephony in unsigned 32-bit integers separated by space",{"$nulls":4},"Yes","Str"]
[{"$nulls":9},"S60 3.1",null,"0 0 0",null,null,"No","No","Yes",null,null,"R"]
[{"$nulls":9},"S60 3.2",null,"0 0 0",null,null,"No","No","Yes",null,null,"R"]
[{"$nulls":9},"S60 5.0",null,"0 0 0",null,null,"No","No","Yes",null,null,"R"]
[]
[{"$nulls":4},"KVTVideoDecoderDelay","0x00000008",null,"Lists processing delay for MPEG4, H.263 and H.264 decoders for video telephony in unsigned 32-bit integers separated by space",{"$nulls":4},"Yes","Str"]
[{"$nulls":9},"S60 3.1",null,"0 0 0",null,null,"No","No","Yes",null,null,"R"]
[{"$nulls":9},"S60 3.2",null,"0 0 0",null,null,"No","No","Yes",null,null,"R"]
[{"$nulls":9},"S60 5.0",null,"0 0 0",null,null,"No","No","Yes",null,null,"R"]
[]
[{"$nulls":4},"KVTAudioEncoderDelay","0x00000009",null,"Lists processing delay for AMR-NB and future audio encoders for video telephony (in unsigned 32-bit integers, separated by space)",{"$nulls":4},"Yes","Str"]
[{"$nulls":9},"S60 3.1",null,"0 0",null,null,"No","No","Yes",null,null,"R"]
[{"$nulls":9},"S60 3.2",null,"0 0",null,null,"No","No","Yes",null,null,"R"]
[{"$nulls":9},"S60 5.0",null,"0 0",null,null,"No","No","Yes",null,null,"R"]
[]
[{"$nulls":4},"KVTAudioDecoderDelay","0x0000000A",null,"Lists processing delay for AMR-NB and future audio decoders for video telephony (in unsigned 32-bit integers, separated by space)",{"$nulls":4},"Yes","Str"]
[{"$nulls":9},"S60 3.1",null,"0 0",null,null,"No","No","Yes",null,null,"R"]
[{"$nulls":9},"S60 3.2",null,"0 0",null,null,"No","No","Yes",null,null,"R"]
[{"$nulls":9},"S60 5.0",null,"0 0",null,null,"No","No","Yes",null,null,"R"]
[]
[{"$nulls":4},"KVTToolbarCommands","0x0000000B",null,"Specifies number of toolbar buttons.",{"$nulls":4},"Yes","Int"]
[{"$nulls":9},"S60 3.2",null,6,null,null,"No","No","Yes",null,null,"R"]