This file contains a list of UID's allocated for use by cone.
Please use ones in this list before getting some more allocated.

Cone UID's:			Decimal		Hexadecimal
MCoeControlStateObserver	271080005	10285A45
Start Range moved to SSMA	271080006	10285A46
End Range moved to SSMA		271080020	10285A54
