[test0]

# Sim.tsy accepts a message sent from the emulator, checks that it is what is expected, and then ACK's.
# EmailToAddress=UserName<test@test.com>
# SentToAddress=+44111111111


IndicatorCheckPeriod= 1
NetworkInfo= TEST, Network0, Test, Test, Test, 5
RegStatus= 5,5

NotifySignalStrengthChangeCap= 1
	# Part 1 of msg
SmsTx= 55000B914411111111F13200A7A0050003000201AAF3B2DC196E9779F4F29C0EA097E774D7F8DDF6A1A8E8F41C949E83CC69F99C0E12CBD72E10159D9E83D273D0BC3C7EBBC920B17CED0251D1E939283D07D1D16939192496AF5D202A3A3D07A5E7201A1D0D12CBD72E10159D9E83D273508D8E0689E56B17888A4ECF41E939C8464783C4F2B50B4445A7E7A0F41C74A3A34162F9DA05A2A2D3, +358405202000, 0, 010010807141731480, 0
	#         r**********        ccm***********************
	# r =Recipients= +44111111111
	# cc = message count
	# m = Message= UserName<test@test.com>
	# 55000B914411111111F10004A72A03200126456D61696C546F416464726573733A557365724E616D653C7465737440746573742E636F6D3E
	# Note exta E in email address to make the number of hex bytes even.
	#  +358405202000 =  sca = service centre address and is not actually used by the sim.tsy for anything (at the moment).
	# 1 = MsgRef
	# 02070100 = SubmitReportPdu. Basically an ACK	
	# SmsTx	<pdu>, <sca>, <MsgRef> <SubmitReportPdu> <ExpectedError>
