{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Main","Key values"],"not_rendered":{"macros":1,"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Main","index":0,"n_rows":12,"n_cols":6,"rows_kept":12,"flags":["formulas_cached_only"]}
[{"$nulls":5},"DO NOT DELETE THIS SHEET. THE FUTURE CONVERSION SCRIPTS NEED THE TEMPLATE VERSION INFORMATION"]
[null,"Template version","2.0"]
[null,"Purpose"]
[null,"CenRep keys "]
[]
[null,"Entity","Synchronization & Provisioning team"]
[null,"Owner","pekka.paadar@nokia.com"]
[null,"Version",{"v":1,"d":"1.00"}]
[]
[null,"Version History"]
[null,"Date","Version","Type","Author","Comments"]
[null,"2005-10-06",{"v":1,"d":"1.00"},"Proposal","Pekka Paadar","Initial version"]

{"sheet":"Key values","index":1,"n_rows":26,"n_cols":59,"rows_kept":26,"flags":["formulas_cached_only"]}
["Uid Name","Uid Value","Range From","Range To","Key Name","Key Int","Shared Data Name","Purpose","Removed","Platform Release","Variant Name","Def Value","Read  Only","Key Type","Backup","RFS","Cust Config","Owner","Related Features","AlwaysPass","NetworkServices","LocalServices","ReadUserData","WriteUserData","Location","ReadDeviceData","WriteDeviceData","ProtServ","DRM","SwEvent","PowerMgmt","AllFiles","DiskAdmin","NetworkControl","MultiMediaDD","CommDD","TCB","TrustedUI","UserEnvironment","SurroundingsDD","SID Read","SID Write","Yes","No","Must","Int","Real","Str","Bin","R","W","RW","elaf","apac","thai","japan","gsm","low_cost","Do not delete AN1 -> BC1, since they are used in the multichoise column validation"]
["KCRUidFotaServer","0x102072C4",{"$nulls":5},"fotaserver configuration keys"]
[{"$nulls":9},"s60 3.1",{"$nulls":4},"No","no","must","0x102072C4",null,"R",{"$nulls":6},"W"]
[{"$nulls":4},"KSimulateUpdateAgent","0x00000001",null,"Should update agent be simulated by fotaserver?",{"$nulls":4},"Yes","Int"]
[{"$nulls":9},"s60 3.1",null,"0x1",null,null,"No","No","Yes",null,"__SYNCML_DM_FOTA","R"]
[{"$nulls":4},"KSilentOmaDlUIBehavior","0x00000002",null,"Determines the UI behavior of OMA DL during silent DM session\nValues:\n0 (default)  -  Descriptor Off, Download Progress bar Off\n1  -  DD Descriptor Off, Download Progress bar On\n2  -  DD Descriptor On, Download Progress bar Off\n3  -  DD Descriptor On, Download Progress bar On",{"$nulls":4},"Yes","Int"]
[{"$nulls":9},"s60 3.2",null,"0x0",null,null,"No","No","Yes","0x102072C4",null,"R"]
[{"$nulls":4},"KGenericAlertResendAfterBoot","0x00000003",null,"Flag to enable/disable the  feature ,..\n\"Send Generic alert after device reboots\"\nAllowed values\n1  , 0 \nIf value is  1 : \n FOTA status report (through generic alert – 1226), after the phone reboot will be sent if there is pending status report.\nIf value is 0: \nGeneric alert will not be sent after phone reboot.",{"$nulls":4},"Yes","Int"]
[{"$nulls":9},"s60 3.2",null,"0x0",null,null,"No","No","Yes","0x102072C4",null,"R"]
[{"$nulls":4},"KGenericAlertRetries","0x00000004",null,"Flag to configure number of retries for sending GA in failure cases.\nDefault value is 3. \n",{"$nulls":4},"Yes","Int"]
[{"$nulls":9},"s60 3.2",null,"0x3",null,null,"No","No","Yes","0x102072C4",null,"R"]
[{"$nulls":4},"KFotaUpdateState","0x00000005",null,"Determines state of fota update.\n0 - Default , no action taken. \n1 - Firmware update/GA \n2. Download Interrupted\n",{"$nulls":4},"No","Int"]
[{"$nulls":9},"s60 3.2",null,"0x0",null,null,"No","No","No","0x102072C4",null,"R",{"$nulls":6},"W"]
[{"$nulls":4},"KSuspendResumeFeatureSupported","0x00000006",null,"Determines whether the Fota Suspend and Resume Feature is supported or not.\n0 (default in S60 3.2) - Feature OFF \n1  (default in S60 5.0) - Feature ON",{"$nulls":4},"No","Int"]
[{"$nulls":9},"s60 3.2",null,"0x0",null,null,"No","No","Yes",null,null,"R",{"$nulls":6},"W",{"$nulls":14},"0x101F9A02"]
[{"$nulls":9},"s60 5.0",null,"0x1",null,null,"No","No","Yes",null,null,"R",{"$nulls":6},"W",{"$nulls":14},"0x101F9A02"]
[{"$nulls":4},"KFotaMonitoryServiceEnabled","0x00000007",null,"Determines whether the Fota Monitory Service is enabled or not.\n0 (default in S60 3.2) - Feature OFF\n1  (default in S60 5.0) - Feature ON",{"$nulls":4},"No","Int"]
[{"$nulls":9},"s60 3.2",null,"0x0",null,null,"No","No","Yes",null,null,"R",{"$nulls":6},"W",{"$nulls":14},"0x101F9A02"]
[{"$nulls":9},"s60 5.0",null,"0x1",null,null,"No","No","Yes",null,null,"R",{"$nulls":6},"W",{"$nulls":14},"0x101F9A02"]
[{"$nulls":4},"KFotaOptionsForReminderDuration","0x00000008",null,"This key is to configure  the reminder options .\nFormat :\n1h:4h:1d:3m:NROFF\nh - hour/s. \nd- day/s\nm - minute/s\n\":\" Is the separator.\nCurrently only first 4 options are read to show reminder duration.\n5th option can have value NROFF which means that \"No reminder\" option  will not be shown.\nif 5th option has any other value other than NROFF , \"No reminder\" option will be shown\nDefault value : NULL.  Which means current options  1h:4h:1d:3d are taken into consideration along with No Reminder option.",{"$nulls":4},"Yes","Str"]
[{"$nulls":9},"s60 3.2",{"$nulls":4},"No","No","Yes","0x102072C4",null,"R"]
[{"$nulls":4},"KFotaReminderTimerReset","0x00000009",null,"This key is to enable feature to reset the timer after device reboot  .\nIf value is 0 : Feature is OFF. - Default value\nIf value is 1  : Feature is ON.\nAny other value its feature OFF\nIf feature is ON then if there was a reminder  set once device reboots timer should be reset and note to install Firmware update is shown .",{"$nulls":4},"Yes","Int"]
[{"$nulls":9},"s60 3.2",null,"0x0",null,null,"No","No","Yes","0x102072C4",null,"R"]
[{"$nulls":4},"KFotaUSBChargerEnabled","0x0000000A",null,"This key is to differntiate the USB charger enabled device and Dynamo charger enabled device\nIf value is 0 : Dynamo Charger\nIf value is 1  : USB charger                                                                                                                                                                                              In case of USB charger mode,if the battery is low to update the device then device will monitor for the appropriate battery level to allow the update to continue\nif both the mode of charging should be enabled then this key should have the value of  1.",{"$nulls":4},"Yes","Int"]
[{"$nulls":9},"s60 3.2",null,"0x0",null,null,"No","No","Yes","0x102072C4",null,"R"]
[{"$nulls":9},"s60 5.0",null,"0x1",null,null,"No","No","Yes","0x102072C4",null,"R"]