{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Main","Key values"],"not_rendered":{"macros":1,"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Main","index":0,"n_rows":13,"n_cols":6,"rows_kept":13,"flags":["formulas_cached_only"]}
[{"$nulls":5},"DO NOT DELETE THIS SHEET. THE FUTURE CONVERSION SCRIPTS NEED THE TEMPLATE VERSION INFORMATION"]
[null,"Template version","2.1"]
[null,"Purpose"]
[null,"CenRep keys "]
[]
[]
[]
[null,"Version",{"v":0.2,"d":"0.20"}]
[]
[null,"Version History"]
[null,"Date","Version","Type",null,"Comments"]
[null,"2004-11-17",0.1,"Draft",null,"Initial draft for CR"]
[null,"2006-11-02",0.2,null,null,"New CR key KOMAProvAuthenticationLV  (101-28506)"]

{"sheet":"Key values","index":1,"n_rows":10,"n_cols":59,"rows_kept":10,"flags":["formulas_cached_only"]}
["Uid Name","Uid Value","Range From","Range To","Key Name","Key Int","Shared Data Name","Purpose","Removed","Platform Release","Variant Name","Def Value","Read  Only","Key Type","Backup","RFS","Cust Config","Owner","Related Features","AlwaysPass","NetworkServices","LocalServices","ReadUserData","WriteUserData","Location","ReadDeviceData","WriteDeviceData","ProtServ","DRM","SwEvent","PowerMgmt","AllFiles","DiskAdmin","NetworkControl","MultiMediaDD","CommDD","TCB","TrustedUI","UserEnvironment","SurroundingsDD","SID Read","SID Write","Yes","No","Must","Int","Real","Str","Bin","R","W","RW","elaf","apac","thai","japan","gsm","low_cost","Do not delete AN1 -> BC1, since they are used in the multichoise column validation"]
["KCRUidOMAProvisioningLV","0x101F87AA"]
[{"$nulls":9},"S60 3.0",{"$nulls":4},"No","No",null,"0x101F84D6",null,"R",{"$nulls":6},"W"]
[{"$nulls":4},"KOMAProvisioningLVFlag","0x00000000","KOMALVFlag","Binding settings to a configuration context. When a configuration context is deleted, this flag indicates that the settings in the context are deleted, too. ",{"$nulls":4},"Yes","Int"]
[{"$nulls":9},"S60 3.0",null,1,null,null,"No","No","Yes",null,null,"R"]
[{"$nulls":4},"KOMAProvAuthenticationLV","0x00000001",null,"For OMA Provisioning authentication mechanism variation. Default (0xF): all mechanisms (NETWPIN, NETWUSERPIN, USERPIN, USERPINMAC) are supported. The value 0x1 means that only NETWPIN is supported. Other values are reserved for future use and are handled like the default value.  ",{"$nulls":4},"No","Int"]
[{"$nulls":9},"S60 3.2",null,15,null,null,"No","No","Yes",null,null,"R",{"$nulls":6},"W"]
[{"$nulls":4},"KOMAProvAuthFailMsgHandling","0x00000002",null,"This flag is used to handle the message when a setting message received and a authetication failure happens for this message. \nValid values for this variation, cenrep key are 0 and 1.\nIf value is \"0\" : An informative message will be stored in to inbox and a new message dialog is popped up.\nIf the value is \"1\": The informative message with class 0 characteristics will be put to inbox, the outcome would be this informative message is shown immediately and deleted after user exiting.\n",{"$nulls":4},"No","Int"]
[{"$nulls":9},"S60 3.2",null,0,null,null,"No","No","Yes",null,null,"R",{"$nulls":6},"W"]
[{"$nulls":4},"KOMAProvOriginatorContent","0x00000003",null,"This flag is used to store the originator of the Configuration message.",null,"S60 3.2",null,"\"\"","No","Str","No","No","Yes",null,null,"R",{"$nulls":6},"W"]