[test0]
DiallingPauseDuration= 3
ConnectingPauseDuration= 1
DisconnectingPauseDuration= 5
AnswerIncomingPauseDuration= 5

AttachPauseDuration= 4, 0
DetachPauseDuration= 3, 0

# xxxPauseDuration = <Duration> <Error code>

ActivatePauseDuration= 3, 0
DeactivatePauseDuration= 5, 0
DeletePauseDuration= 4, 0
SetConfigFail = NEG_99, 1, 0
# TSetConfigFail = <TName contextName>, <TInt numberofTimes>, <TInt errorCode>
ContextConfigRel99 = REQ_99, 1, 0, 1, 2, 2, 1
# TRel99ContextConfig <TName contextName>, <TUint iActivatePause>, 
# <TUint iActivateErrorCode>, <TUint iDeactivatePause>, <TUint iDeactivateErrorCode> 
# <TUint iDeletionPause>, <TUint iDeletionErrorCode>
PacketFilterInfo = 2, 0, 10.32.2.1, 10.32.2.2, 1, 2, 2, 4, 3, 2, 1, 2

# xxxPauseDuration = <Duration> <Error code>
QosProfileReqR99 = REQ_99, 0x04, 0x02, 0x04, 0x02, 0x08, 0x04, 0x02, 0x04, 0x02, 0x08, 0x04, 0x02, 0x04, 0x02, 0x08, 0x04, 0x02, 0x04, 0x02, 0x08, 0x04, 0x02, 0x04, 0x02
QosProfileNegR99 = NEG_99, 0x04, 0x02, 0x04, 0x02, 0x08, 0x04, 0x02, 0x04, 0x02, 0x08, 0x04, 0x02, 0x04
QosProfileCapsR99= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04
QosNetworkNotification = NEG_99, 0x04, 0x02, 0x04, 0x02, 0x08, 0x04, 0x02, 0x04, 0x02, 0x08, 0x04, 0x02, 0x04
SetProfileFail = NEG_99, 0x04, 0x02
QosProfileReqGPRS= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020
QosProfileReqGPRS= 0x04, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002
QosProfileCapsGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002 

# QosProfileReq = <min TQoSPrecedence>, <req TQoSPrecedence>, <min TQoSDelay>, <req TQoSDelay>, 
#		  <min TQoSReliability>, <req TQoSReliability>, <min TQoSPeakThroughput>, <req TQoSPeakThroughput>, 
#		  <min TQoSMeanThroughput>, <req TQoSMeanThroughput>
# QosProfileNeg = <TQoSPrecedence>, <TQoSDelay>, <TQoSReliability>, <TQoSPeakThroughput>, <TQoSMeanThroughput>

QosProfileReqCDMA= 0x0, 0x08, 0x0002, 0x02, 0x04, 0x01, 0x08, 0x02, 0x04, 0x04, 0x04, 0x20, 0x40, 0x20, 0x40
QosProfileNegCDMA= 0x1, 0x08, 0x0002, 0x04, 0x04, 0x04, 0x04, 0x20, 0x20
QosProfileCapsCDMA= 0x0002, 0x04, 0x04, 0x04, 0x04, 0x20, 0x20		

# QosProfileReqCDMA = <TBool>, <TRLPMode>, <TQoSLinkPriority>, <TQoSDataRate>, <TQoSDataRate>, <TQoSDataRate>, 
#		      	<TQoSDataRate>, <TQoSDataLoss>, <TQoSDataLoss>, <TQoSDataLoss>, <TQoSDataLoss>, <TQoSDelay>, 
#			<TQoSDelay>, <TQoSDelay>, <TQoSDelay>

# QosProfileNegCDMA = <TBool>, <TRLPMode>, <TQoSLinkPriority>, <TQoSDataRate>, <TQoSDataRate>, <TQoSDataLoss>, 
#			<TQoSDataLoss>, <TQoSDelay>, <TQoSDelay>

SetContextConfigGPRS= 3, ACME INTERNET PROVIDERS LTD, i-MODE GATEWAY, 1, 2, 1
SetContextConfigGPRS= 1, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1
GetContextConfigGPRS= 1, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1
GetContextConfigGPRS= 3, ACME INTERNET PROVIDERS LTD, i-MODE GATEWAY,  1, 2, 1
# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TBool>

SetContextConfigCDMA= 4, 3
GetContextConfigCDMA= 4, 3
# SetContextConfigCDMA = <ServiceOption>, <ProtocolType>

SetContextConfigRel99= 1, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL
SetContextConfigRel99= 1, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL
# Release 99 stuff uses same struct ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>
# no anonymous access or data compression

DefaultContextparamCDMA= 4, 3
# DefaultContextparamCDMA= <ServiceOption>, <ProtocolType>

DefaultContextparamGPRS= 3, ACME INTERNET PROVIDERS LTD, i-MODE GATEWAY, 1, 2
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>

PacketReleaseMode = 4, 4
# PacketReleaseMode = <TInt Duration>, <TInt ReleaseMode>

SmsControlCaps= 455
#SmsControlCaps= caps in DECIMAL

SmsPhoneStoreCaps= 0xFC000000
#SmsPhoneStoreCaps= TMobilePhoneCaps in the smsStore in hexadecimal

SmsRxPeriod= 2
SmsRx= 01A0, 01632960000
SmsRx= 01A1, 01632960000
SmsRx= 01A1, 01632960000
SmsAckNackPause= 1
SmsResumePause= 1

SmsStore= S14, 10
SmsStoreEntry= S14, 1, 4, 01A2, 41632960000
SmsStoreIndividualReqPause= 1
SmsStoreBatchReqPause= 2

# SmsStoreEntry = <store>, <index>, <stat>, <pdu>
# SmsStore = <store>, <maxnumslots>
# S14 is equivalent to KETelIccSmsStore 

PhBkStore= S7, 100, 50, 60
PhBkStoreEntry= S7, 1, 01632960000, AndyLocal
PhBkStoreEntry= S7, 2, +441632960000, AndyInternat
PhBkStoreIndividualReqPause= 3
PhBkStoreBatchReqPause= 4
PhBkPhoneStoreCaps=  0xFC000000


# PhBkStore = <store>, <maxnumslots>, <TelNumMaxLen>, <AlphaTagMaxLen>
# PhBkStoreEntry = <store>, <index>, <TelNum>, <AlphaTag>
# S7 is equivalent to KETelIccAdnPhoneBook
#PhBkPhoneStoreCaps the phone store caps for the phone book

SmsParamEntry= 1, Vodaphone, 00, 00, 24, 01632960000, 447785016005
SmsParamEntry= 2, BT, 00, 00, 12, 01632960000, 447802000332
SmsParamBatchReqPause= 4
SmsParamMaxNumSlots= 10

# SmsParam = <maxnumslots>, <TelNumMaxLen>, <AlphaTagMaxLen>
# SmsParamEntry = <Index>, <Name>, <PID>, <DCS>, <Validity Period(hour)> <DA> <SCA>

SignalStrengthLevel= 2, -20, 3, 0
SignalStrengthLevel= 2, -30, 2, 0
SignalStrengthLevel= 3, -40, 1, 0

# SignalStrengthLevel = <duration>, <dbLevel>, <barLevel> <error code>


SatRefresh= 3, 2, 6F3A
SatRefresh= 5, 1, 6F3B
SatRefresh= 7, 5, 6F3A6F3B

# SatRefresh = <duration>, <TRefreshType>, <TRefreshFileList>


NetworkInfo= ABCD, Network0, Vodafone, Voda, Vodafone_UK, 0
NetworkInfo= EFGH, Network1, Cellnet, Cell, Cellnet_UK, 1
NetworkInfo= IJKL, Network2, One2One, 121, One2One_UK, 1
NetworkInfo= MNOP, Network3, Orange, Orgn, Orange_UK, 1

RegStatus= 5,3
RegStatus= 2,5,0
RegStatus= 2,7,3
RegStatus= 5,2
RegStatus= 2,5,0

PacketRegStatus= 5,2
PacketRegStatus= 2,1
PacketRegStatus= 3,5

# PacketRegStatus = <Duration>, <RegStatus>

NitzInfo= 6,2001,09,15,10,15,0,0,1234,5678
NitzInfo= 2,2002,10,16,11,16,1,1,9012,3456

# NetworkInfo = <CountryCode>, <NetworkId>, <DisplayTag>, <ShortName>, <LongName> <status>
# Note: First NetworkInfo assumed "home" network.

# RegStatus = <Duration>, <RegStatus>, <NetworkIndex>
# Note: <NetworkIndex> is the index from the above list.

# NitzInfo = <Duration>, <Year>, <Month>, <Day>, <Hour>, <Minute>, <Second>, <MicroSecond>, <timezone>, <dst>

DynamicCaps= 4, 1024
DynamicCaps= 2, 512
# DynamicCaps= <Duration>, <DynamicCaps>
# Note: <DynamicCaps> is a bitmap of RPacketService::TDynamicCaps flags. 

NetworkMode= 4, 2
NetworkMode= 2, 6
# NetworkMode= <Duration>, <NetworkMode>
# Note: <NetworkMode> is a enum of RMobilePhone::TMobilePhoneNetworkMode. 

CellInfo= 10,1,1211,111, 1
CellInfo= 2,2,3122, 73, 0


# CellInfo = <Duration>, <Mode>, <cellId>, <timingAdvance>, <cellInfoStatus>


SubscriberId= 5601632960000

CommSetup= SIMTSYLOOPBACK.CSY, SIMTSYLOOPBACK::0, 18, 0

# CommSetup = ECUART.CSY, COMM::0, 14, 0
# CommSetup = <csy name>, <port name>, <datarate>, <handshake>

BearerService= 1, 3
# BearerService = <bearer caps>, <bearer speed>

Indicators= 2, -2017

# Indicators = <notification number>, <error code>

BatteryCharger= 2, 0, 0, 0
BatteryCharger= 5, 1, 3, 0
BatteryCharger= 5, 2, 5, 0
BatteryCharger= 5, 1, 3, 0

# BatteryCharger = <duration>, <status> <battery level> <error code>

[test1]
PhBkStore= S7, 100, 50, 60
PhBkStoreEntry= S7, 1, 01632960000, AndyLocal
PhBkStoreEntry= S7, 2, +441632960000, AndyInternat
PhBkStoreIndividualReqPause= 3
PhBkStoreBatchReqPause= 4

PhBkError= 2,-1000
PhBkError= 4,-1001

OOBPhBkWrite= 5, S7, 5, +441632960000, AndyInternat
OOBPhBkDelete= 10, S7, 5

SmsControlCaps= 455
#SmsControlCaps= caps in DECIMAL

SmsPhoneStoreCaps= 0xFC000000
#SmsPhoneStoreCaps= TMobilePhoneCaps in the smsStore in hexadecimal

SmsRxPeriod= 3
SmsRx= 01A0, 01632960000
SmsRx= 02A0, 01632960000
SmsRx= 03A1, 01632960000
SmsRx= 04A1, 01632960000
SmsAckNackPause= 1
SmsResumePause= 1

SmsStore= S14, 2
SmsStoreEntry= S14, 1, 4, 01A2, 41632960000
SmsStoreIndividualReqPause= 1
SmsStoreBatchReqPause= 2

# SmsStoreEntry = <store>, <index>, <stat>, <pdu>
# SmsStore = <store>, <maxnumslots>
# S14 is equivalent to KETelIccSmsStore 
[test2]
# No tags in this test...

[test3]

ICCLockedAtStart= 0
ICCStatus= 2, 0
ICCStatus= 2, 1

PhBkStore= S7, 100, 50, 60
PhBkStoreEntry= S7, 1, 01632960000, AndyLocal
PhBkStoreEntry= S7, 2, +441632960000, AndyInternat
PhBkStoreIndividualReqPause= 3
PhBkStoreBatchReqPause= 4

TriggerEventIPC= 5150, 2, 0


[TEST4]
PhBkStore=  ,1
PhBkStore= S7, 100, 50, 60
PhBkStoreEntry=  ,1
PhBkStoreEntry= S7, 1, 01632960000, AndyLocal
PhBkError=  ,1
PhBkError= 4,-1001
OOBPhBkWrite=  ,1
OOBPhBkDelete=  ,1
ICCStatus=  ,1
TriggerEventIPC=  ,1
SmsStartRxDelay=  ,1
SmsParamEntry=  1,,
SmsStore= S14, 
SmsStore= S14, 2
SmsStoreEntry= S14, , ,
SetContextConfigGPRS=  ,1
GetContextConfigGPRS=  ,1
SetContextConfigCDMA=  ,1
GetContextConfigCDMA=  ,1
PacketRegStatus=  ,1
QosProfileReqGPRS=  ,1
QosProfileNegGPRS=  ,1
QosProfileReqCDMA=  ,1
QosProfileNegCDMA=  ,1
DefaultContextparamGPRS=  ,1
DefaultContextparamCDMA=  ,1
NetworkInfo=  ,1
RegStatus=  ,1
NitzInfo=  ,1
CellInfo=  ,1
SignalStrengthLevel=  ,1
BearerService=  ,, 1
Indicators=  ,1
BatteryCharger=  ,1
SatRefresh=  ,1
CommSetup=  1,


