############################################################################
############################################################################
###################              T E S T 1              ####################
############################################################################
############################################################################
# Successful Start of Primary PDP context
############################################################################
[test1]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,192.168.2.4, 0, 2, 0, 0,RasUser,,,,194.72.6.51,194.72.6.51,0

# TRel99ContextConfig = <TName iContextName>,  <TUint iActivatePause>, <TUint iActivateErrorCode>, <TUint iDeactivatePause>, 
# <TUint iDeactivateErrorCode>, <TUint iDeletionPause>, <TUint iDeletionErrorCode> <TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, 0, 0, 0, 0, 0, 0


#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0


#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3

QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0



# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= PKTLOOPBACK, PKTLOOPBACK::502, 18, 0, PRIMARY1

# failure events
NotifyContextStatusChangeType = PublishSubscribe
NotifyContextStatusChange = PRIMARY1, 0, 1
NotifyContextStatusChange = PRIMARY1, 0, 1
NotifyContextStatusChange = PRIMARY1, 0, 2
NotifyContextStatusChange = PRIMARY1, 0, 3
NotifyContextStatusChange = PRIMARY1, 0, 4
NotifyContextStatusChange = PRIMARY1, 0, 5
NotifyContextStatusChange = PRIMARY1, 0, 6


# NotifyContextStatusChange <iContextName>, <iDuration>, <iStatus>
# EStatusDeactivating = 4 EStatusInactive = 1 EStatusDeleted = 6
# EStatusSuspended = 5 EStatusActive = 3

############################################################################
############################################################################
###################              T E S T 1 1            ####################
############################################################################
############################################################################
# Successful Start of Primary PDP context, delay on primary deletion
############################################################################
[test11]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,192.168.2.4, 0, 2, 0, 0,RasUser,,,,194.72.6.51,194.72.6.51,0

# TRel99ContextConfig = <TName iContextName>,  <TUint iActivatePause>, <TUint iActivateErrorCode>, <TUint iDeactivatePause>, 
# <TUint iDeactivateErrorCode>, <TUint iDeletionPause>, <TUint iDeletionErrorCode> <TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, 0, 0, 0, 30, 0, 0


#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0

#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3

QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0

# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= PKTLOOPBACK, PKTLOOPBACK::502, 18, 0, PRIMARY1

############################################################################
############################################################################
###################              T E S T 2              ####################
############################################################################
############################################################################
# Primary and Secondary: delay on secondary deletion.
############################################################################
[test2]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,192.168.2.4, 0, 2, 0, 0,RasUser,,,,194.72.6.51,194.72.6.51,0

# TRel99ContextConfig = <TName iContextName>,  <TUint iActivatePause>, <TUint iActivateErrorCode>, <TUint iDeactivatePause>, 
# <TUint iDeactivateErrorCode>, <TUint iDeletionPause>, <TUint iDeletionErrorCode> <TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, 0, 0, 0, 0, 0, 0
R99ContextConfig = SECONDARY1, 0, 0, 0, 0, 20, 0, 0
R99ContextConfig = SECONDARY2, 0, 0, 0, 0, 0, 0, 0

# TFTfilter = 0<id> 1<evaluationPrecedenceIndex> 2<srcAddr> 3<srcAddrSubnetMask>  4<protocolNumberOrNextHeader>
#	      5<srcPortMin> 6<srcPortMax> 7<destPortMin> 8<destPortMax> 9<ipSecSPI> 10<toSorTrafficClass>
#	      11<flowLabel>
TFTfilter = 1, 0, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0

#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0
QosProfileReqR99 = SECONDARY1,0x04, 0x04, 0x01, 0x01, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 250, 250, -1, -1, 0, 0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY1,0x04, 0x04, 0x01, 0x01, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 250, 250, -1, -1, 0, 0, 0, 0


#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY2, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = SECONDARY2, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0


#TQosProfileCapsR99 = <trafficCap> <deliveryOrderReqCap> <deliverErroneousSDUCap>
#		      <BERCap> <SDUErrorRatioCap> <trafficHandlingPriorityCap>
QosProfileCapsR99= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04

QosNetworkNotificationType = PublishSubscribe
# QosNetworkNotification = <contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> <negMaxSDUSize>
QosNetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = PRIMARY2, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosR5NetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = PRIMARY2, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0

#SetProfileFail= <contextName> <numberOfTimes> <errorCode> <setProfileDigit>
SetProfileFail = NEG_99, 0x04, 0x02

#QosprofileReqGPRS= <minPrecedence> <reqPrecedence> <minDelay> <reqDelay> <minReliability> <reqReliability> <minPeek> <reqPeek>
#		    <minMean> <reqMean>
QosProfileReqGPRS= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020
QosProfileReqGPRS= 0x04, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020

#QosProfileNegGPRS=<negPrecedence> <negDelay><negReliability> <negPeek> <negMean>
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002

#QosProfileCapsGPRS=<negPrecedenceCap> <negDelayCap> <negReliabilityCap><negPeekCap> <negMeanCap>
QosProfileCapsGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002 

# QosProfileReq
# = <TTrafficClass>, <TTrafficClass>, <TDeliveryOrder>, <TDeliveryOrder>
# <TErroneousSDUDelivery>, <TErroneousSDUDelivery>
# <TErroneousSDUDelivery>, <TInt iReqMaxSDUSize>, <TInt iMinAcceptableMaxSDUSize>
# <TBitRate>, <TBitRate>, <TBitErrorRatio>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>, <TTrafficHandlingPriority>
# <TInt	iReqTransferDelay>, <TInt iMaxTransferDelay>, <TBitRate>, <TBitRate>

# QosProfileNeg = <TQoSPrecedence>, <TQoSDelay>, <TQoSReliability>, <TQoSPeakThroughput>, <TQoSMeanThroughput>
# <TTrafficClass>, <TDeliveryOrder>, <TErroneousSDUDelivery>, <TInt iMaxSDUSize>, <TBitRate>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>
# <TInt iTransferDelay>, <TBitRate>		

DefaultContextparamRel99= 3, ACME INTERNET PROVIDERS LTD, i-MODE GATEWAY, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2
# DefaultContextparamRel99 = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>

ReleaseMode = 5, 5
# Packet Release mode = <Release> <Duration>

#RegStatus=<duration> <regStat> <networkIndex> 
RegStatus= 5,3
RegStatus= 2,5,0
RegStatus= 2,7,3
RegStatus= 5,2
RegStatus= 2,5,0

# NetworkRegStatus = <Duration>, <RegistrationStatus>
NetworkRegStatusType = PublishSubscribe
NetworkRegStatus= 5,2
NetworkRegStatus= 5,1
NetworkRegStatus= 5,1

# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= PKTLOOPBACK, PKTLOOPBACK::502, 18, 0, PRIMARY1
CommSetup= PKTLOOPBACK.CSY, PKTLOOPBACK::504, 18, 0, SECONDARY1

############################################################################
############################################################################
###################              T E S T 2 2            ####################
############################################################################
############################################################################
# Secondary delay on Activation
# Primary and Secondary.
############################################################################
[test22]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,192.168.2.4, 0, 2, 0, 0,RasUser,,,,194.72.6.51,194.72.6.51,0

# TRel99ContextConfig = <TName iContextName>,  <TUint iActivatePause>, <TUint iActivateErrorCode>, <TUint iDeactivatePause>, 
# <TUint iDeactivateErrorCode>, <TUint iDeletionPause>, <TUint iDeletionErrorCode> <TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, 0, 0, 0, 0, 0, 0
R99ContextConfig = SECONDARY1, 0, 0, 0, 0, 0, 0, 0

# TFTfilter = 0<id> 1<evaluationPrecedenceIndex> 2<srcAddr> 3<srcAddrSubnetMask>  4<protocolNumberOrNextHeader>
#	      5<srcPortMin> 6<srcPortMax> 7<destPortMin> 8<destPortMax> 9<ipSecSPI> 10<toSorTrafficClass>
#	      11<flowLabel>
TFTfilter = 1, 0, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0

#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0
QosProfileReqR99 = SECONDARY1,0x04, 0x04, 0x02, 0x02, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x08, 0x08, 250, 250, -1, -1, 0, 0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY1,0x04, 0x04, 0x02, 0x02, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x08, 0x08, 250, 250, -1, -1, 0, 0, 0, 0


#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY2, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = SECONDARY2, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0

#TQosProfileCapsR99 = <trafficCap> <deliveryOrderReqCap> <deliverErroneousSDUCap>
#		      <BERCap> <SDUErrorRatioCap> <trafficHandlingPriorityCap>
QosProfileCapsR99= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04

QosNetworkNotificationType = PublishSubscribe
# QosNetworkNotification = <contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> <negMaxSDUSize>
QosNetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = PRIMARY2, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosR5NetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = PRIMARY2, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0

#SetProfileFail= <contextName> <numberOfTimes> <errorCode> <setProfileDigit>
SetProfileFail = NEG_99, 0x04, 0x02

#QosprofileReqGPRS= <minPrecedence> <reqPrecedence> <minDelay> <reqDelay> <minReliability> <reqReliability> <minPeek> <reqPeek>
#		    <minMean> <reqMean>
QosProfileReqGPRS= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020
QosProfileReqGPRS= 0x04, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020

#QosProfileNegGPRS=<negPrecedence> <negDelay><negReliability> <negPeek> <negMean>
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002

#QosProfileCapsGPRS=<negPrecedenceCap> <negDelayCap> <negReliabilityCap><negPeekCap> <negMeanCap>
QosProfileCapsGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002 

# QosProfileReq
# = <TTrafficClass>, <TTrafficClass>, <TDeliveryOrder>, <TDeliveryOrder>
# <TErroneousSDUDelivery>, <TErroneousSDUDelivery>
# <TErroneousSDUDelivery>, <TInt iReqMaxSDUSize>, <TInt iMinAcceptableMaxSDUSize>
# <TBitRate>, <TBitRate>, <TBitErrorRatio>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>, <TTrafficHandlingPriority>
# <TInt	iReqTransferDelay>, <TInt iMaxTransferDelay>, <TBitRate>, <TBitRate>

# QosProfileNeg = <TQoSPrecedence>, <TQoSDelay>, <TQoSReliability>, <TQoSPeakThroughput>, <TQoSMeanThroughput>
# <TTrafficClass>, <TDeliveryOrder>, <TErroneousSDUDelivery>, <TInt iMaxSDUSize>, <TBitRate>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>
# <TInt iTransferDelay>, <TBitRate>		

DefaultContextparamRel99= 3, ACME INTERNET PROVIDERS LTD, i-MODE GATEWAY, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2
# DefaultContextparamRel99 = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>

ReleaseMode = 5, 5
# Packet Release mode = <Release> <Duration>

#RegStatus=<duration> <regStat> <networkIndex> 
RegStatus= 5,3
RegStatus= 2,5,0
RegStatus= 2,7,3
RegStatus= 5,2
RegStatus= 2,5,0

# NetworkRegStatus = <Duration>, <RegistrationStatus>
NetworkRegStatusType = PublishSubscribe
NetworkRegStatus= 5,2
NetworkRegStatus= 5,1
NetworkRegStatus= 5,1

# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= PKTLOOPBACK, PKTLOOPBACK::502, 18, 0, PRIMARY1
CommSetup= PKTLOOPBACK, PKTLOOPBACK::504, 18, 0, SECONDARY1

############################################################################
############################################################################
###################              T E S T 2 3            ####################
############################################################################
############################################################################
# Secondary delay on Deletion
# Primary and Secondary.
############################################################################
[test23]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,192.168.2.4, 0, 2, 0, 0,RasUser,,,,194.72.6.51,194.72.6.51,0

# TRel99ContextConfig = <TName iContextName>,  <TUint iActivatePause>, <TUint iActivateErrorCode>, <TUint iDeactivatePause>, 
# <TUint iDeactivateErrorCode>, <TUint iDeletionPause>, <TUint iDeletionErrorCode> <TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, 0, 0, 0, 0, 0, 0
R99ContextConfig = SECONDARY1, 0, 0, 0, 0, 20, 0, 0

# TFTfilter = 0<id> 1<evaluationPrecedenceIndex> 2<srcAddr> 3<srcAddrSubnetMask>  4<protocolNumberOrNextHeader>
#	      5<srcPortMin> 6<srcPortMax> 7<destPortMin> 8<destPortMax> 9<ipSecSPI> 10<toSorTrafficClass>
#	      11<flowLabel>
TFTfilter = 1, 0, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0

#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0
QosProfileReqR99 = SECONDARY1,0x04, 0x04, 0x01, 0x01, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 250, 250, -1, -1, 0, 0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY1,0x04, 0x04, 0x01, 0x01, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 250, 250, -1, -1, 0, 0, 0, 0


#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY2, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = SECONDARY2, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0

#TQosProfileCapsR99 = <trafficCap> <deliveryOrderReqCap> <deliverErroneousSDUCap>
#		      <BERCap> <SDUErrorRatioCap> <trafficHandlingPriorityCap>
QosProfileCapsR99= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04

QosNetworkNotificationType = PublishSubscribe
# QosNetworkNotification = <contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> <negMaxSDUSize>
QosNetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = PRIMARY2, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosR5NetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = PRIMARY2, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0

#SetProfileFail= <contextName> <numberOfTimes> <errorCode> <setProfileDigit>
SetProfileFail = NEG_99, 0x04, 0x02

#QosprofileReqGPRS= <minPrecedence> <reqPrecedence> <minDelay> <reqDelay> <minReliability> <reqReliability> <minPeek> <reqPeek>
#		    <minMean> <reqMean>
QosProfileReqGPRS= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020
QosProfileReqGPRS= 0x04, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020

#QosProfileNegGPRS=<negPrecedence> <negDelay><negReliability> <negPeek> <negMean>
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002

#QosProfileCapsGPRS=<negPrecedenceCap> <negDelayCap> <negReliabilityCap><negPeekCap> <negMeanCap>
QosProfileCapsGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002 

# QosProfileReq
# = <TTrafficClass>, <TTrafficClass>, <TDeliveryOrder>, <TDeliveryOrder>
# <TErroneousSDUDelivery>, <TErroneousSDUDelivery>
# <TErroneousSDUDelivery>, <TInt iReqMaxSDUSize>, <TInt iMinAcceptableMaxSDUSize>
# <TBitRate>, <TBitRate>, <TBitErrorRatio>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>, <TTrafficHandlingPriority>
# <TInt	iReqTransferDelay>, <TInt iMaxTransferDelay>, <TBitRate>, <TBitRate>

# QosProfileNeg = <TQoSPrecedence>, <TQoSDelay>, <TQoSReliability>, <TQoSPeakThroughput>, <TQoSMeanThroughput>
# <TTrafficClass>, <TDeliveryOrder>, <TErroneousSDUDelivery>, <TInt iMaxSDUSize>, <TBitRate>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>
# <TInt iTransferDelay>, <TBitRate>		

DefaultContextparamRel99= 3, ACME INTERNET PROVIDERS LTD, i-MODE GATEWAY, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2
# DefaultContextparamRel99 = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>

ReleaseMode = 5, 5
# Packet Release mode = <Release> <Duration>

#RegStatus=<duration> <regStat> <networkIndex> 
RegStatus= 5,3
RegStatus= 2,5,0
RegStatus= 2,7,3
RegStatus= 5,2
RegStatus= 2,5,0

# NetworkRegStatus = <Duration>, <RegistrationStatus>
NetworkRegStatusType = PublishSubscribe
NetworkRegStatus= 5,2
NetworkRegStatus= 5,1
NetworkRegStatus= 5,1

# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= PKTLOOPBACK, PKTLOOPBACK::502, 18, 0, PRIMARY1
CommSetup= PKTLOOPBACK, PKTLOOPBACK::504, 18, 0, SECONDARY1

############################################################################
############################################################################
###################              T E S T 2 4            ####################
############################################################################
############################################################################
# Secondary delay on Activation
# Primary and Secondary.
############################################################################
[test24]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,192.168.2.4, 0, 2, 0, 0,RasUser,,,,194.72.6.51,194.72.6.51,0

# TRel99ContextConfig = <TName iContextName>,  <TUint iActivatePause>, <TUint iActivateErrorCode>, <TUint iDeactivatePause>, 
# <TUint iDeactivateErrorCode>, <TUint iDeletionPause>, <TUint iDeletionErrorCode> <TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, 0, 0, 0, 0, 0, 0
R99ContextConfig = SECONDARY1, 60, 0, 0, 0, 0, 0, 0

# TFTfilter = 0<id> 1<evaluationPrecedenceIndex> 2<srcAddr> 3<srcAddrSubnetMask>  4<protocolNumberOrNextHeader>
#	      5<srcPortMin> 6<srcPortMax> 7<destPortMin> 8<destPortMax> 9<ipSecSPI> 10<toSorTrafficClass>
#	      11<flowLabel>
TFTfilter = 1, 0, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0

#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0
QosProfileReqR99 = SECONDARY1,0x04, 0x04, 0x02, 0x02, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x08, 0x08, 250, 250, -1, -1, 0, 0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY1,0x04, 0x04, 0x02, 0x02, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x08, 0x08, 250, 250, -1, -1, 0, 0, 0, 0


#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY2, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = SECONDARY2, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0

#TQosProfileCapsR99 = <trafficCap> <deliveryOrderReqCap> <deliverErroneousSDUCap>
#		      <BERCap> <SDUErrorRatioCap> <trafficHandlingPriorityCap>
QosProfileCapsR99= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04

QosNetworkNotificationType = PublishSubscribe
# QosNetworkNotification = <contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> <negMaxSDUSize>
QosNetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = PRIMARY2, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4


QosR5NetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = PRIMARY2, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0


#SetProfileFail= <contextName> <numberOfTimes> <errorCode> <setProfileDigit>
SetProfileFail = NEG_99, 0x04, 0x02

#QosprofileReqGPRS= <minPrecedence> <reqPrecedence> <minDelay> <reqDelay> <minReliability> <reqReliability> <minPeek> <reqPeek>
#		    <minMean> <reqMean>
QosProfileReqGPRS= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020
QosProfileReqGPRS= 0x04, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020

#QosProfileNegGPRS=<negPrecedence> <negDelay><negReliability> <negPeek> <negMean>
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002

#QosProfileCapsGPRS=<negPrecedenceCap> <negDelayCap> <negReliabilityCap><negPeekCap> <negMeanCap>
QosProfileCapsGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002 

# QosProfileReq
# = <TTrafficClass>, <TTrafficClass>, <TDeliveryOrder>, <TDeliveryOrder>
# <TErroneousSDUDelivery>, <TErroneousSDUDelivery>
# <TErroneousSDUDelivery>, <TInt iReqMaxSDUSize>, <TInt iMinAcceptableMaxSDUSize>
# <TBitRate>, <TBitRate>, <TBitErrorRatio>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>, <TTrafficHandlingPriority>
# <TInt	iReqTransferDelay>, <TInt iMaxTransferDelay>, <TBitRate>, <TBitRate>

# QosProfileNeg = <TQoSPrecedence>, <TQoSDelay>, <TQoSReliability>, <TQoSPeakThroughput>, <TQoSMeanThroughput>
# <TTrafficClass>, <TDeliveryOrder>, <TErroneousSDUDelivery>, <TInt iMaxSDUSize>, <TBitRate>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>
# <TInt iTransferDelay>, <TBitRate>		

DefaultContextparamRel99= 3, ACME INTERNET PROVIDERS LTD, i-MODE GATEWAY, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2
# DefaultContextparamRel99 = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>

ReleaseMode = 5, 5
# Packet Release mode = <Release> <Duration>

#RegStatus=<duration> <regStat> <networkIndex> 
RegStatus= 5,3
RegStatus= 2,5,0
RegStatus= 2,7,3
RegStatus= 5,2
RegStatus= 2,5,0

# NetworkRegStatus = <Duration>, <RegistrationStatus>
NetworkRegStatusType = PublishSubscribe
NetworkRegStatus= 5,2
NetworkRegStatus= 5,1
NetworkRegStatus= 5,1

# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= PKTLOOPBACK, PKTLOOPBACK::502, 18, 0, PRIMARY1
CommSetup= PKTLOOPBACK, PKTLOOPBACK::504, 18, 0, SECONDARY1

############################################################################
############################################################################
###################              T E S T 2 5            ####################
############################################################################
############################################################################
# Secondary delay on Setting TFT
# Primary and Secondary.
############################################################################
[test25]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,192.168.2.4, 0, 2, 0, 0,RasUser,,,,194.72.6.51,194.72.6.51,0

# TRel99ContextConfig = <TName iContextName>,  <TUint iActivatePause>, <TUint iActivateErrorCode>, <TUint iDeactivatePause>, 
# <TUint iDeactivateErrorCode>, <TUint iDeletionPause>, <TUint iDeletionErrorCode> <TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, 0, 0, 0, 0, 0, 0
R99ContextConfig = SECONDARY1, 0, 0, 0, 0, 0, 0, 0

# delay creating TFT for secondary
CreateTftConfig = PRIMARY1, 0, 0, 60

# TFTfilter = 0<id> 1<evaluationPrecedenceIndex> 2<srcAddr> 3<srcAddrSubnetMask>  4<protocolNumberOrNextHeader>
#	      5<srcPortMin> 6<srcPortMax> 7<destPortMin> 8<destPortMax> 9<ipSecSPI> 10<toSorTrafficClass>
#	      11<flowLabel>
TFTfilter = 1, 0, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0

#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0
QosProfileReqR99 = SECONDARY1,0x04, 0x04, 0x02, 0x02, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x08, 0x08, 250, 250, -1, -1, 0, 0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY1,0x04, 0x04, 0x02, 0x02, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x08, 0x08, 250, 250, -1, -1, 0, 0, 0, 0

#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY2, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4


QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = SECONDARY2, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0

#TQosProfileCapsR99 = <trafficCap> <deliveryOrderReqCap> <deliverErroneousSDUCap>
#		      <BERCap> <SDUErrorRatioCap> <trafficHandlingPriorityCap>
QosProfileCapsR99= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04

QosNetworkNotificationType = PublishSubscribe
# QosNetworkNotification = <contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> <negMaxSDUSize>
QosNetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = PRIMARY2, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosR5NetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = PRIMARY2, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0

#SetProfileFail= <contextName> <numberOfTimes> <errorCode> <setProfileDigit>
SetProfileFail = NEG_99, 0x04, 0x02

#QosprofileReqGPRS= <minPrecedence> <reqPrecedence> <minDelay> <reqDelay> <minReliability> <reqReliability> <minPeek> <reqPeek>
#		    <minMean> <reqMean>
QosProfileReqGPRS= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020
QosProfileReqGPRS= 0x04, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020

#QosProfileNegGPRS=<negPrecedence> <negDelay><negReliability> <negPeek> <negMean>
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002

#QosProfileCapsGPRS=<negPrecedenceCap> <negDelayCap> <negReliabilityCap><negPeekCap> <negMeanCap>
QosProfileCapsGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002 

# QosProfileReq
# = <TTrafficClass>, <TTrafficClass>, <TDeliveryOrder>, <TDeliveryOrder>
# <TErroneousSDUDelivery>, <TErroneousSDUDelivery>
# <TErroneousSDUDelivery>, <TInt iReqMaxSDUSize>, <TInt iMinAcceptableMaxSDUSize>
# <TBitRate>, <TBitRate>, <TBitErrorRatio>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>, <TTrafficHandlingPriority>
# <TInt	iReqTransferDelay>, <TInt iMaxTransferDelay>, <TBitRate>, <TBitRate>

# QosProfileNeg = <TQoSPrecedence>, <TQoSDelay>, <TQoSReliability>, <TQoSPeakThroughput>, <TQoSMeanThroughput>
# <TTrafficClass>, <TDeliveryOrder>, <TErroneousSDUDelivery>, <TInt iMaxSDUSize>, <TBitRate>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>
# <TInt iTransferDelay>, <TBitRate>		

DefaultContextparamRel99= 3, ACME INTERNET PROVIDERS LTD, i-MODE GATEWAY, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2
# DefaultContextparamRel99 = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>

ReleaseMode = 5, 5
# Packet Release mode = <Release> <Duration>

#RegStatus=<duration> <regStat> <networkIndex> 
RegStatus= 5,3
RegStatus= 2,5,0
RegStatus= 2,7,3
RegStatus= 5,2
RegStatus= 2,5,0

# NetworkRegStatus = <Duration>, <RegistrationStatus>
NetworkRegStatusType = PublishSubscribe
NetworkRegStatus= 5,2
NetworkRegStatus= 5,1
NetworkRegStatus= 5,1

# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= PKTLOOPBACK, PKTLOOPBACK::502, 18, 0, PRIMARY1
CommSetup= PKTLOOPBACK, PKTLOOPBACK::504, 18, 0, SECONDARY1

############################################################################
############################################################################
###################              T E S T 2 6            ####################
############################################################################
############################################################################
#Primary and secondary: test long secondary start on lower NIF: 
# Valid wintunnel for Primary, loopback to nothing for secondary.
# Secondary delay on Starting Lower NIF
# Primary and Secondary.
############################################################################
[test26]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,192.168.2.4, 0, 2, 0, 0,RasUser,,,,194.72.6.51,194.72.6.51,0

# TRel99ContextConfig = <TName iContextName>,  <TUint iActivatePause>, <TUint iActivateErrorCode>, <TUint iDeactivatePause>, 
# <TUint iDeactivateErrorCode>, <TUint iDeletionPause>, <TUint iDeletionErrorCode> <TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, 0, 0, 0, 0, 0, 1
R99ContextConfig = SECONDARY1, 0, 0, 0, 0, 0, 0, 0

# delay creating TFT for secondary
CreateTftConfig = PRIMARY1, 0, 0, 60

# TFTfilter = 0<id> 1<evaluationPrecedenceIndex> 2<srcAddr> 3<srcAddrSubnetMask>  4<protocolNumberOrNextHeader>
#	      5<srcPortMin> 6<srcPortMax> 7<destPortMin> 8<destPortMax> 9<ipSecSPI> 10<toSorTrafficClass>
#	      11<flowLabel>
TFTfilter = 1, 0, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0

#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0
QosProfileReqR99 = SECONDARY1,0x04, 0x04, 0x02, 0x02, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x08, 0x08, 250, 250, -1, -1, 0, 0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY1,0x04, 0x04, 0x02, 0x02, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x08, 0x08, 250, 250, -1, -1, 0, 0, 0, 0


#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY2, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = SECONDARY2, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0

#TQosProfileCapsR99 = <trafficCap> <deliveryOrderReqCap> <deliverErroneousSDUCap>
#		      <BERCap> <SDUErrorRatioCap> <trafficHandlingPriorityCap>
QosProfileCapsR99= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04

QosNetworkNotificationType = PublishSubscribe
# QosNetworkNotification = <contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> <negMaxSDUSize>
QosNetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = PRIMARY2, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosR5NetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = PRIMARY2, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0


#SetProfileFail= <contextName> <numberOfTimes> <errorCode> <setProfileDigit>
SetProfileFail = NEG_99, 0x04, 0x02

#QosprofileReqGPRS= <minPrecedence> <reqPrecedence> <minDelay> <reqDelay> <minReliability> <reqReliability> <minPeek> <reqPeek>
#		    <minMean> <reqMean>
QosProfileReqGPRS= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020
QosProfileReqGPRS= 0x04, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020

#QosProfileNegGPRS=<negPrecedence> <negDelay><negReliability> <negPeek> <negMean>
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002

#QosProfileCapsGPRS=<negPrecedenceCap> <negDelayCap> <negReliabilityCap><negPeekCap> <negMeanCap>
QosProfileCapsGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002 

# QosProfileReq
# = <TTrafficClass>, <TTrafficClass>, <TDeliveryOrder>, <TDeliveryOrder>
# <TErroneousSDUDelivery>, <TErroneousSDUDelivery>
# <TErroneousSDUDelivery>, <TInt iReqMaxSDUSize>, <TInt iMinAcceptableMaxSDUSize>
# <TBitRate>, <TBitRate>, <TBitErrorRatio>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>, <TTrafficHandlingPriority>
# <TInt	iReqTransferDelay>, <TInt iMaxTransferDelay>, <TBitRate>, <TBitRate>

# QosProfileNeg = <TQoSPrecedence>, <TQoSDelay>, <TQoSReliability>, <TQoSPeakThroughput>, <TQoSMeanThroughput>
# <TTrafficClass>, <TDeliveryOrder>, <TErroneousSDUDelivery>, <TInt iMaxSDUSize>, <TBitRate>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>
# <TInt iTransferDelay>, <TBitRate>		

DefaultContextparamRel99= 3, ACME INTERNET PROVIDERS LTD, i-MODE GATEWAY, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2
# DefaultContextparamRel99 = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>

ReleaseMode = 5, 5
# Packet Release mode = <Release> <Duration>

#RegStatus=<duration> <regStat> <networkIndex> 
RegStatus= 5,3
RegStatus= 2,5,0
RegStatus= 2,7,3
RegStatus= 5,2
RegStatus= 2,5,0

# NetworkRegStatus = <Duration>, <RegistrationStatus>
NetworkRegStatusType = PublishSubscribe
NetworkRegStatus= 5,2
NetworkRegStatus= 5,1
NetworkRegStatus= 5,1

# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= ECUART, COMM::0, 18, 0, PRIMARY1
CommSetup= LOOPBACK, LOOPBACK::0, 18, 0, SECONDARY1


# Primary context loops back to nothing: this causes PPP LCP negotiation to take a long time.
[test27]
## Successful Start of Primary PDP context
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,192.168.2.4, 0, 2, 0, 0,RasUser,,,,194.72.6.51,194.72.6.51,0

# TRel99ContextConfig = <TName iContextName>,  <TUint iActivatePause>, <TUint iActivateErrorCode>, <TUint iDeactivatePause>, 
# <TUint iDeactivateErrorCode>, <TUint iDeletionPause>, <TUint iDeletionErrorCode> <TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, 0, 0, 0, 0, 0, 0


#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0

#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3

QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0



# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= LOOPBACK, LOOPBACK::0, 18, 0, PRIMARY1

