############################################################################
############################################################################
###################              T E S T 1              ####################
############################################################################
############################################################################
# Test case for success results
############################################################################
[test1]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,,0, 2, 0, 0,RasUser,,,,,,0

# TRel99ContextConfig = <TName iContextName>,  <TUint iActivatePause>, <TUint iActivateErrorCode>, <TUint iDeactivatePause>, 
# <TUint iDeactivateErrorCode>, <TUint iDeletionPause>, <TUint iDeletionErrorCode> <TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, 0, 0, 0, 0, 0, 0
R99ContextConfig = SECONDARY1, 0, 0, 0, 0, 0, 0, 0
R99ContextConfig = SECONDARY2, 0, 0, 0, 0, 0, 0, 0

# TFTfilter = 0<id> 1<evaluationPrecedenceIndex> 2<srcAddr> 3<srcAddrSubnetMask>  4<protocolNumberOrNextHeader>
#	      5<srcPortMin> 6<srcPortMax> 7<destPortMin> 8<destPortMax> 9<ipSecSPI> 10<toSorTrafficClass>
#	      11<flowLabel>
TFTfilter = 1, 96, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0
TFTfilter = 1, 0, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0
TFTfilter = 1, 1, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0

#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0
QosProfileReqR99 = SECONDARY1,0x04, 0x04, 0x01, 0x01, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 250, 250, -1, -1, 0, 0
QosProfileReqR99 = SECONDARY1,0x04, 0x04, 0x01, 0x01, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 250, 250, -1, -1, 0, 0
QosProfileReqR99 = SECONDARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0
QosProfileReqR99 = SECONDARY2,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY1,0x04, 0x04, 0x01, 0x01, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 250, 250, -1, -1, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY1,0x04, 0x04, 0x01, 0x01, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 250, 250, -1, -1, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY2,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0



#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY2, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = SECONDARY2, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0


#TQosProfileCapsR99 = <trafficCap> <deliveryOrderReqCap> <deliverErroneousSDUCap>
#		      <BERCap> <SDUErrorRatioCap> <trafficHandlingPriorityCap>
QosProfileCapsR99= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04

QosNetworkNotificationType = PublishSubscribe
# QosNetworkNotification = <contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> <negMaxSDUSize>
QosNetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = PRIMARY2, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosR5NetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = PRIMARY2, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0


#SetProfileFail= <contextName> <numberOfTimes> <errorCode> <setProfileDigit>
SetProfileFail = NEG_99, 0x04, 0x02

#QosprofileReqGPRS= <minPrecedence> <reqPrecedence> <minDelay> <reqDelay> <minReliability> <reqReliability> <minPeek> <reqPeek>
#		    <minMean> <reqMean>
QosProfileReqGPRS= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020
QosProfileReqGPRS= 0x04, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020

#QosProfileNegGPRS=<negPrecedence> <negDelay><negReliability> <negPeek> <negMean>
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002

#QosProfileCapsGPRS=<negPrecedenceCap> <negDelayCap> <negReliabilityCap><negPeekCap> <negMeanCap>
QosProfileCapsGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002 

# QosProfileReq
# = <TTrafficClass>, <TTrafficClass>, <TDeliveryOrder>, <TDeliveryOrder>
# <TErroneousSDUDelivery>, <TErroneousSDUDelivery>
# <TErroneousSDUDelivery>, <TInt iReqMaxSDUSize>, <TInt iMinAcceptableMaxSDUSize>
# <TBitRate>, <TBitRate>, <TBitErrorRatio>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>, <TTrafficHandlingPriority>
# <TInt	iReqTransferDelay>, <TInt iMaxTransferDelay>, <TBitRate>, <TBitRate>

# QosProfileNeg = <TQoSPrecedence>, <TQoSDelay>, <TQoSReliability>, <TQoSPeakThroughput>, <TQoSMeanThroughput>
# <TTrafficClass>, <TDeliveryOrder>, <TErroneousSDUDelivery>, <TInt iMaxSDUSize>, <TBitRate>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>
# <TInt iTransferDelay>, <TBitRate>		

DefaultContextparamRel99= 3, ACME INTERNET PROVIDERS LTD, i-MODE GATEWAY, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2
# DefaultContextparamRel99 = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>

ReleaseMode = 5, 5
# Packet Release mode = <Release> <Duration>

#RegStatus=<duration> <regStat> <networkIndex> 
RegStatus= 5,3
RegStatus= 2,5,0
RegStatus= 2,7,3
RegStatus= 5,2
RegStatus= 2,5,0

# NetworkRegStatus = <Duration>, <RegistrationStatus>
NetworkRegStatusType = PublishSubscribe
NetworkRegStatus= 5,2
NetworkRegStatus= 5,1
NetworkRegStatus= 5,1

# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= PKTLOOPBACK.CSY, PKTLOOPBACK::502, 18, 0, PRIMARY1
CommSetup= PKTLOOPBACK.CSY, PKTLOOPBACK::504, 18, 0, SECONDARY1
CommSetup= PKTLOOPBACK.CSY, PKTLOOPBACK::506, 18, 0, SECONDARY2

############################################################################
# failure events
# Configure the context's status to be changed using publish and subscribe
NotifyContextStatusChangeType = PublishSubscribe
# NotifyContextStatusChange <iContextName>, <iDuration>, <iStatus>

# EStatusDeactivating = 4 EStatusInactive = 1 EStatusDeleted = 6
NotifyContextStatusChange = PRIMARY1, 0, 6
NotifyContextStatusChange = PRIMARY1, 0, 4
NotifyContextStatusChange = PRIMARY1, 0, 1
NotifyContextStatusChange = SECONDARY1, 0, 6
NotifyContextStatusChange = SECONDARY1, 0, 4
NotifyContextStatusChange = SECONDARY1, 0, 1

# EStatusSuspended = 5 EStatusActive = 3
NotifyContextStatusChange = PRIMARY1, 0, 5
NotifyContextStatusChange = PRIMARY1, 0, 3
NotifyContextStatusChange = SECONDARY1, 0, 5
NotifyContextStatusChange = SECONDARY1, 0, 3

############################################################################
############################################################################
###################              T E S T 7 0 1          ####################
############################################################################
############################################################################
# This test messes up with QosProfileNegR99 entry to trigger KContextDelete on SPUDMAN
############################################################################
[test701]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,, 0, 2, 0, 0,RasUser,,,,,,0

# TRel99ContextConfig = <TName iContextName>,  <TUint iActivatePause>, <TUint iActivateErrorCode>, <TUint iDeactivatePause>, 
# <TUint iDeactivateErrorCode>, <TUint iDeletionPause>, <TUint iDeletionErrorCode> <TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, 0, 0, 0, 0, 0, 0
R99ContextConfig = SECONDARY1, 0, 0, 0, 0, 0, 0, 0
R99ContextConfig = SECONDARY2, 0, 0, 0, 0, 0, 0, 0

# TFTfilter = 0<id> 1<evaluationPrecedenceIndex> 2<srcAddr> 3<srcAddrSubnetMask>  4<protocolNumberOrNextHeader>
#	      5<srcPortMin> 6<srcPortMax> 7<destPortMin> 8<destPortMax> 9<ipSecSPI> 10<toSorTrafficClass>
#	      11<flowLabel>
TFTfilter = 1, 0, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0

#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0
QosProfileReqR99 = SECONDARY1,0x04, 0x04, 0x01, 0x01, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 250, 250, -1, -1, 0, 0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY1,0x04, 0x04, 0x01, 0x01, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 250, 250, -1, -1, 0, 0, 0, 0



#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 700, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY2, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4


QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 700, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = SECONDARY2, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0

#TQosProfileCapsR99 = <trafficCap> <deliveryOrderReqCap> <deliverErroneousSDUCap>
#		      <BERCap> <SDUErrorRatioCap> <trafficHandlingPriorityCap>
QosProfileCapsR99= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04

QosNetworkNotificationType = PublishSubscribe
# QosNetworkNotification = <contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> <negMaxSDUSize>
QosNetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = PRIMARY2, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosR5NetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = PRIMARY2, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0

#SetProfileFail= <contextName> <numberOfTimes> <errorCode> <setProfileDigit>
SetProfileFail = NEG_99, 0x04, 0x02

#QosprofileReqGPRS= <minPrecedence> <reqPrecedence> <minDelay> <reqDelay> <minReliability> <reqReliability> <minPeek> <reqPeek>
#		    <minMean> <reqMean>
QosProfileReqGPRS= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020
QosProfileReqGPRS= 0x04, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020

#QosProfileNegGPRS=<negPrecedence> <negDelay><negReliability> <negPeek> <negMean>
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002

#QosProfileCapsGPRS=<negPrecedenceCap> <negDelayCap> <negReliabilityCap><negPeekCap> <negMeanCap>
QosProfileCapsGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002 

# QosProfileReq
# = <TTrafficClass>, <TTrafficClass>, <TDeliveryOrder>, <TDeliveryOrder>
# <TErroneousSDUDelivery>, <TErroneousSDUDelivery>
# <TErroneousSDUDelivery>, <TInt iReqMaxSDUSize>, <TInt iMinAcceptableMaxSDUSize>
# <TBitRate>, <TBitRate>, <TBitErrorRatio>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>, <TTrafficHandlingPriority>
# <TInt	iReqTransferDelay>, <TInt iMaxTransferDelay>, <TBitRate>, <TBitRate>

# QosProfileNeg = <TQoSPrecedence>, <TQoSDelay>, <TQoSReliability>, <TQoSPeakThroughput>, <TQoSMeanThroughput>
# <TTrafficClass>, <TDeliveryOrder>, <TErroneousSDUDelivery>, <TInt iMaxSDUSize>, <TBitRate>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>
# <TInt iTransferDelay>, <TBitRate>		

DefaultContextparamRel99= 3, ACME INTERNET PROVIDERS LTD, i-MODE GATEWAY, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2
# DefaultContextparamRel99 = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>

ReleaseMode = 5, 5
# Packet Release mode = <Release> <Duration>

#RegStatus=<duration> <regStat> <networkIndex> 
RegStatus= 5,3
RegStatus= 2,5,0
RegStatus= 2,7,3
RegStatus= 5,2
RegStatus= 2,5,0

# NetworkRegStatus = <Duration>, <RegistrationStatus>
NetworkRegStatusType = PublishSubscribe
NetworkRegStatus= 5,2
NetworkRegStatus= 5,1
NetworkRegStatus= 5,1

# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= PKTLOOPBACK, PKTLOOPBACK::502, 18, 0, PRIMARY1
CommSetup= PKTLOOPBACK.CSY, PKTLOOPBACK::504, 18, 0, SECONDARY1

############################################################################
# failure events
# Configure the context's status to be changed using publish and subscribe
NotifyContextStatusChangeType = PublishSubscribe
# NotifyContextStatusChange <iContextName>, <iDuration>, <iStatus>

# EStatusInactive = 5 EStatusDeleted = 6)
NotifyContextStatusChange = PRIMARY1, 5, 6
NotifyContextStatusChange = PRIMARY1, 5, 5
NotifyContextStatusChange = SECONDARY1, 5, 6
NotifyContextStatusChange = SECONDARY1, 5, 5


############################################################################
############################################################################
###################              T E S T 8 0 1          ####################
############################################################################
############################################################################
# This test sets the R99ContextConfig's iActivateErrorCode to -4 for Primary PDP Context
############################################################################
[test801]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,, 0, 2, 0, 0,RasUser,,,,,,0

# TRel99ContextConfig = <TName iContextName>,  <TUint iActivatePause>, <TUint iActivateErrorCode>, <TUint iDeactivatePause>, 
# <TUint iDeactivateErrorCode>, <TUint iDeletionPause>, <TUint iDeletionErrorCode> <TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, -4, 0, 0, 0, 0, 0
R99ContextConfig = SECONDARY1, 0, 0, 0, 0, 0, 0, 0
R99ContextConfig = SECONDARY2, 0, 0, 0, 0, 0, 0, 0

# TFTfilter = 0<id> 1<evaluationPrecedenceIndex> 2<srcAddr> 3<srcAddrSubnetMask>  4<protocolNumberOrNextHeader>
#	      5<srcPortMin> 6<srcPortMax> 7<destPortMin> 8<destPortMax> 9<ipSecSPI> 10<toSorTrafficClass>
#	      11<flowLabel>
TFTfilter = 1, 0, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0

#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0
QosProfileReqR99 = SECONDARY1,0x04, 0x04, 0x02, 0x02, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x08, 0x08, 250, 250, -1, -1, 0, 0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY1,0x04, 0x04, 0x02, 0x02, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x08, 0x08, 250, 250, -1, -1, 0, 0, 0, 0



#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY2, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = SECONDARY2, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0



#TQosProfileCapsR99 = <trafficCap> <deliveryOrderReqCap> <deliverErroneousSDUCap>
#		      <BERCap> <SDUErrorRatioCap> <trafficHandlingPriorityCap>
QosProfileCapsR99= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04

QosNetworkNotificationType = PublishSubscribe
# QosNetworkNotification = <contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> <negMaxSDUSize>
QosNetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = PRIMARY2, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosR5NetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = PRIMARY2, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0

#SetProfileFail= <contextName> <numberOfTimes> <errorCode> <setProfileDigit>
SetProfileFail = NEG_99, 0x04, 0x02

#QosprofileReqGPRS= <minPrecedence> <reqPrecedence> <minDelay> <reqDelay> <minReliability> <reqReliability> <minPeek> <reqPeek>
#		    <minMean> <reqMean>
QosProfileReqGPRS= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020
QosProfileReqGPRS= 0x04, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020

#QosProfileNegGPRS=<negPrecedence> <negDelay><negReliability> <negPeek> <negMean>
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002

#QosProfileCapsGPRS=<negPrecedenceCap> <negDelayCap> <negReliabilityCap><negPeekCap> <negMeanCap>
QosProfileCapsGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002 

# QosProfileReq
# = <TTrafficClass>, <TTrafficClass>, <TDeliveryOrder>, <TDeliveryOrder>
# <TErroneousSDUDelivery>, <TErroneousSDUDelivery>
# <TErroneousSDUDelivery>, <TInt iReqMaxSDUSize>, <TInt iMinAcceptableMaxSDUSize>
# <TBitRate>, <TBitRate>, <TBitErrorRatio>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>, <TTrafficHandlingPriority>
# <TInt	iReqTransferDelay>, <TInt iMaxTransferDelay>, <TBitRate>, <TBitRate>

# QosProfileNeg = <TQoSPrecedence>, <TQoSDelay>, <TQoSReliability>, <TQoSPeakThroughput>, <TQoSMeanThroughput>
# <TTrafficClass>, <TDeliveryOrder>, <TErroneousSDUDelivery>, <TInt iMaxSDUSize>, <TBitRate>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>
# <TInt iTransferDelay>, <TBitRate>		

DefaultContextparamRel99= 3, ACME INTERNET PROVIDERS LTD, i-MODE GATEWAY, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2
# DefaultContextparamRel99 = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>

ReleaseMode = 5, 5
# Packet Release mode = <Release> <Duration>

#RegStatus=<duration> <regStat> <networkIndex> 
RegStatus= 5,3
RegStatus= 2,5,0
RegStatus= 2,7,3
RegStatus= 5,2
RegStatus= 2,5,0

# NetworkRegStatus = <Duration>, <RegistrationStatus>
NetworkRegStatusType = PublishSubscribe
NetworkRegStatus= 5,2
NetworkRegStatus= 5,1
NetworkRegStatus= 5,1

# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= PKTLOOPBACK, PKTLOOPBACK::502, 18, 0, PRIMARY1
CommSetup= PKTLOOPBACK.CSY, PKTLOOPBACK::504, 18, 0, SECONDARY1

############################################################################
# failure events
# Configure the context's status to be changed using publish and subscribe
NotifyContextStatusChangeType = PublishSubscribe
# NotifyContextStatusChange <iContextName>, <iDuration>, <iStatus>

# EStatusInactive = 5 EStatusDeleted = 6)
NotifyContextStatusChange = PRIMARY1, 5, 6
NotifyContextStatusChange = PRIMARY1, 5, 5
NotifyContextStatusChange = SECONDARY1, 5, 6
NotifyContextStatusChange = SECONDARY1, 5, 5


############################################################################
############################################################################
###################              T E S T 9 0 1          ####################
############################################################################
############################################################################
# This test sets the R99ContextConfig's iActivateErrorCode to -4 for Secondary PDP Context
############################################################################
[test901]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,, 0, 2, 0, 0,RasUser,,,,,,0

# TRel99ContextConfig = <TName iContextName>,  <TUint iActivatePause>, <TUint iActivateErrorCode>, <TUint iDeactivatePause>, 
# <TUint iDeactivateErrorCode>, <TUint iDeletionPause>, <TUint iDeletionErrorCode> <TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, 0, 0, 0, 0, 0, 0
R99ContextConfig = SECONDARY1, 0, -4, 0, 0, 0, 0, 0
R99ContextConfig = SECONDARY2, 0, 0, 0, 0, 0, 0, 0

# TFTfilter = 0<id> 1<evaluationPrecedenceIndex> 2<srcAddr> 3<srcAddrSubnetMask>  4<protocolNumberOrNextHeader>
#	      5<srcPortMin> 6<srcPortMax> 7<destPortMin> 8<destPortMax> 9<ipSecSPI> 10<toSorTrafficClass>
#	      11<flowLabel>
TFTfilter = 1, 0, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0

#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0
QosProfileReqR99 = SECONDARY1,0x04, 0x04, 0x01, 0x01, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 250, 250, -1, -1, 0, 0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY1,0x04, 0x04, 0x01, 0x01, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 250, 250, -1, -1, 0, 0, 0, 0



#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY2, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = SECONDARY2, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0


#TQosProfileCapsR99 = <trafficCap> <deliveryOrderReqCap> <deliverErroneousSDUCap>
#		      <BERCap> <SDUErrorRatioCap> <trafficHandlingPriorityCap>
QosProfileCapsR99= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04

QosNetworkNotificationType = PublishSubscribe
# QosNetworkNotification = <contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> <negMaxSDUSize>
QosNetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = PRIMARY2, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosR5NetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = PRIMARY2, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0

#SetProfileFail= <contextName> <numberOfTimes> <errorCode> <setProfileDigit>
SetProfileFail = NEG_99, 0x04, 0x02

#QosprofileReqGPRS= <minPrecedence> <reqPrecedence> <minDelay> <reqDelay> <minReliability> <reqReliability> <minPeek> <reqPeek>
#		    <minMean> <reqMean>
QosProfileReqGPRS= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020
QosProfileReqGPRS= 0x04, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020

#QosProfileNegGPRS=<negPrecedence> <negDelay><negReliability> <negPeek> <negMean>
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002

#QosProfileCapsGPRS=<negPrecedenceCap> <negDelayCap> <negReliabilityCap><negPeekCap> <negMeanCap>
QosProfileCapsGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002 

# QosProfileReq
# = <TTrafficClass>, <TTrafficClass>, <TDeliveryOrder>, <TDeliveryOrder>
# <TErroneousSDUDelivery>, <TErroneousSDUDelivery>
# <TErroneousSDUDelivery>, <TInt iReqMaxSDUSize>, <TInt iMinAcceptableMaxSDUSize>
# <TBitRate>, <TBitRate>, <TBitErrorRatio>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>, <TTrafficHandlingPriority>
# <TInt	iReqTransferDelay>, <TInt iMaxTransferDelay>, <TBitRate>, <TBitRate>

# QosProfileNeg = <TQoSPrecedence>, <TQoSDelay>, <TQoSReliability>, <TQoSPeakThroughput>, <TQoSMeanThroughput>
# <TTrafficClass>, <TDeliveryOrder>, <TErroneousSDUDelivery>, <TInt iMaxSDUSize>, <TBitRate>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>
# <TInt iTransferDelay>, <TBitRate>		

DefaultContextparamRel99= 3, ACME INTERNET PROVIDERS LTD, i-MODE GATEWAY, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2
# DefaultContextparamRel99 = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>

ReleaseMode = 5, 5
# Packet Release mode = <Release> <Duration>

#RegStatus=<duration> <regStat> <networkIndex> 
RegStatus= 5,3
RegStatus= 2,5,0
RegStatus= 2,7,3
RegStatus= 5,2
RegStatus= 2,5,0

# NetworkRegStatus = <Duration>, <RegistrationStatus>
NetworkRegStatusType = PublishSubscribe
NetworkRegStatus= 5,2
NetworkRegStatus= 5,1
NetworkRegStatus= 5,1

# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= PKTLOOPBACK, PKTLOOPBACK::502, 18, 0, PRIMARY1
CommSetup= PKTLOOPBACK.CSY, PKTLOOPBACK::504, 18, 0, SECONDARY1

############################################################################
# failure events
# Configure the context's status to be changed using publish and subscribe
NotifyContextStatusChangeType = PublishSubscribe
# NotifyContextStatusChange <iContextName>, <iDuration>, <iStatus>

# EStatusInactive = 5 EStatusDeleted = 6)
NotifyContextStatusChange = PRIMARY1, 5, 6
NotifyContextStatusChange = PRIMARY1, 5, 5
NotifyContextStatusChange = SECONDARY1, 5, 6
NotifyContextStatusChange = SECONDARY1, 5, 5


############################################################################
############################################################################
###################              T E S T 2 0 1          ####################
############################################################################
############################################################################
# Failure to Activate Primary PDP context
############################################################################
[test201]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,, 0, 2, 0, 0,RasUser,,,,,,0

# TRel99ContextConfig = <TName iContextName>,  <TUint iActivatePause>, <TUint iActivateErrorCode>, <TUint iDeactivatePause>, 
# <TUint iDeactivateErrorCode>, <TUint iDeletionPause>, <TUint iDeletionErrorCode> <TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, -19, 0, 0, 0, 0, 0
R99ContextConfig = PRIMARY1, 0, -19, 0, 0, 0, 0, 0

#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0


#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3

QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0

# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= PKTLOOPBACK, PKTLOOPBACK::502, 18, 0, PRIMARY1

############################################################################
############################################################################
###################              T E S T 2 1 0          ####################
############################################################################
############################################################################
# Failure to Start the Lower Nif for the Primary Context
############################################################################
[test210]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,, 0, 2, 0, 0,RasUser,,,,,,0

# TRel99ContextConfig = <TName iContextName>,  <TUint iActivatePause>, <TUint iActivateErrorCode>, <TUint iDeactivatePause>, 
# <TUint iDeactivateErrorCode>, <TUint iDeletionPause>, <TUint iDeletionErrorCode> <TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, 0, 0, 0, 0, 0, 0


#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0

#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3

QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0


# Supply an invalid port name for primary context to SPUD
# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= PKTLOOPBACK, INVALID::1, 18, 0, PRIMARY1

############################################################################
############################################################################
###################              T E S T 2 1 1          ####################
############################################################################
############################################################################
# 
############################################################################
NTRAS PPP
[test211]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,, 0, 2, 0, 0,RasUser,,,,,,0

# TRel99ContextConfig = <TName iContextName>,  <TUint iActivatePause>, <TUint iActivateErrorCode>, <TUint iDeactivatePause>, 
# <TUint iDeactivateErrorCode>, <TUint iDeletionPause>, <TUint iDeletionErrorCode> <TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, 0, 0, 0, 0, 0, 1


#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0

#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3

QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0

# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= ECUART, COMM::0, 18, 0, PRIMARY1

############################################################################
############################################################################
###################              T E S T 2 1 2         ####################
############################################################################
############################################################################
# 'la-la land loopback' PPP: No peer is provided, all LPC frames are discarded by the CSY.
# This results in the LCP negotiation taking as long as we want. This gives up time to inject events.
############################################################################
[test212]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,, 0, 2, 0, 0,RasUser,,,,,,0

# TRel99ContextConfig = <TName iContextName>,  <TUint iActivatePause>, <TUint iActivateErrorCode>, <TUint iDeactivatePause>, 
# <TUint iDeactivateErrorCode>, <TUint iDeletionPause>, <TUint iDeletionErrorCode> <TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, 0, 0, 0, 0, 0, 0


#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0

QosProfileReqR5  = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0

#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3

QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0

# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= PKTLOOPBACK, PKTLOOPBACK::0, 18, 0, PRIMARY1

############################################################################
# failure events
# Configure the context's status to be changed using publish and subscribe
NotifyContextStatusChangeType = PublishSubscribe
# NotifyContextStatusChange <iContextName>, <iDuration>, <iStatus>

# EStatusDeactivating = 4 EStatusInactive = 1 EStatusDeleted = 6
NotifyContextStatusChange = PRIMARY1, 0, 6
NotifyContextStatusChange = PRIMARY1, 0, 4
NotifyContextStatusChange = PRIMARY1, 0, 1
NotifyContextStatusChange = SECONDARY1, 0, 6
NotifyContextStatusChange = SECONDARY1, 0, 4
NotifyContextStatusChange = SECONDARY1, 0, 1

# EStatusSuspended = 5 EStatusActive = 3
NotifyContextStatusChange = PRIMARY1, 0, 5
NotifyContextStatusChange = PRIMARY1, 0, 3
NotifyContextStatusChange = SECONDARY1, 0, 5
NotifyContextStatusChange = SECONDARY1, 0, 3

############################################################################
############################################################################
###################              T E S T 3 0 1          ####################
############################################################################
############################################################################
# failure to activate secondary PDP context
############################################################################
[test301]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,, 0, 2, 0, 0,RasUser,,,,,,0

# TRel99ContextConfig = <TName iContextName>,  <TUint iActivatePause>, <TUint iActivateErrorCode>, <TUint iDeactivatePause>, 
# <TUint iDeactivateErrorCode>, <TUint iDeletionPause>, <TUint iDeletionErrorCode> <TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, 0, 0, 0, 0, 0, 0
R99ContextConfig = SECONDARY1, 0, -19, 0, 0, 0, 0, 0

# TFTfilter = 0<id> 1<evaluationPrecedenceIndex> 2<srcAddr> 3<srcAddrSubnetMask>  4<protocolNumberOrNextHeader>
#	      5<srcPortMin> 6<srcPortMax> 7<destPortMin> 8<destPortMax> 9<ipSecSPI> 10<toSorTrafficClass>
#	      11<flowLabel>
TFTfilter = 1, 0, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0


# Configure the context's status to be changed using publish and subscribe
NotifyContextStatusChangeType = PublishSubscribe
# NotifyContextStatusChange <iContextName>, <iDuration>, <iStatus>
# When the value 0 is published to KPSSimtsyPacketContextStatusChange the first primary context will be deleted (status = EStatusDeleted = 6)
NotifyContextStatusChange = SECONDARY1, 0, 6

#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0
QosProfileReqR99 = SECONDARY1,0x04, 0x04, 0x01, 0x01, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 250, 250, -1, -1, 0, 0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY1,0x04, 0x04, 0x01, 0x01, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 250, 250, -1, -1, 0, 0, 0, 0

#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3

QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0


#TQosProfileCapsR99 = <trafficCap> <deliveryOrderReqCap> <deliverErroneousSDUCap>
#		      <BERCap> <SDUErrorRatioCap> <trafficHandlingPriorityCap>
QosProfileCapsR99= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04

QosNetworkNotificationType = PublishSubscribe
# QosNetworkNotification = <contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> <negMaxSDUSize>
QosNetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosR5NetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0



#QosprofileReqGPRS= <minPrecedence> <reqPrecedence> <minDelay> <reqDelay> <minReliability> <reqReliability> <minPeek> <reqPeek>
#		    <minMean> <reqMean>
QosProfileReqGPRS= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020
QosProfileReqGPRS= 0x04, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020

#QosProfileNegGPRS=<negPrecedence> <negDelay><negReliability> <negPeek> <negMean>
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002

#QosProfileCapsGPRS=<negPrecedenceCap> <negDelayCap> <negReliabilityCap><negPeekCap> <negMeanCap>
QosProfileCapsGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002 

# QosProfileReq
# = <TTrafficClass>, <TTrafficClass>, <TDeliveryOrder>, <TDeliveryOrder>
# <TErroneousSDUDelivery>, <TErroneousSDUDelivery>
# <TErroneousSDUDelivery>, <TInt iReqMaxSDUSize>, <TInt iMinAcceptableMaxSDUSize>
# <TBitRate>, <TBitRate>, <TBitErrorRatio>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>, <TTrafficHandlingPriority>
# <TInt	iReqTransferDelay>, <TInt iMaxTransferDelay>, <TBitRate>, <TBitRate>

# QosProfileNeg = <TQoSPrecedence>, <TQoSDelay>, <TQoSReliability>, <TQoSPeakThroughput>, <TQoSMeanThroughput>
# <TTrafficClass>, <TDeliveryOrder>, <TErroneousSDUDelivery>, <TInt iMaxSDUSize>, <TBitRate>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>
# <TInt iTransferDelay>, <TBitRate>		

DefaultContextparamRel99= 3, ACME INTERNET PROVIDERS LTD, i-MODE GATEWAY, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2
# DefaultContextparamRel99 = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>


# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= PKTLOOPBACK, PKTLOOPBACK::502, 18, 0, PRIMARY1
CommSetup= PKTLOOPBACK.CSY, PKTLOOPBACK::504, 18, 0, SECONDARY1

############################################################################
############################################################################
###################              T E S T 3 1 0          ####################
############################################################################
############################################################################
# failure to Start the lower NIF for the Secondary PDP context
############################################################################
[test310]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,, 0, 2, 0, 0,RasUser,,,,,,0

# TRel99ContextConfig = <TName iContextName>,  <TUint iActivatePause>, <TUint iActivateErrorCode>, <TUint iDeactivatePause>, 
# <TUint iDeactivateErrorCode>, <TUint iDeletionPause>, <TUint iDeletionErrorCode> <TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, 0, 0, 0, 0, 0, 0
R99ContextConfig = SECONDARY1, 0, 0, 0, 0, 0, 0, 0

# TFTfilter = 0<id> 1<evaluationPrecedenceIndex> 2<srcAddr> 3<srcAddrSubnetMask>  4<protocolNumberOrNextHeader>
#	      5<srcPortMin> 6<srcPortMax> 7<destPortMin> 8<destPortMax> 9<ipSecSPI> 10<toSorTrafficClass>
#	      11<flowLabel>
TFTfilter = 1, 0, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0


# Configure the context's status to be changed using publish and subscribe
NotifyContextStatusChangeType = PublishSubscribe
# NotifyContextStatusChange <iContextName>, <iDuration>, <iStatus>
# When the value 0 is published to KPSSimtsyPacketContextStatusChange the first primary context will be deleted (status = EStatusDeleted = 6)
NotifyContextStatusChange = SECONDARY1, 0, 6

#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0
QosProfileReqR99 = SECONDARY1,0x04, 0x04, 0x01, 0x01, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 250, 250, -1, -1, 0, 0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY1,0x04, 0x04, 0x01, 0x01, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 250, 250, -1, -1, 0, 0, 0, 0


#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3

QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0

#TQosProfileCapsR99 = <trafficCap> <deliveryOrderReqCap> <deliverErroneousSDUCap>
#		      <BERCap> <SDUErrorRatioCap> <trafficHandlingPriorityCap>
QosProfileCapsR99= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04

QosNetworkNotificationType = PublishSubscribe
# QosNetworkNotification = <contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> <negMaxSDUSize>
QosNetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosR5NetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0


#QosprofileReqGPRS= <minPrecedence> <reqPrecedence> <minDelay> <reqDelay> <minReliability> <reqReliability> <minPeek> <reqPeek>
#		    <minMean> <reqMean>
QosProfileReqGPRS= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020
QosProfileReqGPRS= 0x04, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020

#QosProfileNegGPRS=<negPrecedence> <negDelay><negReliability> <negPeek> <negMean>
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002

#QosProfileCapsGPRS=<negPrecedenceCap> <negDelayCap> <negReliabilityCap><negPeekCap> <negMeanCap>
QosProfileCapsGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002 

# QosProfileReq
# = <TTrafficClass>, <TTrafficClass>, <TDeliveryOrder>, <TDeliveryOrder>
# <TErroneousSDUDelivery>, <TErroneousSDUDelivery>
# <TErroneousSDUDelivery>, <TInt iReqMaxSDUSize>, <TInt iMinAcceptableMaxSDUSize>
# <TBitRate>, <TBitRate>, <TBitErrorRatio>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>, <TTrafficHandlingPriority>
# <TInt	iReqTransferDelay>, <TInt iMaxTransferDelay>, <TBitRate>, <TBitRate>

# QosProfileNeg = <TQoSPrecedence>, <TQoSDelay>, <TQoSReliability>, <TQoSPeakThroughput>, <TQoSMeanThroughput>
# <TTrafficClass>, <TDeliveryOrder>, <TErroneousSDUDelivery>, <TInt iMaxSDUSize>, <TBitRate>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>
# <TInt iTransferDelay>, <TBitRate>		

DefaultContextparamRel99= 3, ACME INTERNET PROVIDERS LTD, i-MODE GATEWAY, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2
# DefaultContextparamRel99 = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>


# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= PKTLOOPBACK, PKTLOOPBACK::502, 18, 0, PRIMARY1
CommSetup= PKTLOOPBACK, INVALID_PORT::0, 18, 0, SECONDARY1

############################################################################
############################################################################
###################              T E S T 3 1 1          ####################
############################################################################
############################################################################
# failure to Start the lower NIF for the Secondary PDP context 
# (PPP as lower NIF)
############################################################################
[test311]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,, 0, 2, 0, 0,RasUser,,,,,,0

# TRel99ContextConfig = <TName iContextName>,  <TUint iActivatePause>, <TUint iActivateErrorCode>, <TUint iDeactivatePause>, 
# <TUint iDeactivateErrorCode>, <TUint iDeletionPause>, <TUint iDeletionErrorCode> <TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, 0, 0, 0, 0, 0, 1
R99ContextConfig = SECONDARY1, 0, 0, 0, 0, 0, 0, 0

# TFTfilter = 0<id> 1<evaluationPrecedenceIndex> 2<srcAddr> 3<srcAddrSubnetMask>  4<protocolNumberOrNextHeader>
#	      5<srcPortMin> 6<srcPortMax> 7<destPortMin> 8<destPortMax> 9<ipSecSPI> 10<toSorTrafficClass>
#	      11<flowLabel>
TFTfilter = 1, 0, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0


# Configure the context's status to be changed using publish and subscribe
NotifyContextStatusChangeType = PublishSubscribe
# NotifyContextStatusChange <iContextName>, <iDuration>, <iStatus>
# When the value 0 is published to KPSSimtsyPacketContextStatusChange the first primary context will be deleted (status = EStatusDeleted = 6)
NotifyContextStatusChange = SECONDARY1, 0, 6

#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0
QosProfileReqR99 = SECONDARY1,0x04, 0x04, 0x02, 0x02, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x08, 0x08, 250, 250, -1, -1, 0, 0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY1,0x04, 0x04, 0x02, 0x02, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x08, 0x08, 250, 250, -1, -1, 0, 0, 0, 0


#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3

QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0

#TQosProfileCapsR99 = <trafficCap> <deliveryOrderReqCap> <deliverErroneousSDUCap>
#		      <BERCap> <SDUErrorRatioCap> <trafficHandlingPriorityCap>
QosProfileCapsR99= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04

QosNetworkNotificationType = PublishSubscribe
# QosNetworkNotification = <contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> <negMaxSDUSize>
QosNetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosR5NetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0



#QosprofileReqGPRS= <minPrecedence> <reqPrecedence> <minDelay> <reqDelay> <minReliability> <reqReliability> <minPeek> <reqPeek>
#		    <minMean> <reqMean>
QosProfileReqGPRS= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020
QosProfileReqGPRS= 0x04, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020

#QosProfileNegGPRS=<negPrecedence> <negDelay><negReliability> <negPeek> <negMean>
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002

#QosProfileCapsGPRS=<negPrecedenceCap> <negDelayCap> <negReliabilityCap><negPeekCap> <negMeanCap>
QosProfileCapsGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002 

# QosProfileReq
# = <TTrafficClass>, <TTrafficClass>, <TDeliveryOrder>, <TDeliveryOrder>
# <TErroneousSDUDelivery>, <TErroneousSDUDelivery>
# <TErroneousSDUDelivery>, <TInt iReqMaxSDUSize>, <TInt iMinAcceptableMaxSDUSize>
# <TBitRate>, <TBitRate>, <TBitErrorRatio>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>, <TTrafficHandlingPriority>
# <TInt	iReqTransferDelay>, <TInt iMaxTransferDelay>, <TBitRate>, <TBitRate>

# QosProfileNeg = <TQoSPrecedence>, <TQoSDelay>, <TQoSReliability>, <TQoSPeakThroughput>, <TQoSMeanThroughput>
# <TTrafficClass>, <TDeliveryOrder>, <TErroneousSDUDelivery>, <TInt iMaxSDUSize>, <TBitRate>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>
# <TInt iTransferDelay>, <TBitRate>		

DefaultContextparamRel99= 3, ACME INTERNET PROVIDERS LTD, i-MODE GATEWAY, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2
# DefaultContextparamRel99 = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>


# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= ECUART, COMM::0, 18, 0, PRIMARY1
CommSetup= ECUART, INVALID::1, 18, 0, SECONDARY1

############################################################################
############################################################################
###################              T E S T 1 8            ####################
############################################################################
############################################################################
# R99ContextConfig ActivateErrorCode is modified to -19 for PRIMARY1. This 
# way primary context activation will fail with an error code (-19)
############################################################################
[test18]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,, 0, 2, 0, 0,RasUser,,,,,,0

# TRel99ContextConfig = 0<TName iContextName>,  1<TUint iActivatePause>, 2<TUint iActivateErrorCode>, 3<TUint iDeactivatePause>, 
# 4<TUint iDeactivateErrorCode>, 5<TUint iDeletionPause>, 6<TUint iDeletionErrorCode> 7<TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, -19, 0, 0, 0, 0, 0
R99ContextConfig = SECONDARY1, 0, 0, 0, 0, 0, 0, 0

# TFTfilter = 0<id> 1<evaluationPrecedenceIndex> 2<srcAddr> 3<srcAddrSubnetMask>  4<protocolNumberOrNextHeader>
#	      5<srcPortMin> 6<srcPortMax> 7<destPortMin> 8<destPortMax> 9<ipSecSPI> 10<toSorTrafficClass>
#	      11<flowLabel>
TFTfilter = 1, 0, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0

#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0
QosProfileReqR99 = SECONDARY1,0x04, 0x04, 0x02, 0x02, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x08, 0x08, 250, 250, -1, -1, 0, 0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY1,0x04, 0x04, 0x02, 0x02, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x08, 0x08, 250, 250, -1, -1, 0, 0, 0, 0


#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3

QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0


#TQosProfileCapsR99 = <trafficCap> <deliveryOrderReqCap> <deliverErroneousSDUCap>
#		      <BERCap> <SDUErrorRatioCap> <trafficHandlingPriorityCap>
QosProfileCapsR99= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04

QosNetworkNotificationType = PublishSubscribe
# QosNetworkNotification = <contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> <negMaxSDUSize>
QosNetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosR5NetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0

#SetProfileFail= <contextName> <numberOfTimes> <errorCode> <setProfileDigit>
SetProfileFail = NEG_99, 0x04, 0x02

#QosprofileReqGPRS= <minPrecedence> <reqPrecedence> <minDelay> <reqDelay> <minReliability> <reqReliability> <minPeek> <reqPeek>
#		    <minMean> <reqMean>
QosProfileReqGPRS= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020
QosProfileReqGPRS= 0x04, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020

#QosProfileNegGPRS=<negPrecedence> <negDelay><negReliability> <negPeek> <negMean>
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002

#QosProfileCapsGPRS=<negPrecedenceCap> <negDelayCap> <negReliabilityCap><negPeekCap> <negMeanCap>
QosProfileCapsGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002 

# QosProfileReq
# = <TTrafficClass>, <TTrafficClass>, <TDeliveryOrder>, <TDeliveryOrder>
# <TErroneousSDUDelivery>, <TErroneousSDUDelivery>
# <TErroneousSDUDelivery>, <TInt iReqMaxSDUSize>, <TInt iMinAcceptableMaxSDUSize>
# <TBitRate>, <TBitRate>, <TBitErrorRatio>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>, <TTrafficHandlingPriority>
# <TInt	iReqTransferDelay>, <TInt iMaxTransferDelay>, <TBitRate>, <TBitRate>

# QosProfileNeg = <TQoSPrecedence>, <TQoSDelay>, <TQoSReliability>, <TQoSPeakThroughput>, <TQoSMeanThroughput>
# <TTrafficClass>, <TDeliveryOrder>, <TErroneousSDUDelivery>, <TInt iMaxSDUSize>, <TBitRate>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>
# <TInt iTransferDelay>, <TBitRate>		

DefaultContextparamRel99= 3, ACME INTERNET PROVIDERS LTD, i-MODE GATEWAY, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2
# DefaultContextparamRel99 = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>

ReleaseMode = 5, 5
# Packet Release mode = <Release> <Duration>

#RegStatus=<duration> <regStat> <networkIndex> 
RegStatus= 5,3
RegStatus= 2,5,0
RegStatus= 2,7,3
RegStatus= 5,2
RegStatus= 2,5,0

# NetworkRegStatus = <Duration>, <RegistrationStatus>
NetworkRegStatusType = PublishSubscribe
NetworkRegStatus= 5,2
NetworkRegStatus= 5,1
NetworkRegStatus= 5,1

# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= PKTLOOPBACK, PKTLOOPBACK::502, 18, 0, PRIMARY1
CommSetup= PKTLOOPBACK.CSY, PKTLOOPBACK::504, 18, 0, SECONDARY1

############################################################################
############################################################################
###################              T E S T 1 9            ####################
############################################################################
############################################################################
# TFT filter, srcAddr value is modified so that the secondary context 
# creation fails due to TFT settings failure.
############################################################################
[test19]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,, 0, 2, 0, 0,RasUser,,,,,,0

# TRel99ContextConfig = 0<TName iContextName>,  1<TUint iActivatePause>, 2<TUint iActivateErrorCode>, 3<TUint iDeactivatePause>, 
# 4<TUint iDeactivateErrorCode>, 5<TUint iDeletionPause>, 6<TUint iDeletionErrorCode> 7<TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, 0, 0, 0, 0, 0, 0
R99ContextConfig = SECONDARY1, 0, 0, 0, 0, 0, 0, 0

# TFTfilter = 0<id> 1<evaluationPrecedenceIndex> 2<srcAddr> 3<srcAddrSubnetMask>  4<protocolNumberOrNextHeader>
#	      5<srcPortMin> 6<srcPortMax> 7<destPortMin> 8<destPortMax> 9<ipSecSPI> 10<toSorTrafficClass>
#	      11<flowLabel>
TFTfilter = 1, 0, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.3, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0

#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0
QosProfileReqR99 = SECONDARY1,0x04, 0x04, 0x02, 0x02, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x08, 0x08, 250, 250, -1, -1, 0, 0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY1,0x04, 0x04, 0x02, 0x02, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x08, 0x08, 250, 250, -1, -1, 0, 0, 0, 0

#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3

QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0

#TQosProfileCapsR99 = <trafficCap> <deliveryOrderReqCap> <deliverErroneousSDUCap>
#		      <BERCap> <SDUErrorRatioCap> <trafficHandlingPriorityCap>
QosProfileCapsR99= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04

QosNetworkNotificationType = PublishSubscribe
# QosNetworkNotification = <contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> <negMaxSDUSize>
QosNetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosR5NetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0

#SetProfileFail= <contextName> <numberOfTimes> <errorCode> <setProfileDigit>
SetProfileFail = NEG_99, 0x04, 0x02

#QosprofileReqGPRS= <minPrecedence> <reqPrecedence> <minDelay> <reqDelay> <minReliability> <reqReliability> <minPeek> <reqPeek>
#		    <minMean> <reqMean>
QosProfileReqGPRS= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020
QosProfileReqGPRS= 0x04, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020

#QosProfileNegGPRS=<negPrecedence> <negDelay><negReliability> <negPeek> <negMean>
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002

#QosProfileCapsGPRS=<negPrecedenceCap> <negDelayCap> <negReliabilityCap><negPeekCap> <negMeanCap>
QosProfileCapsGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002 

# QosProfileReq
# = <TTrafficClass>, <TTrafficClass>, <TDeliveryOrder>, <TDeliveryOrder>
# <TErroneousSDUDelivery>, <TErroneousSDUDelivery>
# <TErroneousSDUDelivery>, <TInt iReqMaxSDUSize>, <TInt iMinAcceptableMaxSDUSize>
# <TBitRate>, <TBitRate>, <TBitErrorRatio>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>, <TTrafficHandlingPriority>
# <TInt	iReqTransferDelay>, <TInt iMaxTransferDelay>, <TBitRate>, <TBitRate>

# QosProfileNeg = <TQoSPrecedence>, <TQoSDelay>, <TQoSReliability>, <TQoSPeakThroughput>, <TQoSMeanThroughput>
# <TTrafficClass>, <TDeliveryOrder>, <TErroneousSDUDelivery>, <TInt iMaxSDUSize>, <TBitRate>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>
# <TInt iTransferDelay>, <TBitRate>		

DefaultContextparamRel99= 3, ACME INTERNET PROVIDERS LTD, i-MODE GATEWAY, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2
# DefaultContextparamRel99 = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>

ReleaseMode = 5, 5
# Packet Release mode = <Release> <Duration>

#RegStatus=<duration> <regStat> <networkIndex> 
RegStatus= 5,3
RegStatus= 2,5,0
RegStatus= 2,7,3
RegStatus= 5,2
RegStatus= 2,5,0

# NetworkRegStatus = <Duration>, <RegistrationStatus>
NetworkRegStatusType = PublishSubscribe
NetworkRegStatus= 5,2
NetworkRegStatus= 5,1
NetworkRegStatus= 5,1

# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= PKTLOOPBACK, PKTLOOPBACK::502, 18, 0, PRIMARY1
CommSetup= PKTLOOPBACK.CSY, PKTLOOPBACK::504, 18, 0, SECONDARY1


############################################################################
############################################################################
###################              T E S T 2 0            ####################
############################################################################
############################################################################
# QosProfileReqR99 for SECONDARY1 reqTraffic and minTraffic values are 
# modified so that secondary PDP context creation fails due to Requested QoS
# parameter mismatch.
############################################################################
[test20]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,, 0, 2, 0, 0,RasUser,,,,,,0

# TRel99ContextConfig = 0<TName iContextName>,  1<TUint iActivatePause>, 2<TUint iActivateErrorCode>, 3<TUint iDeactivatePause>, 
# 4<TUint iDeactivateErrorCode>, 5<TUint iDeletionPause>, 6<TUint iDeletionErrorCode> 7<TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, 0, 0, 0, 0, 0, 0
R99ContextConfig = SECONDARY1, 0, 0, 0, 0, 0, 0, 0

# TFTfilter = 0<id> 1<evaluationPrecedenceIndex> 2<srcAddr> 3<srcAddrSubnetMask>  4<protocolNumberOrNextHeader>
#	      5<srcPortMin> 6<srcPortMax> 7<destPortMin> 8<destPortMax> 9<ipSecSPI> 10<toSorTrafficClass>
#	      11<flowLabel>
TFTfilter = 1, 0, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0

#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0
QosProfileReqR99 = SECONDARY1,0x08, 0x08, 0x02, 0x02, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x08, 0x08, 250, 250, -1, -1, 0, 0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY1,0x08, 0x08, 0x02, 0x02, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x08, 0x08, 250, 250, -1, -1, 0, 0, 0, 0


#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3

QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0


#TQosProfileCapsR99 = <trafficCap> <deliveryOrderReqCap> <deliverErroneousSDUCap>
#		      <BERCap> <SDUErrorRatioCap> <trafficHandlingPriorityCap>
QosProfileCapsR99= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04

QosNetworkNotificationType = PublishSubscribe
# QosNetworkNotification = <contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> <negMaxSDUSize>
QosNetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosR5NetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0

#SetProfileFail= <contextName> <numberOfTimes> <errorCode> <setProfileDigit>
SetProfileFail = NEG_99, 0x04, 0x02

#QosprofileReqGPRS= <minPrecedence> <reqPrecedence> <minDelay> <reqDelay> <minReliability> <reqReliability> <minPeek> <reqPeek>
#		    <minMean> <reqMean>
QosProfileReqGPRS= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020
QosProfileReqGPRS= 0x04, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020

#QosProfileNegGPRS=<negPrecedence> <negDelay><negReliability> <negPeek> <negMean>
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002

#QosProfileCapsGPRS=<negPrecedenceCap> <negDelayCap> <negReliabilityCap><negPeekCap> <negMeanCap>
QosProfileCapsGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002 

# QosProfileReq
# = <TTrafficClass>, <TTrafficClass>, <TDeliveryOrder>, <TDeliveryOrder>
# <TErroneousSDUDelivery>, <TErroneousSDUDelivery>
# <TErroneousSDUDelivery>, <TInt iReqMaxSDUSize>, <TInt iMinAcceptableMaxSDUSize>
# <TBitRate>, <TBitRate>, <TBitErrorRatio>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>, <TTrafficHandlingPriority>
# <TInt	iReqTransferDelay>, <TInt iMaxTransferDelay>, <TBitRate>, <TBitRate>

# QosProfileNeg = <TQoSPrecedence>, <TQoSDelay>, <TQoSReliability>, <TQoSPeakThroughput>, <TQoSMeanThroughput>
# <TTrafficClass>, <TDeliveryOrder>, <TErroneousSDUDelivery>, <TInt iMaxSDUSize>, <TBitRate>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>
# <TInt iTransferDelay>, <TBitRate>		

DefaultContextparamRel99= 3, ACME INTERNET PROVIDERS LTD, i-MODE GATEWAY, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2
# DefaultContextparamRel99 = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>

ReleaseMode = 5, 5
# Packet Release mode = <Release> <Duration>

#RegStatus=<duration> <regStat> <networkIndex> 
RegStatus= 5,3
RegStatus= 2,5,0
RegStatus= 2,7,3
RegStatus= 5,2
RegStatus= 2,5,0

# NetworkRegStatus = <Duration>, <RegistrationStatus>
NetworkRegStatusType = PublishSubscribe
NetworkRegStatus= 5,2
NetworkRegStatus= 5,1
NetworkRegStatus= 5,1

# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= PKTLOOPBACK, PKTLOOPBACK::502, 18, 0, PRIMARY1
CommSetup= PKTLOOPBACK.CSY, PKTLOOPBACK::504, 18, 0, SECONDARY1

############################################################################
############################################################################
###################              T E S T 2 1            ####################
############################################################################
############################################################################
# R99ContextConfig DeletionErrorCode is modified to -19 for PRIMARY1. This 
# way primary context deletion will fail with an error code (-19)
############################################################################
[test21]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,, 0, 2, 0, 0,RasUser,,,,,,0

# TRel99ContextConfig = 0<TName iContextName>,  1<TUint iActivatePause>, 2<TUint iActivateErrorCode>, 3<TUint iDeactivatePause>, 
# 4<TUint iDeactivateErrorCode>, 5<TUint iDeletionPause>, 6<TUint iDeletionErrorCode> 7<TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, 0, 0, 0, 0, -19, 0
R99ContextConfig = SECONDARY1, 0, 0, 0, 0, 0, 0, 0

# TFTfilter = 0<id> 1<evaluationPrecedenceIndex> 2<srcAddr> 3<srcAddrSubnetMask>  4<protocolNumberOrNextHeader>
#	      5<srcPortMin> 6<srcPortMax> 7<destPortMin> 8<destPortMax> 9<ipSecSPI> 10<toSorTrafficClass>
#	      11<flowLabel>
TFTfilter = 1, 0, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0

#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0
QosProfileReqR99 = SECONDARY1,0x04, 0x04, 0x02, 0x02, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x08, 0x08, 250, 250, -1, -1, 0, 0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY1,0x04, 0x04, 0x02, 0x02, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x08, 0x08, 250, 250, -1, -1, 0, 0, 0, 0


#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3

QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0

#TQosProfileCapsR99 = <trafficCap> <deliveryOrderReqCap> <deliverErroneousSDUCap>
#		      <BERCap> <SDUErrorRatioCap> <trafficHandlingPriorityCap>
QosProfileCapsR99= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04

QosNetworkNotificationType = PublishSubscribe
# QosNetworkNotification = <contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> <negMaxSDUSize>
QosNetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosR5NetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0

#SetProfileFail= <contextName> <numberOfTimes> <errorCode> <setProfileDigit>
SetProfileFail = NEG_99, 0x04, 0x02

#QosprofileReqGPRS= <minPrecedence> <reqPrecedence> <minDelay> <reqDelay> <minReliability> <reqReliability> <minPeek> <reqPeek>
#		    <minMean> <reqMean>
QosProfileReqGPRS= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020
QosProfileReqGPRS= 0x04, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020

#QosProfileNegGPRS=<negPrecedence> <negDelay><negReliability> <negPeek> <negMean>
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002

#QosProfileCapsGPRS=<negPrecedenceCap> <negDelayCap> <negReliabilityCap><negPeekCap> <negMeanCap>
QosProfileCapsGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002 

# QosProfileReq
# = <TTrafficClass>, <TTrafficClass>, <TDeliveryOrder>, <TDeliveryOrder>
# <TErroneousSDUDelivery>, <TErroneousSDUDelivery>
# <TErroneousSDUDelivery>, <TInt iReqMaxSDUSize>, <TInt iMinAcceptableMaxSDUSize>
# <TBitRate>, <TBitRate>, <TBitErrorRatio>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>, <TTrafficHandlingPriority>
# <TInt	iReqTransferDelay>, <TInt iMaxTransferDelay>, <TBitRate>, <TBitRate>

# QosProfileNeg = <TQoSPrecedence>, <TQoSDelay>, <TQoSReliability>, <TQoSPeakThroughput>, <TQoSMeanThroughput>
# <TTrafficClass>, <TDeliveryOrder>, <TErroneousSDUDelivery>, <TInt iMaxSDUSize>, <TBitRate>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>
# <TInt iTransferDelay>, <TBitRate>		

DefaultContextparamRel99= 3, ACME INTERNET PROVIDERS LTD, i-MODE GATEWAY, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2
# DefaultContextparamRel99 = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>

ReleaseMode = 5, 5
# Packet Release mode = <Release> <Duration>

#RegStatus=<duration> <regStat> <networkIndex> 
RegStatus= 5,3
RegStatus= 2,5,0
RegStatus= 2,7,3
RegStatus= 5,2
RegStatus= 2,5,0

# NetworkRegStatus = <Duration>, <RegistrationStatus>
NetworkRegStatusType = PublishSubscribe
NetworkRegStatus= 5,2
NetworkRegStatus= 5,1
NetworkRegStatus= 5,1

# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= PKTLOOPBACK, PKTLOOPBACK::502, 18, 0, PRIMARY1
CommSetup= PKTLOOPBACK.CSY, PKTLOOPBACK::504, 18, 0, SECONDARY1


############################################################################
############################################################################
###################              T E S T 2 2            ####################
############################################################################
############################################################################
# R99ContextConfig DeletionErrorCode is modified to -19 for SECONDARY1. This 
# way primary context deletion will fail with an error code (-19)
############################################################################
[test22]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,, 0, 2, 0, 0,RasUser,,,,,,0

# TRel99ContextConfig = 0<TName iContextName>,  1<TUint iActivatePause>, 2<TUint iActivateErrorCode>, 3<TUint iDeactivatePause>, 
# 4<TUint iDeactivateErrorCode>, 5<TUint iDeletionPause>, 6<TUint iDeletionErrorCode> 7<TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, 0, 0, 0, 0, 0, 0
R99ContextConfig = SECONDARY1, 0, 0, 0, 0, 0, -19, 0

# TFTfilter = 0<id> 1<evaluationPrecedenceIndex> 2<srcAddr> 3<srcAddrSubnetMask>  4<protocolNumberOrNextHeader>
#	      5<srcPortMin> 6<srcPortMax> 7<destPortMin> 8<destPortMax> 9<ipSecSPI> 10<toSorTrafficClass>
#	      11<flowLabel>
TFTfilter = 1, 0, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0

#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0
QosProfileReqR99 = SECONDARY1,0x04, 0x04, 0x01, 0x01, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 250, 250, -1, -1, 0, 0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY1,0x04, 0x04, 0x01, 0x01, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 250, 250, -1, -1, 0, 0, 0, 0

#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3

QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0

#TQosProfileCapsR99 = <trafficCap> <deliveryOrderReqCap> <deliverErroneousSDUCap>
#		      <BERCap> <SDUErrorRatioCap> <trafficHandlingPriorityCap>
QosProfileCapsR99= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04

QosNetworkNotificationType = PublishSubscribe
# QosNetworkNotification = <contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> <negMaxSDUSize>
QosNetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosR5NetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0

#SetProfileFail= <contextName> <numberOfTimes> <errorCode> <setProfileDigit>
SetProfileFail = NEG_99, 0x04, 0x02

#QosprofileReqGPRS= <minPrecedence> <reqPrecedence> <minDelay> <reqDelay> <minReliability> <reqReliability> <minPeek> <reqPeek>
#		    <minMean> <reqMean>
QosProfileReqGPRS= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020
QosProfileReqGPRS= 0x04, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020

#QosProfileNegGPRS=<negPrecedence> <negDelay><negReliability> <negPeek> <negMean>
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002

#QosProfileCapsGPRS=<negPrecedenceCap> <negDelayCap> <negReliabilityCap><negPeekCap> <negMeanCap>
QosProfileCapsGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002 

# QosProfileReq
# = <TTrafficClass>, <TTrafficClass>, <TDeliveryOrder>, <TDeliveryOrder>
# <TErroneousSDUDelivery>, <TErroneousSDUDelivery>
# <TErroneousSDUDelivery>, <TInt iReqMaxSDUSize>, <TInt iMinAcceptableMaxSDUSize>
# <TBitRate>, <TBitRate>, <TBitErrorRatio>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>, <TTrafficHandlingPriority>
# <TInt	iReqTransferDelay>, <TInt iMaxTransferDelay>, <TBitRate>, <TBitRate>

# QosProfileNeg = <TQoSPrecedence>, <TQoSDelay>, <TQoSReliability>, <TQoSPeakThroughput>, <TQoSMeanThroughput>
# <TTrafficClass>, <TDeliveryOrder>, <TErroneousSDUDelivery>, <TInt iMaxSDUSize>, <TBitRate>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>
# <TInt iTransferDelay>, <TBitRate>		

DefaultContextparamRel99= 3, ACME INTERNET PROVIDERS LTD, i-MODE GATEWAY, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2
# DefaultContextparamRel99 = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>

ReleaseMode = 5, 5
# Packet Release mode = <Release> <Duration>

#RegStatus=<duration> <regStat> <networkIndex> 
RegStatus= 5,3
RegStatus= 2,5,0
RegStatus= 2,7,3
RegStatus= 5,2
RegStatus= 2,5,0

# NetworkRegStatus = <Duration>, <RegistrationStatus>
NetworkRegStatusType = PublishSubscribe
NetworkRegStatus= 5,2
NetworkRegStatus= 5,1
NetworkRegStatus= 5,1

# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= PKTLOOPBACK, PKTLOOPBACK::502, 18, 0, PRIMARY1
CommSetup= PKTLOOPBACK.CSY, PKTLOOPBACK::504, 18, 0, SECONDARY1

############################################################################
############################################################################
###################              T E S T 24             ####################
############################################################################
############################################################################
[test24]
PhoneInitialiseDelay = 999

############################################################################
############################################################################
############################################################################
############################################################################

############################################################################
############################################################################
###################              T E S T 25             ####################
############################################################################
############################################################################
# Test case for success results
############################################################################
[test25]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,,0, 2, 0, 0,RasUser,,,,,,0

# TRel99ContextConfig = <TName iContextName>,  <TUint iActivatePause>, <TUint iActivateErrorCode>, <TUint iDeactivatePause>, 
# <TUint iDeactivateErrorCode>, <TUint iDeletionPause>, <TUint iDeletionErrorCode> <TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, 0, 0, 0, 0, 0, 0
R99ContextConfig = PRIMARY2, 0, 0, 0, 0, 0, 0, 0
R99ContextConfig = PRIMARY3, 0, 0, 0, 0, 0, 0, 0
R99ContextConfig = PRIMARY4, 0, 0, 0, 0, 0, 0, 0
R99ContextConfig = PRIMARY5, 0, 0, 0, 0, 0, 0, 0
R99ContextConfig = SECONDARY1, 0, 0, 0, 0, 0, 0, 0
R99ContextConfig = SECONDARY2, 0, 0, 0, 0, 0, 0, 0

# TFTfilter = 0<id> 1<evaluationPrecedenceIndex> 2<srcAddr> 3<srcAddrSubnetMask>  4<protocolNumberOrNextHeader>
#	      5<srcPortMin> 6<srcPortMax> 7<destPortMin> 8<destPortMax> 9<ipSecSPI> 10<toSorTrafficClass>
#	      11<flowLabel>
TFTfilter = 1, 96, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0
TFTfilter = 1, 0, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0
TFTfilter = 1, 1, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0

#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0
QosProfileReqR99 = PRIMARY2,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0
QosProfileReqR99 = PRIMARY3,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0
QosProfileReqR99 = PRIMARY4,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0
QosProfileReqR99 = PRIMARY5,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0
QosProfileReqR99 = SECONDARY1,0x04, 0x04, 0x01, 0x01, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 250, 250, -1, -1, 0, 0
QosProfileReqR99 = SECONDARY1,0x04, 0x04, 0x01, 0x01, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 250, 250, -1, -1, 0, 0
QosProfileReqR99 = SECONDARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0
QosProfileReqR99 = SECONDARY2,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = PRIMARY2,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = PRIMARY3,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = PRIMARY4,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = PRIMARY5,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY1,0x04, 0x04, 0x01, 0x01, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 250, 250, -1, -1, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY1,0x04, 0x04, 0x01, 0x01, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 250, 250, -1, -1, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY2,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0

#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosProfileNegR99 = PRIMARY2, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = PRIMARY3, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = PRIMARY4, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = PRIMARY5, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY2, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosProfileNegR5 = PRIMARY2, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = PRIMARY3, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = PRIMARY4, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = PRIMARY5, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = SECONDARY2, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0

#TQosProfileCapsR99 = <trafficCap> <deliveryOrderReqCap> <deliverErroneousSDUCap>
#		      <BERCap> <SDUErrorRatioCap> <trafficHandlingPriorityCap>
QosProfileCapsR99= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04

QosNetworkNotificationType = PublishSubscribe
# QosNetworkNotification = <contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> <negMaxSDUSize>
QosNetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = PRIMARY2, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = PRIMARY3, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = PRIMARY4, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = PRIMARY5, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4


QosR5NetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = PRIMARY2, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = PRIMARY3, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = PRIMARY4, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = PRIMARY5, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0


#SetProfileFail= <contextName> <numberOfTimes> <errorCode> <setProfileDigit>
SetProfileFail = NEG_99, 0x04, 0x02

#QosprofileReqGPRS= <minPrecedence> <reqPrecedence> <minDelay> <reqDelay> <minReliability> <reqReliability> <minPeek> <reqPeek>
#		    <minMean> <reqMean>
QosProfileReqGPRS= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020
QosProfileReqGPRS= 0x04, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020

#QosProfileNegGPRS=<negPrecedence> <negDelay><negReliability> <negPeek> <negMean>
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002

#QosProfileCapsGPRS=<negPrecedenceCap> <negDelayCap> <negReliabilityCap><negPeekCap> <negMeanCap>
QosProfileCapsGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002 

# QosProfileReq
# = <TTrafficClass>, <TTrafficClass>, <TDeliveryOrder>, <TDeliveryOrder>
# <TErroneousSDUDelivery>, <TErroneousSDUDelivery>
# <TErroneousSDUDelivery>, <TInt iReqMaxSDUSize>, <TInt iMinAcceptableMaxSDUSize>
# <TBitRate>, <TBitRate>, <TBitErrorRatio>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>, <TTrafficHandlingPriority>
# <TInt	iReqTransferDelay>, <TInt iMaxTransferDelay>, <TBitRate>, <TBitRate>

# QosProfileNeg = <TQoSPrecedence>, <TQoSDelay>, <TQoSReliability>, <TQoSPeakThroughput>, <TQoSMeanThroughput>
# <TTrafficClass>, <TDeliveryOrder>, <TErroneousSDUDelivery>, <TInt iMaxSDUSize>, <TBitRate>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>
# <TInt iTransferDelay>, <TBitRate>		

DefaultContextparamRel99= 3, ACME INTERNET PROVIDERS LTD, i-MODE GATEWAY, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2
# DefaultContextparamRel99 = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>

ReleaseMode = 5, 5
# Packet Release mode = <Release> <Duration>

#RegStatus=<duration> <regStat> <networkIndex> 
RegStatus= 5,3
RegStatus= 2,5,0
RegStatus= 2,7,3
RegStatus= 5,2
RegStatus= 2,5,0

# NetworkRegStatus = <Duration>, <RegistrationStatus>
NetworkRegStatusType = PublishSubscribe
NetworkRegStatus= 5,2
NetworkRegStatus= 5,1
NetworkRegStatus= 5,1

# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= PKTLOOPBACK.CSY, PKTLOOPBACK::502, 18, 0, PRIMARY1
CommSetup= PKTLOOPBACK.CSY, PKTLOOPBACK::510, 18, 0, PRIMARY2
CommSetup= PKTLOOPBACK.CSY, PKTLOOPBACK::512, 18, 0, PRIMARY3
CommSetup= PKTLOOPBACK.CSY, PKTLOOPBACK::514, 18, 0, PRIMARY4
CommSetup= PKTLOOPBACK.CSY, PKTLOOPBACK::516, 18, 0, PRIMARY5
CommSetup= PKTLOOPBACK.CSY, PKTLOOPBACK::504, 18, 0, SECONDARY1
CommSetup= PKTLOOPBACK.CSY, PKTLOOPBACK::506, 18, 0, SECONDARY2

############################################################################
# failure events
# Configure the context's status to be changed using publish and subscribe
NotifyContextStatusChangeType = PublishSubscribe
# NotifyContextStatusChange <iContextName>, <iDuration>, <iStatus>

# EStatusDeactivating = 4 EStatusInactive = 1 EStatusDeleted = 6
NotifyContextStatusChange = PRIMARY1, 0, 6
NotifyContextStatusChange = PRIMARY1, 0, 4
NotifyContextStatusChange = PRIMARY1, 0, 1
NotifyContextStatusChange = PRIMARY2, 0, 6
NotifyContextStatusChange = PRIMARY3, 0, 6
NotifyContextStatusChange = PRIMARY4, 0, 6
NotifyContextStatusChange = PRIMARY5, 0, 6
NotifyContextStatusChange = SECONDARY1, 0, 6
NotifyContextStatusChange = SECONDARY1, 0, 4
NotifyContextStatusChange = SECONDARY1, 0, 1

# EStatusSuspended = 5 EStatusActive = 3
NotifyContextStatusChange = PRIMARY1, 0, 5
NotifyContextStatusChange = PRIMARY1, 0, 3
NotifyContextStatusChange = PRIMARY2, 0, 5
NotifyContextStatusChange = PRIMARY3, 0, 5
NotifyContextStatusChange = PRIMARY4, 0, 5
NotifyContextStatusChange = PRIMARY5, 0, 5
NotifyContextStatusChange = SECONDARY1, 0, 5
NotifyContextStatusChange = SECONDARY1, 0, 3


############################################################################
############################################################################
###################              T E S T 100              ####################
############################################################################
############################################################################
# Test case for success results
############################################################################
[test100]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,,0, 2, 0, 0,RasUser,,,,,,0

#SetContextConfigR5= <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <TUseEdge>, <Authentication Protocol>, <Username>, <Password>, <Challenge>,
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>, <THeaderCompression>, <TDataCompression>, <No. Additional Context Config Params>
SetContextConfigR5= 0, SYMBIAN INTERNET PROVIDER, PROTOCOL ADDRESS, 0, 2, USER3, PASSWORD3, CHALLENGE3, RESPONSE3, PRIMARYSERVER3, SECONDARYSERVER3, 3, 2, 1, 1

#AdditionalParamItem= <TPcoProtocolId>, <TBuf8 AdditionalParamData>
AdditionalParamItem= 0x04, ADDITIONALPARAM1

# TRel99ContextConfig = <TName iContextName>,  <TUint iActivatePause>, <TUint iActivateErrorCode>, <TUint iDeactivatePause>, 
# <TUint iDeactivateErrorCode>, <TUint iDeletionPause>, <TUint iDeletionErrorCode> <TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, 0, 0, 0, 0, 0, 0
R99ContextConfig = SECONDARY1, 0, 0, 0, 0, 0, 0, 0


# TFTfilter = 0<id> 1<evaluationPrecedenceIndex> 2<srcAddr> 3<srcAddrSubnetMask>  4<protocolNumberOrNextHeader>
#	      5<srcPortMin> 6<srcPortMax> 7<destPortMin> 8<destPortMax> 9<ipSecSPI> 10<toSorTrafficClass>
#	      11<flowLabel>
TFTfilter = 1, 96, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0
TFTfilter = 1, 0, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0
TFTfilter = 1, 1, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0

#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>

QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0

QosProfileReqR99 = SECONDARY1,0x04, 0x04, 0x04, 0x01, 0x08, 0x08, -1, -1, -1, -1,0,0, 0x20, 1, 0x10 ,1 ,2 ,1 ,1 ,250 ,-1 ,-1 ,0 ,0
#Added for test case 29
QosProfileReqR99 = SECONDARY1,0x04, 0x04, 0x01, 0x01, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 250, 250, -1, -1, 0, 0
#Added for test case 30
QosProfileReqR99 = SECONDARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0


QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY1,0x04, 0x04, 0x04, 0x01, 0x08, 0x08, -1, -1, -1, -1,0,0, 0x20, 1, 0x10 ,1 ,2 ,1 ,1 ,250 ,-1 ,-1 ,0 ,0 ,1 ,1
#Added for test case 29
QosProfileReqR5 = SECONDARY1,0x04, 0x04, 0x04, 0x01, 0x08, 0x08, -1, -1, -1, -1,0,0, 0x20, 1, 0x10 ,1 ,2 ,1 ,1 ,250 ,-1 ,-1 ,0 ,0 ,0 ,0
#Added for test case 30
QosProfileReqR5 = SECONDARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0


#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 

QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3


QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 1, 1
#for test case 29
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
#for test case 30
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0


#TQosProfileCapsR99 = <trafficCap> <deliveryOrderReqCap> <deliverErroneousSDUCap>
#		      <BERCap> <SDUErrorRatioCap> <trafficHandlingPriorityCap>
QosProfileCapsR99= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04

QosNetworkNotificationType = PublishSubscribe
# QosNetworkNotification = <contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> <negMaxSDUSize>
QosNetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosR5NetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 1
QosR5NetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 1


#SetProfileFail= <contextName> <numberOfTimes> <errorCode> <setProfileDigit>
SetProfileFail = NEG_99, 0x04, 0x02

#QosprofileReqGPRS= <minPrecedence> <reqPrecedence> <minDelay> <reqDelay> <minReliability> <reqReliability> <minPeek> <reqPeek>
#		    <minMean> <reqMean>
QosProfileReqGPRS= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020
QosProfileReqGPRS= 0x04, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020

#QosProfileNegGPRS=<negPrecedence> <negDelay><negReliability> <negPeek> <negMean>
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002

#QosProfileCapsGPRS=<negPrecedenceCap> <negDelayCap> <negReliabilityCap><negPeekCap> <negMeanCap>
QosProfileCapsGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002 

# QosProfileReq
# = <TTrafficClass>, <TTrafficClass>, <TDeliveryOrder>, <TDeliveryOrder>
# <TErroneousSDUDelivery>, <TErroneousSDUDelivery>
# <TErroneousSDUDelivery>, <TInt iReqMaxSDUSize>, <TInt iMinAcceptableMaxSDUSize>
# <TBitRate>, <TBitRate>, <TBitErrorRatio>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>, <TTrafficHandlingPriority>
# <TInt	iReqTransferDelay>, <TInt iMaxTransferDelay>, <TBitRate>, <TBitRate>

# QosProfileNeg = <TQoSPrecedence>, <TQoSDelay>, <TQoSReliability>, <TQoSPeakThroughput>, <TQoSMeanThroughput>
# <TTrafficClass>, <TDeliveryOrder>, <TErroneousSDUDelivery>, <TInt iMaxSDUSize>, <TBitRate>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>
# <TInt iTransferDelay>, <TBitRate>		

DefaultContextparamRel99= 3, ACME INTERNET PROVIDERS LTD, i-MODE GATEWAY, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2
# DefaultContextparamRel99 = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>

ReleaseMode = 5, 5
# Packet Release mode = <Release> <Duration>

#RegStatus=<duration> <regStat> <networkIndex> 
RegStatus= 5,3
RegStatus= 2,5,0
RegStatus= 2,7,3
RegStatus= 5,2
RegStatus= 2,5,0

# NetworkRegStatus = <Duration>, <RegistrationStatus>
NetworkRegStatusType = PublishSubscribe
NetworkRegStatus= 5,2
NetworkRegStatus= 5,1
NetworkRegStatus= 5,1

# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= PKTLOOPBACK.CSY, PKTLOOPBACK::502, 18, 0, PRIMARY1
CommSetup= PKTLOOPBACK.CSY, PKTLOOPBACK::504, 18, 0, SECONDARY1


############################################################################
# failure events
# Configure the context's status to be changed using publish and subscribe
NotifyContextStatusChangeType = PublishSubscribe
# NotifyContextStatusChange <iContextName>, <iDuration>, <iStatus>

# EStatusDeactivating = 4 EStatusInactive = 1 EStatusDeleted = 6
NotifyContextStatusChange = PRIMARY1, 0, 6
NotifyContextStatusChange = PRIMARY1, 0, 4
NotifyContextStatusChange = PRIMARY1, 0, 1
NotifyContextStatusChange = SECONDARY1, 0, 6
NotifyContextStatusChange = SECONDARY1, 0, 4
NotifyContextStatusChange = SECONDARY1, 0, 1

# EStatusSuspended = 5 EStatusActive = 3
NotifyContextStatusChange = PRIMARY1, 0, 5
NotifyContextStatusChange = PRIMARY1, 0, 3
NotifyContextStatusChange = SECONDARY1, 0, 5
NotifyContextStatusChange = SECONDARY1, 0, 3

############################################################################
############################################################################
###################              T E S T 1 0 1           ####################
############################################################################
############################################################################
# QosProfileReqR99 for SECONDARY1 reqTraffic and minTraffic values are 
# modified so that secondary PDP context creation fails due to Requested QoS
# parameter mismatch.
############################################################################
[test101]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,, 0, 2, 0, 0,RasUser,,,,,,0

#SetContextConfigR5= <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <TUseEdge>, <Authentication Protocol>, <Username>, <Password>, <Challenge>,
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>, <THeaderCompression>, <TDataCompression>, <No. Additional Context Config Params>
SetContextConfigR5= 0, SYMBIAN INTERNET PROVIDER, PROTOCOL ADDRESS, 0, 2, USER3, PASSWORD3, CHALLENGE3, RESPONSE3, PRIMARYSERVER3, SECONDARYSERVER3, 3, 2, 1, 1

#AdditionalParamItem= <TPcoProtocolId>, <TBuf8 AdditionalParamData>
AdditionalParamItem= 0x04, ADDITIONALPARAM1



# TRel99ContextConfig = 0<TName iContextName>,  1<TUint iActivatePause>, 2<TUint iActivateErrorCode>, 3<TUint iDeactivatePause>, 
# 4<TUint iDeactivateErrorCode>, 5<TUint iDeletionPause>, 6<TUint iDeletionErrorCode> 7<TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, 0, 0, 0, 0, 0, 0
R99ContextConfig = SECONDARY1, 0, 0, 0, 0, 0, 0, 0

# TFTfilter = 0<id> 1<evaluationPrecedenceIndex> 2<srcAddr> 3<srcAddrSubnetMask>  4<protocolNumberOrNextHeader>
#	      5<srcPortMin> 6<srcPortMax> 7<destPortMin> 8<destPortMax> 9<ipSecSPI> 10<toSorTrafficClass>
#	      11<flowLabel>
TFTfilter = 1, 0, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0

#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>
QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0
QosProfileReqR99 = SECONDARY1,0x08, 0x08, 0x02, 0x02, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x08, 0x08, 250, 250, -1, -1, 0, 0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY1,0x08, 0x08, 0x02, 0x02, 0x08, 0x08, -1, -1, -1, -1, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x08, 0x08, 250, 250, -1, -1, 0, 0, 0, 0


#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 
QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3

QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 0, 0


#TQosProfileCapsR99 = <trafficCap> <deliveryOrderReqCap> <deliverErroneousSDUCap>
#		      <BERCap> <SDUErrorRatioCap> <trafficHandlingPriorityCap>
QosProfileCapsR99= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04

QosNetworkNotificationType = PublishSubscribe
# QosNetworkNotification = <contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> <negMaxSDUSize>
QosNetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosR5NetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0

#SetProfileFail= <contextName> <numberOfTimes> <errorCode> <setProfileDigit>
SetProfileFail = NEG_99, 0x04, 0x02

#QosprofileReqGPRS= <minPrecedence> <reqPrecedence> <minDelay> <reqDelay> <minReliability> <reqReliability> <minPeek> <reqPeek>
#		    <minMean> <reqMean>
QosProfileReqGPRS= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020
QosProfileReqGPRS= 0x04, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020

#QosProfileNegGPRS=<negPrecedence> <negDelay><negReliability> <negPeek> <negMean>
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002

#QosProfileCapsGPRS=<negPrecedenceCap> <negDelayCap> <negReliabilityCap><negPeekCap> <negMeanCap>
QosProfileCapsGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002 

# QosProfileReq
# = <TTrafficClass>, <TTrafficClass>, <TDeliveryOrder>, <TDeliveryOrder>
# <TErroneousSDUDelivery>, <TErroneousSDUDelivery>
# <TErroneousSDUDelivery>, <TInt iReqMaxSDUSize>, <TInt iMinAcceptableMaxSDUSize>
# <TBitRate>, <TBitRate>, <TBitErrorRatio>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>, <TTrafficHandlingPriority>
# <TInt	iReqTransferDelay>, <TInt iMaxTransferDelay>, <TBitRate>, <TBitRate>

# QosProfileNeg = <TQoSPrecedence>, <TQoSDelay>, <TQoSReliability>, <TQoSPeakThroughput>, <TQoSMeanThroughput>
# <TTrafficClass>, <TDeliveryOrder>, <TErroneousSDUDelivery>, <TInt iMaxSDUSize>, <TBitRate>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>
# <TInt iTransferDelay>, <TBitRate>		

DefaultContextparamRel99= 3, ACME INTERNET PROVIDERS LTD, i-MODE GATEWAY, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2
# DefaultContextparamRel99 = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>

ReleaseMode = 5, 5
# Packet Release mode = <Release> <Duration>

#RegStatus=<duration> <regStat> <networkIndex> 
RegStatus= 5,3
RegStatus= 2,5,0
RegStatus= 2,7,3
RegStatus= 5,2
RegStatus= 2,5,0

# NetworkRegStatus = <Duration>, <RegistrationStatus>
NetworkRegStatusType = PublishSubscribe
NetworkRegStatus= 5,2
NetworkRegStatus= 5,1
NetworkRegStatus= 5,1

# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= PKTLOOPBACK, PKTLOOPBACK::502, 18, 0, PRIMARY1
CommSetup= PKTLOOPBACK.CSY, PKTLOOPBACK::504, 18, 0, SECONDARY1

############################################################################
############################################################################
###################              T E S T 102              ####################
############################################################################
############################################################################
# Test case for success results
############################################################################
[test102]
# DefaultContextparamGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
DefaultContextparamGPRS= 3, SYMBIAN EMPLOYEE INTRANET, A WAP PORTAL, 2, 1, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2

# ContextConfigGPRS = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <PdpDataCompression>, <TAnonymousAccess>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>
SetContextConfigGPRS= 0,Test,,0, 2, 0, 0,RasUser,,,,,,0

#SetContextConfigR5= <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <TUseEdge>, <Authentication Protocol>, <Username>, <Password>, <Challenge>,
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>, <THeaderCompression>, <TDataCompression>, <No. Additional Context Config Params>
SetContextConfigR5= 0, SYMBIAN INTERNET PROVIDER, PROTOCOL ADDRESS, 0, 2, USER3, PASSWORD3, CHALLENGE3, RESPONSE3, PRIMARYSERVER3, SECONDARYSERVER3, 3, 2, 1, 1

#AdditionalParamItem= <TPcoProtocolId>, <TBuf8 AdditionalParamData>
AdditionalParamItem= 0x04, ADDITIONALPARAM1

# TRel99ContextConfig = <TName iContextName>,  <TUint iActivatePause>, <TUint iActivateErrorCode>, <TUint iDeactivatePause>, 
# <TUint iDeactivateErrorCode>, <TUint iDeletionPause>, <TUint iDeletionErrorCode> <TBool iConnectToNtRas>
R99ContextConfig = PRIMARY1, 0, 0, 0, 0, 0, 0, 0
R99ContextConfig = SECONDARY1, 0, 0, 0, 0, 0, 0, 0


# TFTfilter = 0<id> 1<evaluationPrecedenceIndex> 2<srcAddr> 3<srcAddrSubnetMask>  4<protocolNumberOrNextHeader>
#	      5<srcPortMin> 6<srcPortMax> 7<destPortMin> 8<destPortMax> 9<ipSecSPI> 10<toSorTrafficClass>
#	      11<flowLabel>
TFTfilter = 1, 96, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0
TFTfilter = 1, 0, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0
TFTfilter = 1, 1, 0.0.0.0.0.0.0.0.0.0.255.255.192.168.1.1, 255.255.255.255.255.255.255.255.255.255.255.255.255.255.255.255, 17, 3461, 3461, 1031, 1031, 0, 0, 0

#TProfileReqR99 = 0<contextName> 1<reqTraffic> 2<minTraffic> 3<reqDeliveryOrder> 4<minDeliveryOrder>
#		  5<reqErroneousSDU> 6<minErroneousSDU> 7<maxSDUSize> 8<minSDUSize>
#		 9<reqUpLinkBitRate> 10<reqDownLinkBitRate> 11<minUpLinkBitRate> 12<minDownLinkBitRate> 
#		 
#		 13<reqBitErrorRatio> 14<minBitErrorRatio> 15<reqSDUErrorRatio> 16<minSDUErrorRatio>
#		 17<reqTrafficHandlingPriority> 18<minTrafficHandlingPriority>
#		 19<reqTransferDelay> 20<minTransferDelay> 21<reqGuaranteedUpLinkBitRate> 22<reqGuaranteedDownLinkBitRate>
#		 23<minGuaranteedUpLinkBitRate> 24<minGuaranteedDownLinkBitRate>

QosProfileReqR99 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0

QosProfileReqR99 = SECONDARY1,0x04, 0x04, 0x04, 0x01, 0x08, 0x08, -1, -1, -1, -1,0,0, 0x20, 1, 0x10 ,1 ,2 ,1 ,1 ,250 ,-1 ,-1 ,0 ,0

QosProfileReqR5 = PRIMARY1,0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0x01, 0x01, 0x01, 0x01, 0x01, 0x01, 0, 0, 0, 0, 0, 0, 0, 0
QosProfileReqR5 = SECONDARY1,0x04, 0x04, 0x04, 0x01, 0x08, 0x08, -1, -1, -1, -1,0,0, 0x20, 1, 0x10 ,1 ,2 ,1 ,1 ,250 ,-1 ,-1 ,0 ,0 ,1 ,1


#TProfileNegR99 =<contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery> <negMaxSDUSize>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> 

QosProfileNegR99 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3
QosProfileNegR99 = SECONDARY1, 0x03, 0x01, 0x01, 0x01, 1501, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3

QosProfileNegR5 = PRIMARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 1, 1
QosProfileNegR5 = SECONDARY1, 0x03, 0x01, 0x03, 0x01, 1, 0x03, 0x01, 0x03, 1, 1, 3, 1, 3, 1, 1


#TQosProfileCapsR99 = <trafficCap> <deliveryOrderReqCap> <deliverErroneousSDUCap>
#		      <BERCap> <SDUErrorRatioCap> <trafficHandlingPriorityCap>
QosProfileCapsR99= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04

QosNetworkNotificationType = PublishSubscribe
# QosNetworkNotification = <contextName> <duration> <negTraffic> <negDeliveryOrder> <negErroneousSDUDelivery>
#		 <negBitErrorRatio> <negSDUErrorRatio> <negTrafficHandlingPriority>
#		 <negTransferDelay> <negGuaranteedUpLinkBitRate> <negGuaranteedDownLinkBitRate>
#		 <negMaxUpLinkRate> <negMaxDownLinkRate> <negMaxSDUSize>
QosNetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4
QosNetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4

QosR5NetworkNotification = PRIMARY1, 0x04, 0x02, 0x04, 0x02, 2, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 0, 0
QosR5NetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 1, 0
QosR5NetworkNotification = SECONDARY1, 0x04, 0x02, 0x04, 0x02, 1, 0x04, 0x02, 0x04, 2, 2, 4, 2, 4, 1, 0


#SetProfileFail= <contextName> <numberOfTimes> <errorCode> <setProfileDigit>
SetProfileFail = NEG_99, 0x04, 0x02

#QosprofileReqGPRS= <minPrecedence> <reqPrecedence> <minDelay> <reqDelay> <minReliability> <reqReliability> <minPeek> <reqPeek>
#		    <minMean> <reqMean>
QosProfileReqGPRS= 0x08, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020
QosProfileReqGPRS= 0x04, 0x04, 0x02, 0x04, 0x02, 0x04, 0x020, 0x080, 0x00004, 0x00020

#QosProfileNegGPRS=<negPrecedence> <negDelay><negReliability> <negPeek> <negMean>
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002
QosProfileNegGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002

#QosProfileCapsGPRS=<negPrecedenceCap> <negDelayCap> <negReliabilityCap><negPeekCap> <negMeanCap>
QosProfileCapsGPRS= 0x04, 0x04, 0x04, 0x080, 0x00002 

# QosProfileReq
# = <TTrafficClass>, <TTrafficClass>, <TDeliveryOrder>, <TDeliveryOrder>
# <TErroneousSDUDelivery>, <TErroneousSDUDelivery>
# <TErroneousSDUDelivery>, <TInt iReqMaxSDUSize>, <TInt iMinAcceptableMaxSDUSize>
# <TBitRate>, <TBitRate>, <TBitErrorRatio>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>, <TTrafficHandlingPriority>
# <TInt	iReqTransferDelay>, <TInt iMaxTransferDelay>, <TBitRate>, <TBitRate>

# QosProfileNeg = <TQoSPrecedence>, <TQoSDelay>, <TQoSReliability>, <TQoSPeakThroughput>, <TQoSMeanThroughput>
# <TTrafficClass>, <TDeliveryOrder>, <TErroneousSDUDelivery>, <TInt iMaxSDUSize>, <TBitRate>, 
# <TBitErrorRatio>, <TSDUErrorRatio>, <TTrafficHandlingPriority>
# <TInt iTransferDelay>, <TBitRate>		

DefaultContextparamRel99= 3, ACME INTERNET PROVIDERS LTD, i-MODE GATEWAY, 1, 1, USER2, PASSWORD2, NULL, NULL, PRIMARYSERVER2, SECONDARYSERVER2, 2
# DefaultContextparamRel99 = <TProtocolType>, <TGSNAddress>, <TProtocolAddress>, <TUseEdge>
# ProtocolConfigOption = <Authentication Protocol>, <Username>, <Password>, <Challenge>, 
# <Response>, <PrimaryDNS>, <SecondaryDNS>, <TUint iId>

ReleaseMode = 5, 5
# Packet Release mode = <Release> <Duration>

#RegStatus=<duration> <regStat> <networkIndex> 
RegStatus= 5,3
RegStatus= 2,5,0
RegStatus= 2,7,3
RegStatus= 5,2
RegStatus= 2,5,0

# NetworkRegStatus = <Duration>, <RegistrationStatus>
NetworkRegStatusType = PublishSubscribe
NetworkRegStatus= 5,2
NetworkRegStatus= 5,1
NetworkRegStatus= 5,1

# CommSetup = <CsyName> <portName> <datarate> <handshake> <contextName> 
CommSetup= PKTLOOPBACK.CSY, PKTLOOPBACK::502, 18, 0, PRIMARY1
CommSetup= PKTLOOPBACK.CSY, PKTLOOPBACK::504, 18, 0, SECONDARY1


############################################################################
# failure events
# Configure the context's status to be changed using publish and subscribe
NotifyContextStatusChangeType = PublishSubscribe
# NotifyContextStatusChange <iContextName>, <iDuration>, <iStatus>

# EStatusDeactivating = 4 EStatusInactive = 1 EStatusDeleted = 6
NotifyContextStatusChange = PRIMARY1, 0, 6
NotifyContextStatusChange = PRIMARY1, 0, 4
NotifyContextStatusChange = PRIMARY1, 0, 1
NotifyContextStatusChange = SECONDARY1, 0, 6
NotifyContextStatusChange = SECONDARY1, 0, 4
NotifyContextStatusChange = SECONDARY1, 0, 1

# EStatusSuspended = 5 EStatusActive = 3
NotifyContextStatusChange = PRIMARY1, 0, 5
NotifyContextStatusChange = PRIMARY1, 0, 3
NotifyContextStatusChange = SECONDARY1, 0, 5
NotifyContextStatusChange = SECONDARY1, 0, 3

