// Copyright (c) 1995-2009 Nokia Corporation and/or its subsidiary(-ies).
// All rights reserved.
// This component and the accompanying materials are made available
// under the terms of the License "Eclipse Public License v1.0"
// which accompanies this distribution, and is available
// at the URL "http://www.eclipse.org/legal/epl-v10.html".
//
// Initial Contributors:
// Nokia Corporation - initial contribution.
//
// Contributors:
//
// Description:
// e32\euser\epoc\arm\uc_exe.cia
// 
//

#include <e32cia.h>
#include <u32std.h>
// Include this to get imports from User (i.e. User::Invariant and User::HandleException). 
// This sets VISIBILITY to DEFAULT for BPABI builds.
#include <e32std.h>

extern "C" {

void _xxxx_call_user_invariant();
void _xxxx_call_user_handle_exception(void *);

extern void RunThread(TBool aNotFirst, SThreadCreateInfo& aInfo);

// NOTE: This MUST be the first function in this module
__NAKED__ TInt _E32Startup()
	{
	// Process entry point
	// R4 = entry reason
	// SP points to information block
	EKA2_ENTRY_POINT_VERSION_IDENTIFIER;	// DUMMY INSTRUCTION TO INDICATE EKA2 ENTRY POINT
	asm("cmp r4, #%a0" : : "i" ((TInt)KModuleEntryReasonThreadInit) );
	asm("b 1f ");				// branch over space for unique ID

	asm(".word 0 ");			// loader will replace with code seg unique ID
								// for RAM-loaded code segment
								// MUST BE AT OFFSET 12 FROM ENTRY POINT

	asm("1: ");
	asm("movls r0, r4 ");		// r0 = aNotFirst
	asm("movls r1, sp ");		// r1 -> parameter block
	asm("bls RunThread ");		// process or thread init
	asm("cmp r4, #%a0" : : "i" ((TInt)KModuleEntryReasonException) );
//  	asm("bne " CSM_ZN4User9InvariantEv );	// invalid entry reason
  	asm("bne _xxxx_call_user_invariant " );	// invalid entry reason

	// exception entry
	// NOTE: THUMB only works on ARMv5 and above
	asm("mov r0, sp ");			// r0->parameter block
	asm("ldr r4, [sp, #16]");	// r4 = saved CPSR
	asm("tst r4, #0x20 ");		// test for THUMB
	asm("ldrne r1, [sp, #80] ");	// r1 = saved return addr
	asm("orrne r1, r1, #1 ");
	asm("strne r1, [sp, #80] ");	// if THUMB, set bit 0 of return addr

	asm("mov r11, sp ");		// save stack pointer

	// The frame starts 84 bytes (up) from r11 i.e. CFA is r11 + 84
	__EH_FRAME_ADDRESS(sp, 84) // Reg needs to be sp (=r11) here for gcce
	// we can only restore callee-save values, but that's what we want if we 'leave'
	// saved link is -8 bytes from CFA (= r11 + 0x24 + 0x20 + 0x8)
	__EH_FRAME_SAVE1(lr, -8)

	// the other callee saves start at -48 from CFA (= r11 + 0x24)
#if 0
	// would like to say this 
	__EH_FRAME_SAVE1(r4-r11, -48)
	// but the macro expansion gives rise to odd code so we do what follows
#endif
#if defined(__ARMCC__)
	FRAME SAVE {r4-r11}, -48
#elif defined(__GCCE__)
	__EH_FRAME_SAVE1(r4-r11,-48)
#else
#error What compiler?	
#endif


	asm("bic sp, sp, #4 ");		// align stack to 8 byte boundary
//  	asm("bl " CSM_ZN4User15HandleExceptionEPv );
  	asm("bl _xxxx_call_user_handle_exception ");
	asm("add sp, r11, #16 ");	// skip exc type, exc code, FAR, FSR
	asm("ldr r4, [sp], #4 ");	// r4 = saved CPSR
	asm("bic r4, r4, #0x20 ");	// clear THUMB bit
	asm("msr cpsr, r4 ");		// restore flags
	asm("ldmia sp, {r0-r15} ");	// restore r0-r15

#ifdef __ARMCC__
#ifdef __SUPPORT_CPP_EXCEPTIONS__


  /* It is possible no functions included in the image require
   * a handler table. Therefore make only a weak reference to
   * the handler table base symbol, which may be absent.
   */
  extern |.ARM.exidx$$Base|;
  extern |.ARM.exidx$$Limit|;
  extern |.ARM.extab$$Base| [WEAK];
  extern |Image$$ER_RO$$Base|;
  extern |Image$$ER_RO$$Limit|;
  export |Symbian$$CPP$$Exception$$Descriptor|;

|Symbian$$CPP$$Exception$$Descriptor|
#ifdef __LEAVE_EQUALS_THROW__
|Symbian$$eit_base|  		dcd |.ARM.exidx$$Base|;   /* index table base */
|Symbian$$eit_limit|  		dcd |.ARM.exidx$$Limit| ;  /* index table limit */
#endif
#if __ARMCC_VERSION > 220000
|Symbian$$code_seg_base| 	dcd |Image$$ER_RO$$Base| + 1 ; /* RO segment base + mark as ehabi v2 */
|Symbian$$code_seg_limit| 	dcd |Image$$ER_RO$$Limit| ;/* RO segment limit */
|Symbian$$reserved|		dcd 0 ; /* reserved for future use */
#else
|Symbian$$code_seg_base| 	dcd |Image$$ER_RO$$Base| ; /* RO segment base */
|Symbian$$code_seg_limit| 	dcd |Image$$ER_RO$$Limit| ;/* RO segment limit */
#endif

#endif
#endif

	}
void _xxxx_call_user_invariant() { User::Invariant(); }
void _xxxx_call_user_handle_exception(void * arg) { User::HandleException(arg); }

}

