/*
* Copyright (c) 2009 Nokia Corporation and/or its subsidiary(-ies).
* All rights reserved.
* This component and the accompanying materials are made available
* under the terms of the License "Eclipse Public License v1.0"
* which accompanies this distribution, and is available
* at the URL "http://www.eclipse.org/legal/epl-v10.html".
*
* Initial Contributors:
* Nokia Corporation - initial contribution.
*
* Contributors:
*
* Description:
*
*/


REM should be able to just reference the "core" os image by using
REM 
coreimage = dir.rofs

extensionrofs = extension.rofs

rofssize = 0x80000
time = 14/06/2005 20:12:20

REM Round the size up/down to the nearest block size
REM This will enable any ROFS extensions to be found
REM BlockSize is typically 16K for most small-block NAND chips
REM BlockSize is typically 128K for most large-block NAND chips
REM autosize = 0x4000
REM autosize = 0x20000

REM create new files
data=EPOCROOT##epoc32\rom\rofstest\hello8.txt		ext.txt
data=EPOCROOT##epoc32\rom\rofstest\hello8.txt		Dir1\ext.txt

REM hide existing file
rem data=EPOCROOT##epoc32\rom\rofstest\hello8.txt		root.txt
hide= root.txt

REM rename existing file
rem data=EPOCROOT##epoc32\rom\rofstest\hello8.txt		Dir1\level1.txt
rename= Dir1\level1.txt Dir1\level1_ext.txt

#ifndef EXCLUDE_TESTS

REM demand paging stress tests
#include "t_pagestress_ext.iby"

#endif // #ifndef EXCLUDE_TESTS
