: public note

Created: | 1/7/2008 2:59:00 PM
Modified: | 1/7/2008 3:02:07 PM
Project: |
Author: | Symbian
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Advanced: |
UUID: | {F0C40F2E-AF1F-4bcb-B9D6-0F3B01B54D03}
Appears In: | SUPL-MOLR-TA-Standard

<p>Because the positioning mode requested by LBS may be different from the one requested by the network, before sending SUPL_POS_INIT, the SUPL Client must determine what assistance data is required.<br/></p><p>The assistance data set required by an AGPS Module may be different for TB and TA positionings.<br/></p><p><br/></p><p>The SUPL Client must check<br/></p><p> a) the network preferences (from SUPL_RESPONSE message), and<br/></p><p> b) the LBS (AGPS Module) capabilities (by calling GetCapbilities() )<br/></p><p>select an appropriate positioning method and inject location request into LBS.<br/></p>