: public note

Created: | 2/14/2007 3:12:58 PM
Modified: | 2/14/2007 4:44:40 PM
Project: |
Author: |
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Advanced: |
UUID: | {338950CB-0A28-47be-8853-C1A35FED96B5}
Appears In: | RRC-X3P-Hybrid UE Assisted - Client Time Out

<p>***LBS INTERNAL CHANGE***<br/></p><p>NRH does not immediately complete clients request when its X3P Timer Expires.<br/></p><p>It now waits until the session complete message is recieved and returns the final NW pos (if any) and session complete status<br/></p>