: public note

Created: | 1/4/2008 12:21:15 PM
Modified: | 1/7/2008 10:27:43 AM
Project: |
Author: | Symbian
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Advanced: |
UUID: | {FFB9D01A-C133-4171-9C16-6158C12DD7A6}
Appears In: | SUPL-MTLR-Standard

<p>Before sending SUPL_POS_INIT, the SUPL Client must determine what assistance data is required.<br/></p><p>The assistance data set required by an AGPS Module may be different for TB and TA positionings.<br/></p><p><br/></p><p>The SUPL Client must check<br/></p><p> a) the network preferences (from SUPL_INIT message), and<br/></p><p> b) the LBS (AGPS Module) capabilities (by calling GetCapbilities() )<br/></p><p>select an appropriate positioning method and inject location request into LBS.<br/></p>