: public note

Created: | 3/6/2008 1:28:57 PM
Modified: | 4/11/2008 4:13:47 PM
Project: |
Author: | Symbian
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Advanced: |
UUID: | {F140C53E-0DFA-4d2c-BFC6-E2CC3096C681}
Appears In: | Common - Self Location Request - AGPS - First

<p>Note that the network status is only checked when LBS requests a Protocol Module to start a MOLR. The LBS subsystem would not attempt to stop positioning if network coverage was lost (either temporally or permanently) during an ongoing MOLR session.<br/></p><p>In such a case the following scenarios are possible:<br/></p><p> - the AGPS Module generates an accurate or inaccurate location update despite the lack<br/></p><p> of assistance data (Autonomous or Prefer Terminal Based modes)<br/></p><p> - the request times out (Always Terminal Assisted or Prefer Terminal Assisted modes)<br/></p><p> - the Protocol Module decides to terminate the MOLR and the AGPS Module calculates position<br/></p><p> autonomously (Prefer Terminal Assisted mode only)<br/></p>