: public note

Created: | 10/23/2008 1:11:32 PM
Modified: | 10/23/2008 1:14:22 PM
Project: |
Author: | Symbian
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Advanced: |
UUID: | {9A23E45C-6FF6-4ca7-964B-7FB95976BBB5}
Appears In: | Common - Self Location Request - AGPS - Subsequent

<p>The SelfLocationRequest is also sent if the technology type specified in the Location Request from LSF is different from the one used by the currently active MOLR.<br/></p><p><br/></p><p>For simplicity this scenario is not presented in details.<br/></p>