: public note

Created: | 1/14/2008 10:39:58 AM
Modified: | 1/14/2008 10:41:48 AM
Project: |
Author: | Symbian
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Advanced: |
UUID: | {E73D2993-3981-460a-ABA9-325781BA15C0}
Appears In: | Common - Network Measurement Response - AGPS

<p>In both, Timeout and Update cases NRH waits for MFT to expire.<br/></p><p>The difference is that in the Update case the NRH has received at least one Measurement Update before the timeout.<br/></p>