: public note

Created: | 3/28/2007 3:11:48 PM
Modified: | 3/28/2007 3:11:52 PM
Project: |
Author: |
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Advanced: |
UUID: | {2B27772C-B280-4aa5-8225-669E467C72A0}
Appears In: | RRC-X3P-Hybrid - UE Assisted - Late GPS Result

<p>GPS Position does not contain lat or long of current accuracy. Therefore the measurement results are sent to protocol module when timer expires<br/></p>