: public note

Created: | 1/4/2008 3:13:35 PM
Modified: | 3/5/2008 6:43:46 PM
Project: |
Author: | Symbian
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Advanced: |
UUID: | {ADAB71AC-83DF-47ed-A9DA-5BCC1F35DADA}
Appears In: | Common - Self Location Request - AGPS - Subsequent

<p>Normally, by the time of the Subsequent Self Location Request the AGPS Module should have already received all the Assistance Data, so is sets the aDataRequestMask in the new request to 0 to specify that it does NOT need any more assistance data.<br/></p>