cenrep
version 1

[PlatSec]
# Any client can read values. 
# Test Protocol Module can write values - not anticipated at present.
# (271064431 = 10281d6f hex)
cap_rd = AlwaysPass sid_wr = 271064431

[main]
# Entry format is as follows:
# <ID> <type> <conflict decision value> <meta data>

# Conflict decision Values
#   0 = Reject new
#   1 = Queue new
#   2 = Cancel current
#   3 = Queue current

# --------------------------
# MO-LR is current operation
# --------------------------
# MO-LR
  1 int 2 0
# MT-LR
  2 int 0 0
# Emergency MT-LR
  3 int 2 0
# Low priority X3P
  4 int 1 0
# Mid priority X3P
  5 int 0 0
# High priority X3P
  6 int 2 0

# --------------------------
# MT-LR is current operation
# --------------------------
# MO-LR
  7 int 1 0
# MT-LR
  8 int 0 0
# Emergency MT-LR
  9 int 2 0
# Low priority X3P
  10 int 1 0
# Mid priority X3P
  11 int 0 0
# High priority X3P
  12 int 2 0

# ------------------------------
# Emergency is current operation
# ------------------------------
# MO-LR
  13 int 0 0
# MT-LR
  14 int 0 0
# Emergency MT-LR
  15 int 0 0
# Low priority X3P
  16 int 0 0
# Mid priority X3P
  17 int 0 0
# High priority X3P
  18 int 0 0


# ------------------------------
# Low X3P is current operation
# ------------------------------
# MO-LR
  19 int 0 0
# MT-LR
  20 int 0 0
# Emergency MT-LR
  21 int 2 0
# Low priority X3P
  22 int 1 0
# Mid priority X3P
  23 int 0 0
# High priority X3P
  24 int 3 0


# ------------------------------
# Medium X3P is current operation
# ------------------------------
# MO-LR
  25 int 0 0
# MT-LR
  26 int 0 0
# Emergency MT-LR
  27 int 2 0
# Low priority X3P
  28 int 1 0
# Mid priority X3P
  29 int 0 0
# High priority X3P
  30 int 2 0

# ------------------------------
# High X3P is current operation
# ------------------------------
# MO-LR
  31 int 0 0
# MT-LR
  32 int 0 0
# Emergency MT-LR
  33 int 2 0
# Low priority X3P
  34 int 1 0
# Mid priority X3P
  35 int 0 0
# High priority X3P
  36 int 0 0

