Copyright (C) 1999-2007 Nokia. All Rights Reserved.
Version: 1.0
Parser
Introduction
Introduction
Introduction, intro, overview
	IPROTOR is an application to dump incoming IP traffic in a EPOC machine.
archive=iprotor name=screen
	It also have a graphic Rotor that increases its speed when receiving packets and decreases when not.
Tools
Tools
Start, begin, Stop, end
•	Start: Starts the rotor using the current configuration
•	Stop: Stops the rotor.
View
View
Monitoring, view , options, scan, mode, blades, IP header, type
•	IPv4 Monitoring: Dialog that controls the monitoring for all the fields of the diferent types of IPv4 packets (IP, ICMP, TCP, UDP, AH, ESP)
•	IPv6 Monitoring: Dialog that controls the monitoring for all the fields of the diferent types of IPv6 packets (IP, ICMP, TCP, UDP)
•	Options: Other options to configure the application:
•	Scanning mode: IP version to scan. IPv4 or IPv6.
•	Header Type: Type of packet to dump. IP indicates All packets, while the rest are for specific types.
•	Port: Dumps only packets directed to a specific port (only available for IP, TCP, UDP)
•	View IP header: To choose if want to dump the IP header of the packets when monitoring or only other headers.
•	Rotor Blades: Number of blades in the Rotor.
Console
Console
Console, Clear, Screen, font, history, full, scrollbar
To configure console related options.
•	Clear Screen: Clears the contents of the console.
•	Set font: To configure console font type, size and characteristics.
•	History size: The amount of lines stored in the console. Default is 100 lines.          
?	A big history size may require a big amount of memory.
•	Full screen: The app only shows the console and hides the rest of controls to have a maximum size console.
•	Scrollbars: To put scrollbars on the console.