# Copyright (c) 2008-2009 Nokia Corporation and/or its subsidiary(-ies).
# All rights reserved.
# This component and the accompanying materials are made available
# under the terms of "Eclipse Public License v1.0"
# which accompanies this distribution, and is available
# at the URL "http://www.eclipse.org/legal/epl-v10.html".
#
# Initial Contributors:
# Nokia Corporation - initial contribution.
#
# Contributors:
#
# Description:
#
#
#
# 10285c46.txt
#
# Reference mount manager policy definitions
#

cenrep
version 1

[PlatSec]
# Only a client with DiskAdmin,NetworkControl,ProtServ and WriteDeviceData
# capabilities can read and write keys.
cap_rd=DiskAdmin,ProtServ,NetworkControl,WriteDeviceData
cap_wr=DiskAdmin,ProtServ,NetworkControl,WriteDeviceData

[Main]

# A range of drive letters available to be used for Mass Storage drives.
# The first and last available letter shall be stored.
0x00010000 string8 "DX" 0

# A list of drive letters forbidden by licensee.
0x00010001 string8 "E" 0

# Max mounting history record amount. Currently the reference policy 
# plugin set it to 5.
0x00010002 int	5 0

# OTG capable suspend time. Currently the reference policy 
# plugin set it to 5 seconds.
0x00010003 int 5 0

# Media polling time. Currently the reference policy 
# plugin set it to 1 seconds.
0x00010004 int 1 0

# The count of mounting history record
0x00010100 int	0 0

# The mounting history records.
# This is the first record.
# New record will be appended behind this using UID grown by 1.
# For instance, the second record will go with UID 0x00010102.
0x00010101 string8 "" 0
