## System TRK Launch Configuration (Stop-mode)

Select the Symbian OS System TRK launch configuration provides C/C++ stop-mode debug options that use a JTAG interface when a Symbian OS launch configuration is created. The settings included in these launch configuration are a combination of Carbide, CDT, and Eclipse options.

If the New Launch Configuration Wizard was used to create the System TRK launch configuration no changes are usually needed. To modify the launch configuration settings, select the Run > Debug As menu option to open the Debug dialog. Select the System TRK configuration and click a tab to set specific options. Click Apply to save any option modifications. Click Debug to launch a debugging session using the new settings.

Figure 1. System TRK launch configuration in the Debug dialog

The System TRK launch configuration panes include:

- The Main tab defines the project to be launched. Enter the name of the project in the Project field, and the executable name in the Executable field.
- The Debugger tab defines debug configurations, such as entry point to begin debugging and target options.
- The ROM Image tab allows you to define startup options and ROM image download information.
- The Executables tab allows you to specify which executables that you want to debug that are part of the project.
- The Source tab (standard CDT page) defines the location of source files used to display source when debugging an application. By default, these settings are derived from the associated project's build path. You may override these settings here.
- The Common tab (standard CDT page) defines general information about the launch configuration. You may choose to store the launch configuration in a specific file.

#### Other references

- Launch Configuration Overview