## Crash Debugger Commands

Commands consist of a single letter describing the operation to be performed, followed by any arguments. Not all commands take arguments. Commands are case sensitive; the majority are lower case. Commands should be entered at the command prompt, on the PC. The set of supported commands is as follows:

- h - show all debugger commands
- x - leaves the debugger, does a cold restart of the same ROM image; (nb lower case)

- X - leaves the debugger, and returns to the bootloader to wait for a new ROM image to be downloaded; (nb upper case)

- f - displays kernel fault information

- m - does a memory dump

- z - does a memory dump, but skips over unmapped memory space

- i - displays information on the current thread and the current process

- o - displays brief DObject information

- q - displays full DObject information

- c - displays contents of object container; (nb lower case)

- C - displays contents of object container; (nb upper case)

- r - dumps register content

##### Related concepts

- Debug Monitor
- Symbian OS Debugging Information

##### Related tasks

- Setting Up the Debug Monitor