/*
* Copyright (c) 2002-2009 Nokia Corporation and/or its subsidiary(-ies).
* All rights reserved.
* This component and the accompanying materials are made available
* under the terms of the License "Eclipse Public License v1.0"
* which accompanies this distribution, and is available
* at the URL "http://www.eclipse.org/legal/epl-v10.html".
*
* Initial Contributors:
* Nokia Corporation - initial contribution.
*
* Contributors:
*
* Description: 
*
*  The file is included by any code (cpp and resource) that needs to
*  have static (compilation time, link time, image build time) or
*  dynamic (run time) variation support for variant specific features.
*
*  This file is versioned for each platform variant.
*  The file contains declarations of features which are
*  supported and not supported by the S60 platform release 3.2
*
*  Each feature is declared as follows:
*  - declare a supported or  turned-on feature (static variation)
*    - #define __FXX
*  - declare an unsupported or turned-off feature (static variation)
*    - #undef __FXX
*  - declare ID for dynamic variation (see Feature Manager component)
*    - #define KFeatureIdFxx KOtherFeatureFirst + nn
*
*
*/


#ifndef BLDVARIANT_HRH
#define BLDVARIANT_HRH

#include "..\..\..\epoc32\include\oem\features.hrh"
#include "..\..\..\epoc32\include\variant\Symbian_OS_v9.3.hrh"

// Define base for additional features
// Reserve KOtherFeatureFirst..KOtherFeatureFirst+9 for
// feature independent dynamic variability, if needed by platform.
#define KOtherFeatureFirst  KCommonFeatureLast+1

/**
* This flag indicates that a S60 software is built
* (not real feature declaration)
*/
#define __S60_
#define __SERIES60_

/**
* This flag indicates that a S60 software version 3.2
* is built (not real feature declaration).
*/
#define __S60_32__
#define __SERIES60_32__

//
//================================================================
//                FEATURES FROM SYMBIAN_OS_V9.2.HRH
//================================================================
//
// This block lists Symbian OS features that are supported/unsupported by S60 release 3.2
//

/*
* Used to turn on and off the use of the arabica and xercesc components in
* the build system, and code in the layout compiler.
*/
#define RD_XML_PARSER_TOOLCHAIN

/*
* Enables USB mass storage feature in Symbian OS.
*/
#define WITH_MASS_STORAGE

/*
* Enables FAT32 feature in Symbian OS.
*/
#define WITH_FAT32

/*
* Disables the H2LAN plugin delivered by Symbian OS 9.2 (and later versions)
*/
#define _EXCLUDE_SIP_LAN_SUPPORT_

/*
* Excludes Symbian implementation of Java components. S60 offers its own 
* Java implementation.
*
* This flag must be always defined. Do not edit this !
*/
#define EXCLUDE_JAVA




//
//================================================================
//                FEATURES FROM FEATURES.HRH
//================================================================
//
// This block lists features that supported/unsupported by S60 release 3.2:
// See features.hrh for more information.
//

//-----------------------------------
//RnD flags
//-----------------------------------
/*
* This flag is needed for safely (without creating bottle neck)
* incorporating DOS Client/Plug-in/SAE API changes into Series 60 releases.
*/
#define RD_DOS_API_CHANGE

/*
* This R&d flag is needed for incorporating "Shared data migration to
* Central Repository" changes controlled way into Series 60 releases.
*/
#define RD_SD_TO_CENREP_CHANGE

/*
* Because 2.8 feature (scalable UI) is implemented in 2.common CCB,
* we need a temporary feature flag that can be used where needed in code to
* flag scalable UI implementation out of 2.6 builds.
* -> to avoid ROM hit in 2.6 and regression in code maturity.
*
* This flag must be always defined. Do not edit this !
*/
#define RD_SCALABLE_UI

/*
* To incorporate "System Agent migration to Publish and Subscribe"
*/
#define RD_SA_TO_PUBSUB_CHANGE

/*
* RD Feature flag for implementing "enhanced skinning" in 2.x CCB. That
* feature is not wanted in 2.6 but after 2.8 it will be permanently
* supported i.e. not optional feature.
*/
#define RD_ENHANCED_SKINNING

/*
* A R&D flag for integrating SimChanged DLL into SysAp in release 3.0. Flag
* will be removed when 2.8 branches
*
* This flag must be always defined. Do not edit this !
*/
#define RD_SIMCHANGED_REMOVED

/*
* Turning the the flag on enables special UID that can be used by a RAM
* testing tool. A tool using the UID is not closed by out-of-memory
* watchdog. Flag should not be turned on in any end product as it exposes a
* potential security risk. Instead the flag could be used at R&D time, or in
* any custom builds.
*/
#undef RD_RAM_TEST_UID

/*
* Flag is used variate the Increment 9 changes: i.e. relocation of binaries
* and resource files. We need these for 3.0 PF- security implementation.
* They are temporary R&D flags that can be removed once 2.8 is branched
* away.
*/
#define RD_SECURE_BIN_RES

/*
* Flag is in charge of variating the Increment 10 tasks: i.e. moving files
* to private directories. We need these for 3.0 PF- security implementation.
* They are temporary R&D flags that can be removed once 2.8 is branched
* away.
*/
#define RD_SECURE_PRIV_DATA

/*
* This flag must be always defined. Do not edit this !
*/
#define RD_MDF_DEVVIDEO

/*
* This R&D flag is needed for incorporating platform security and
* application architecture changes controlled way into Series 60 releases.
*/
#define RD_PF_SEC_APPARC

/*
* This R&D flag is needed for incorporating apps to exes changes controlled
* way into Series 60 releases.
*/
#define RD_APPS_TO_EXES

/*
* If this feature flag is on then the JSR-226 functionality is available.
* Otherwise it is not.
*/
#define RD_SVGT_JSR_226_API

/*
* This R&D flag is needed for variating PoC (Push-to-talk over Cellular) and
* it's UI integration to other applications / functionality.
*/
#define RD_POCUIAPI

/*
* This R&D flag defines data caging changes to components that use messaging
* API.
*/
#define RD_MESSAGING_API_V2

/*
* This R&D flag defines data caging changes to components that are used by
* messaging API components.
*/
#define RD_FILE_HANDLE_SUPPORT

/*
* This R&D flag defines changes related to start-up.
*/
#undef RD_STARTUP_CHANGE

/*
* This R&D flag defines changes related to vibra and backlight.
*/
#define RD_VIBRA_AND_LIGHT_CHANGE

/*
* Enables USB Configuration Management.
*/
#define RD_USB_WATCHER_CONFIGURATION_MGMT

/*
* This R&D flag is needed to safely integrate changes to the Common Engine
* APIs into Series 60 releases.
*/
#define RD_COMMON_ENGINE_API_CHANGE

/*
* R&D flag for managing the DOS Server and DOS APIs removal.
*/
#undef RD_DOS_SERVER_REMOVE

/*
* R&D flag for managing the Progressive Download feature implementation.
*/
#define RD_PROGDOWNLOAD

//-----------------------------------
//Misc. HW related
//-----------------------------------
/*
* Device supports Multimedia Card (MMC).
*/
#define __MMC

/*
* Device has Camera Application.
*/
#define __CAMERA

/*
* Device has also separate cover display in addition to the main display.
*/
#undef __COVER_DISPLAY

/*
* Device supports Image enhancement for transflective display. If this
* feature is on,  the Display Enhancements Adaptation API has to be
* implemented.
*/
#undef __IETD

/*
* Device contains support for FM radio (TunerUtility and RadioServer
* components).
*/
#define __FM_RADIO

/*
* Device supports automatic accessory identification.
*/
#undef __AUTO_ACCESSORY_IDENTIFICATION

/*
* Device supports side volume keys.
*/
#define __SIDE_VOLUME_KEYS

/*
* Device has Video Recorder (CamCorder) application available.
*/
#define __VIDEO_RECORDER

/*
* The flag defines is the camera lens cover is supported by the HW.
*/
#undef __CAMERA_LENS_COVER

/*
* Indicates whether a device has qwerty keyboard or not.
*/
#define __QWERTY_INPUT

//-----------------------------------
//Misc. SW related
//-----------------------------------
/*
* Device suppors flight mode. Device can be used off-line. RF and Bluetooth
* transmitters are inactive and emergency call is not possible.
*/
#undef __FLIGHT_MODE

/*
* Device suppors off-line mode. Device can be used off-line and Bluetooth
* transmitter can be enabled.  RF transmitter can be activated only for
* emergency calls.
*/
#define __OFFLINE_MODE

/*
* An application UI can control audio routing in addition to adaption layer.
* If  this feature is off, only the adaptation layer controls the audio
* routing and the corresponding DOS Plug-in API has to be implemented.
*/
#undef __APPLICATION_CONTROLLABLE_AUDIO_ROUTING

/*
* Device supports OpenGL ES and EGL versions 1.0. This feature enables 3D
* graphics rendering
*/
#define __OPENGL_ES_3DAPI

/*
* Device has a software implementation of OpenGL ES and EGL. No hardware
* support. If __OPENGL_ES_3DAPI is enabled, either HW or SW implementation
* should exist. If HW is not present, this flag should be enabled.
*/
#define __OPENGL_ES_SW_IMPLEMENTATION

/*
* Accessory framework is a Series 60 subsystem that enables adding various
* accessory types to the platform by licensees.
*/
#define __ACCESSORY_FW

//-----------------------------------
//PAN related
//-----------------------------------
/*
* Device supports Infrared.
*/
#define __IRDA

/*
* Device supports Bluetooth.
*/
#define __BT

/*
* Device supports Universal Serial Bus (USB).
*/
#define __USB

/*
* Device uses Symbian MRrouter technology for PC connectivity.  If this
* feature is on the alternative feature __SRCS shall be off.
*
* Feature not supported, this flag must be always undefined. Do not edit this !
*/
#undef __MROUTER

/*
* Device supports BT handsfree and headset profiles.
*
* This flag must be always defined. Do not edit this !
*/
#define __BT_AUDIO

/*
* Device support BT PAN profile
*
* Feature not supported, this flag must be always undefined. Do not edit this !
*/
#undef __BT_PAN_PROFILE

/*
* Devices uses Short Range Connectivity Server technology for PC
* connectivity.  If this feature is on the alternative feature __MROUTER
* shall be off
*
* This flag must be always defined. Do not edit this !
*/
#define __SRCS

/*
* Device supports Bluetooth fax profile.
*/
#undef __BT_FAX_PROFILE

/*
* Device supports bluetooth imaging profile.
*/
#define __BT_IMAGING_PROFILE

/*
* Device supports bluetooth printing profile.
*
* Feature not supported, this flag must be always undefined. Do not edit this !
*/
#undef __BT_PRINTING_PROFILE

/*
* Video telephony requires USB camera connection. USB streaming interface
* provides fast USB data transfer and control interface for imaging componet
* using the camera.
*/
#undef __USB_STREAMING

/*
* Bluetooth SIM Access Profile (SAP) allows another device to access the SIM
* over Bluetooth.
*/
#define __BT_SAP

/*
* Symbian OS side AT Handler is used with Bluetooth Hands Free profile to
* process and communicate with DOS.
*/
#define __AT_HANDLER

/*
* When this flag is enabled, the device can be put in the BT test mode.
*/
#define __BT_TEST_MODE

/*
* Device supports USB mass storage configuration and USB configuration
* management.
*/
#define __USB_PERSONALITY_AND_MSDC

//-----------------------------------
//Mobile Wallet related
//-----------------------------------
/*
* Device supports Wallet core functionality (Generic ECML Cards, Personal
* Notes and Access code)
*/
#undef __WALLET

/*
* Device supports Radio Frequency Identification (RFID) ticket information
* in Wallet settings.
*/
#undef __RFID

/*
* Device supports Single-Sign-On (SSO) feature (alias name is Mobile
* Personality identify). The feature is used to make user authentication
* easier to end user who is using e-commerce service via Wallet.
*/
#undef __SSO

//-----------------------------------
//WIM related
//-----------------------------------
/*
* Device supports WAP Wireless Identification Module (WIM).
*/
#define __WIM

/*
* Device supports reading certificates from SIM.
*/
#define __SIM_CERTIFICATES

/*
* Device supports reading OMA Provisioning files from SIM/WIM.
*/
#define __SMART_CARD_PROV

/*
* Existing component OMA Provisioning needs to be variated because not all
* platforms are intended to be used in GSM/UMTS networks, that support the
* protocol well. For example CDMA network operators use different methods
* for delivering phone settings. Especially from the 2.7 platform side, this
* kind of variability has been requested.
*/
#define __OMA_PROV

//-----------------------------------
//WAP related
//-----------------------------------
/*
* Device uses WAP WSP protocol for browsing instead of the default HTTP
* protocol.
*/
#undef __WSP

/*
* Device supports authentication based on whitelist
*
* This flag must be always defined. Do not edit this !
*/
#define __PUSH_WHITELIST

/*
* Device has Presence Enhanced Contacts application
*/
#define __DPB

/*
* Device supports Instant Messaging feature of the Wireless Village
* initiative
*/
#define __IM

/*
* Wireless Village features (__IM & __DPB) support standalone TCP/IP binding
* for Communication Initiation Request (CIR).  The TCP/IP binding uses
* persistent connection from the client to WV server to provide
* low-latency always-on CIR channel.
*/
#define __IMPS_STANDALONE_IP_CIR

/*
* Device supports Presence feature of the Wireless Village initiative.
*/
#define __PRESENCE

/*
* Controls the behaviour of the MMS application and message forwarding the
* message without retrieval. If the feature is on, the application allows
* the user to retrieve and re-forward it. If the feature is off, it is
* assumed that the message is not available any more in the MMSC after the
* forwarding.
*/
#undef __MMS_NONDESTRUCTIVE_FORWARD

/*
* Flag is used to incorporate the LightSurf Picture Messaging transport
* engine into the release.
*
* Feature not supported, this flag must be always undefined. Do not edit this !
*/
#undef __LIGHTSURF

/*
* Flag is used for inclusion or exclusion of components from the MMS UIs and
* MMS Engine subsystems.
*/
#define __MMS

//-----------------------------------
//SyncML related
//-----------------------------------
/*
* Device supports SyncML device management standard. This feature enables
* Over The Air (OTA) administration of the device settings.
*/
#define __SYNCML_DM

/*
* Device supports SyncML data synchronization standard. This feature enables
* Over The Air (OTA) synchronisation of device data.
*/
#define __SYNCML_DS

/*
* Device supports MMS data synchronisation using the SyncML.
*/
#undef __SYNCML_DS_MMS

/*
* Device supports Email data synchronization using the SyncML.
*/
#define __SYNCML_DS_EMAIL

/*
* Device supports filtering of Email data in  SyncML synchronization.
*
* Feature not supported, this flag must be always undefined. Do not edit this !
*/
#undef __SYNCML_DS_EMAIL_FILTERING

/*
* Device supports contacts data synchronization using the SyncML.
*/
#define __SYNCML_DS_CON

/*
* Device supports calendar data synchronization using the SyncML.
*/
#define __SYNCML_DS_CAL

/*
* Device supports configuring data synchronisation settings using the
* SyncML.
*/
#define __SYNCML_DM_DS

/*
* Device supports configuring Internet Access Points (IAP) using the SyncML.
*/
#define __SYNCML_DM_IAP

/*
* Device supports configuring Email settings using the SyncML.
*/
#define __SYNCML_DM_EMAIL

/*
* Device supports configuring MMS settings using the SyncML.
*/
#define __SYNCML_DM_MMS

/*
* Device supports SyncML over OBEX. This feature enables device management
* and data synchronisation over local connectivity.
*/
#define __SYNCML_OBEX

/*
* Device supports SyncML data synchronisation alert. This feature enables
* triggering data synchronisation via the alert sent by SyncML server.
*/
#define __SYNCML_DS_ALERT

/*
* Device supports short memos (notes) data synchronisation using the SyncML.
*/
#define __SYNCML_DS_NOTEPAD

/*
* Device supports device management over OBEX.
*/
#undef __SYNCML_DM_OBEX

/*
* Device management WLAN settings supported.
*/
#define __SYNCML_DM_WLAN

/*
* Device supports configuring Streaming using SyncML.
*/
#undef __SYNCML_DM_STREAMING

/*
* Device supports configuring IMPS using SyncML.
*/
#define __SYNCML_DM_IMPS

/*
* Device supports OTA firmware update.
*/
#define __SYNCML_DM_FOTA

//-----------------------------------
//Multimedia
//-----------------------------------
/*
* Device supports MP3 audio codec.
*/
#define __MP3

/*
* Device supports Speaker Independent Name Dialling (SIND). That is an
* ability to voice-dial to any contact in the phone book without first
* training a voice tag.
*/
#define __SIND

/*
* Device supports Adaptive Multi-Rate (AMR) narrowband codec.
*/
#define __AMR_NB

/*
* Device supports Adaptive Multi-Rate (AMR) wideband codec.
*/
#define __AMR_WB

/*
* Device supports Advanced Audio Coding (AAC) codec.
*/
#define __AAC

/*
* Device supports Scalable Vector Graphics - Tiny (SVGT) file format. The
* feature enables viewing 2D vector graphics animations specified by the
* W3C.
*/
#define __SVGT

/*
* Device supports streaming in SMIL content
*
* Feature not supported, this flag must be always undefined. Do not edit this !
*/
#undef __SMIL_STREAMING

/*
* Device supports macrodia flash 6.
*/
#define __MACROMEDIA_FLASH_6

/*
* Device supports MPEG4 encoding.
*/
#define __MPEG4_VIDEO_ENCODING

/*
* Device supports QCELP
*
* Feature not supported, this flag must be always undefined. Do not edit this !
*/
#undef __QCELP

/*
* Device supports MPEG-4 AAC encoding. Together with feature flag
* __MPEG4_VIDEO_ENCODING this flag can also enable enconding for MP4 file
* format.
*/
#define __MPEG4_AAC_ENCODING

/*
* Device supports Speaker Dependent Name Dialling (SIND). That is an ability
* to voice-dial to a contact in the phone book by training a voice tag for
* the contact.
*/
#undef __SDND

/*
* AMR NB codec controller plug-in uses CMMFCodec (all-ARM software
* implementation) instead of using the codec through HWDevice.
*/
#define __USE_AMR_NB_CMMFCODEC

/*
* AMR WB codec controller plug-in uses CMMFCodec (all-ARM software
* implementation) instead of using the codec through HWDevice.
*/
#define __USE_AMR_WB_CMMFCODEC

/*
* AAC codec controller plug-in uses CMMFCodec (all-ARM software
* implementation) instead of using the codec through HWDevice.
*/
#define __USE_AAC_CMMFCODEC

/*
* MP3 codec controller plug-in uses CMMFCodec (all-ARM software
* implementation) instead of using the codec through HWDevice.
*/
#define __USE_MP3_CMMFCODEC

/*
* QCELP codec controller plug-in uses CMMFCodec (all-ARM software
* implementation) instead of using the codec through HWDevice.
*/
#define __USE_QCELP_CMMFCODEC

/*
* AMR NB CMMFCodec (all-ARM software implementation) is included in build to
* be used by some other client  than controller plug-in component.
*/
#define __INCLUDE_AMR_NB_CMMFCODEC

/*
* AMR WB CMMFCodec (all-ARM software implementation) is included in build 
* to be used by some other client than controller plug-in component.
*/
#define __INCLUDE_AMR_WB_CMMFCODEC

/*
* AAC CMMFCodec (all-ARM software implementation) is included in build  to
* be used by some other client than controller plug-in component.
*/
#define __INCLUDE_AAC_CMMFCODEC

/*
* MP3 CMMFCodec (all-ARM software implementation) is included in build  to
* be used by some other client than controller plug-in component.
*/
#define __INCLUDE_MP3_CMMFCODEC

/*
* QCELP CMMFCodec (all-ARM software implementation) is included in build  to
* be used by some other client  than controller plug-in component.
*/
#define __INCLUDE_QCELP_CMMFCODEC

/*
* The component provides metadata information for music clients based on the
* 2.2,2.3,and 2.4 standards of ID3V2.
*
* This flag must be always defined. Do not edit this !
*/
#define __ID3V2_METADATA

/*
* Enables a utility for 3rd party applications to play DRM encrypted audio.
*
* This flag must be always defined. Do not edit this !
*/
#define __MMF_DRM_UTILITY

/*
* Device supports utility APIs and framework for Series 60 Audio
* applications to enable predefined audio effects with audio play/record
* utilities. Features lilke Volume, Graphical Equalizer, Reverb are
* possible.
*/
#define __AUDIO_EFFECTS_API

/*
* Device supports Audio Resource Indications Utility. Applications can use
* the Audio Resource Indications Utility to request feedack when they can
* submit a play request.
*/
#define __AUDIO_RESOURCE_INDICATIONS

/*
* Device supports Multimedia Comms Controller for VoIP.
*
* Feature not supported, this flag must be always undefined. Do not edit this !
*/
#undef __MMCOMMSCONTROLLER

/*
* Device supports Multimedia Comms Controller for OMA PoC.
*/
#define __MMCOMMSAVCONTROLLER

/*
* Device supports Multimedia Comms Engine for OMA PoC.
*/
#define __MMCOMMSENGINE

/*
* Device supports playback of WMA audio files.
*/
#define __WMA

//-----------------------------------
//Telephony
//-----------------------------------
/*
* Device supports GSM cellular stack.
*/
#define __PROTOCOL_GSM

/*
* Device supports WCDMA cellular stack
*/
#define __PROTOCOL_WCDMA

/*
* Device supports CDMA cellular stack.
*
* Feature not supported, this flag must be always undefined. Do not edit this !
*/
#undef __PROTOCOL_CDMA

/*
* Device supports TDMA cellular stack.
*
* Feature not supported, this flag must be always undefined. Do not edit this !
*/
#undef __PROTOCOL_TDMA

/*
* Device supports Internet Over The Air (IOTA), applicable only to CDMA
* devices. This feature enables over the air provisioning of mobile devices
* using HTTP.
*
* Feature not supported, this flag must be always undefined. Do not edit this !
*/
#undef __CDMA_IOTA

/*
*
* Feature not supported, this flag must be always undefined. Do not edit this !
*/
#undef __CDMA_EXTENDED_AMS

/*
* Device supports SIM card in the user interface applications, e.g. SMS
* application. 
*/
#define __SIMCARD

/*
* Device supports circuit switched video telephony
*/
#define __CS_VIDEO_TELEPHONY

/*
*/
#undef __PHONE_HIDE_MO_DATACALL_NUMBER

/*
*
* Feature not supported, this flag must be always undefined. Do not edit this !
*/
#undef __CDMA_FAST_DORMANT

/*
*/
#undef __PHONE_NUMBER_GROUPING

/*
* Number matching from SIM. Feature enables the usage of SIM phonebook in
* addition to Symbian Contacts database.
*/
#define __SIM_PHONEBOOK_MATCH

/*
* When this flag is enabled it Common TSY component is included.
*/
#define __COMMON_TSY

/*
* When this flag is enabled it is possible to dial an emergency call even
* when the off-line mode is on.
*/
#define __COMMON_TSY__EMERGENCY_CALLS_ENABLED_IN_OFFLINE_MODE

/*
* When this flag is enabled it Common DSY component is included.
*/
#define __COMMON_DSY

/*
* VoIP is enabled in terminal when this flag is enabled.
*
* Feature not supported, this flag must be always undefined. Do not edit this !
*/
#undef __VOIP

//-----------------------------------
//Security
//-----------------------------------
/*
* Device supports OMA Digital Rights Management (DRM) partially, only
* forward lock is supported
*/
#define __DRM

/*
* Device uses DRM in closed content policy which prevents sending that
* content out of device which has the configured MIME type.
*/
#define __USE_DRMENGINE_IN_CCP

/*
* Device supports OMA Digital Rights Management (DRM) fully. Includes
* forward lock, combined delivery, separate delivery and super-distribution
*/
#define __DRM_FULL

/*
* Device supports secure HW that can be used through the Secure Environment
* API.
*
* Feature not supported, this flag must be always undefined. Do not edit this !
*/
#undef __SECURE_HW

/*
* This feature flag is used with OMA DRM standard version 2 (Phase2)
* features.
*/
#define __DRM_PHASE2

/*
* DRM clock is a new clock type that is used with DRM interval and datetime
* based constraints. It uses NITZ (other solutions can be studied) to get
* the network time and uses that to determine if the time constrained
* content can be rendered or not. This enables the content providers to sell
* content “twice” e.g. first for a short period of time and after that
* (assumed user lock in) for 2nd time with full usage rights.
* The user shall still have control over the normal clock of the device, but
* setting of that clock shall not have effect to the DRM clock.
*
* If NITZ is not available, user defined clock is used.
*/
#define __DRM_CLOCK

/*
* There must be possibility to transfer downloaded applications and other
* DRM content to the swap phone in a service point through service software.
* UDT makes it possible to transfer user's valuable content and Rights DB
* containig Rights objects for DRM content to another phone (containing same
* functionality) e.g. in warranty cases.
*/
#undef __DRM_USER_DATA_TRANSFER

/*
* This feature flag is used to indicate whether OMA DRM standard version 2
* is enabled.
*/
#define __DRM_OMA2

//-----------------------------------
//Networking
//-----------------------------------
/*
* Device supports Quality of Service (QOS). The QoS is capability of a
* network to provide better service to selected network traffic.
*/
#define __QOS

/*
* Device supports IP Security (IPSec). The IPSec is a set of protocols
* developed by the IETF to support secure exchange of packets at the IP
* layer. IPsec has been deployed widely to implement Virtual Private
* Networks (VPNs).
*/
#define __IPSEC

/*
* This flag defines whether Data Connection Logger component sets Attach
* Mode and Default APN parameters to TSY at system boot.
*/
#define __LOGGER_GPRS

/*
* This flag defines whether the information of current radio link using EDGE
* is available through Connection Monitor component.
*/
#define __EDGE_KNOWLEDGE

/*
* This flag defines whether network registration status including roaming
* information is available from Connection Monitor server component.
*/
#define __NETWORK_REGISTRATION

/*
* Devices supports Mobile IPv6.
*/
#undef __MIPV6

/*
* Device supports Dynamic Host Configuration Protocol (DHCP).
*/
#define __DHCP

/*
* Defines whether the Connection Monitor Extension API is used.
*/
#define __CONNMON_EXTENSION

/*
* Device supports WLAN protocol.
*/
#define __PROTOCOL_WLAN

/*
* Device supports internal (HS)CSD in application UIs.
*/
#define __APP_CSD_SUPPORT

/*
* Devices supports Mobile IPv4
*/
#undef __MIPV4

/*
* Device supports network address translation of IP (version 4) connections.
*/
#undef __IPV4_NAT

//-----------------------------------
//Location
//-----------------------------------
/*
* Defines whether landmarks feature is supprted in the device.
*
* This flag must be always defined. Do not edit this !
*/
#define __LANDMARKS

/*
* Device supports location basic services.    Must always be supported due
* SDK APIs.
*
* This flag must be always defined. Do not edit this !
*/
#define __LOCATIONFRAMEWORKCORE

/*
* Device supports location privacy. It enables controlling end user privacy.
*  Must always be supported due SDK APIs.
*/
#define __PRIVACYFRAMEWORK

/*
* Devices supports Bluetooth based GPS positining. It utilizes bluetooth
* connection to retrieve location information from wireless GPS device,
* which supports required Bluethooth profile.  Must always be supported due
* SDK APIs.
*/
#define __BLUETOOTHGPSPSY

/*
* This feature provides functionality for reading from and writing to the
* XML-based landmarks content format.
* Must always be supported due SDK APIs. There are two components with this
* feature:
* - Ecom plug-in under Landmarks API that converts from the landmarks
* content format to native landmark objects and vise versa.
* - Recognizer Plug-in to recognizer FW for detecting landmarks content
* format.
*
* This flag must be always defined. Do not edit this !
*/
#define __LANDMARKS_CONVERTER

/*
* Device has Location system application.  Must always be supported due SDK
* APIs.
*/
#define __LOCATIONSYSUI

//-----------------------------------
//Imaging
//-----------------------------------
/*
* Optimisation flag of the CamCorder for cases where device replaces the
* default Camcorder plugin. Then this flag must be turned off (#undef) due
* to performance reasons.
*/
#define __CAE_VR_CUSTOM_COMMANDS

/*
* Camera application supports burst mode. It enables taking several
* snapshots with one command.
*/
#define __CAMERA_BURST_MODE

/*
* Java implementation supports Java Mobile Media API (JSR135) version 1.1
*/
#define __JAVA_MMAPI11

/*
* Java implementation supports Java File API (JSR75)
*/
#define __JAVA_FILEAPI

/*
* Java implementation supports Java PIM API (JSR75)
*/
#define __JAVA_PIMAPI

/*
* Java implementation supports 3D API  (JSR184)
*/
#define __JAVA_3DAPI

/*
* Java implementation supports Java Location API (JSR-179)
*/
#define __JAVA_LOCATIONAPI

/*
* Device supports Online Certificate Status Protocol (OCSP). The protocol
* specifies the syntax for communication between the server (which contains
* the certificate status) and the client application (which is informed of
* that status).
*/
#define __OCSP

/*
* Java J2ME Web Services API (JSR-172) compliancy.
* Provides two new capabilities to the J2ME platform:
* (1) access to remote SOAP / XML based web services
* (2) parsing XML data
*/
#define __JAVA_J2MEWEBSERVICESAPI

//-----------------------------------
//Browser
//-----------------------------------
/*
* Purpose is to variate IMEI notification setting in Browser. In case when
* feature is on ,  user can see new
* setting item in Browser setting "IMEI notification" . If user enables the
* setting on browser,  UA prof filter will send phone's IMEI code within
* User-Agent field.
*/
#undef __BROWSER_IMEI_NOTIFICATION

/*
* The PluginAdapterUtil is a variant DLL that guarantees a common interface
* for plugins when interfacing with the Browser (PluginAdapter Interface).
* Proxy interface is used and flag is enabled with Opera browser.
*
* Feature not supported, this flag must be always undefined. Do not edit this !
*/
#undef __BROWSER_PLUGIN_INTERFACE_PROXY

/*
* Browser application supports additional list of bookmarks that gets
* generated automatically from visited links.  List is sorted by automatic
* algorithm which ranks according to combination of most-recently and
* most-often visited pages.
*/
#define __BROWSER_ADAPTIVE_BOOKMARKS

/*
* Browser application supports URL completion. When user manually enters "go
* to" URL, list of previously-visited links will appear for selection based
* on matching entered characters.
*/
#define __BROWSER_URL_COMPLETION

/*
* This feature displays a 'CNN type' ticker of text pushed via cell
* broadcast, onto the idle screen of the phone.
*/
#undef __NEWSTICKER




//================================================================
//                 SERIES60 ADDED FEATURES
//================================================================


#ifdef __BT_AUDIO
// Deprecated define for release 1.x compatibility
#define __SERIES60_BT_AUDIO
#endif

#ifdef __BT
// Deprecated define for release 1.x compatibility
#define __SERIES60_BT
#endif

#ifdef __IRDA
// Deprecated define for release 1.x compatibility
#define __SERIES60_IR
#endif

// Feature on: MMC support
#ifdef __MMC
// Deprecated define for release 1.x compatibility
#define __SERIES60_MMC
#endif

// Feature on: __PHONE_HIDE_MO_DATACALL_NUMBER support
#ifdef __PHONE_HIDE_MO_DATACALL_NUMBER
// Deprecated define for release compatibility
#define __SERIES60_PHONE_HIDE_MO_DATACALL_NUMBER
#endif

// Feature on: __VIDEO_RECORDER support
#ifdef __VIDEO_RECORDER
// Deprecated define for release compatibility
#define __SERIES60_VIDEO_RECORDER
#endif

// Feature on: __PHONE_NUMBER_GROUPING support
#ifdef __PHONE_NUMBER_GROUPING
// Deprecated define for release compatibility
#define __SERIES60_PHONE_NUMBER_GROUPING
#endif


/*
* This R&D flag defines changes to SendUI API clients.
*/
#define RD_SUPPORT_SENDUI_API_V2

/*
* R&D feature flag for implementing new Client/Server FavouritesEngine API.
*/
#define RD_NEW_FAVENG_API

/*
* R&D feature flag for moving idle functionality from Phone application to
* Idle application.
*/
#define RD_IDLE_SEPARATION

/*
* R&D flag for implementing browser launcher API change.
*/
#define RD_BROWSER_LAUNCHER_API_CHANGE

/*
* R&D flag for implementing UIFW 3.0 API changes.
*/
#undef RD_UIFW_3_0_API_CHANGES

/*
* R&D flag for implementing Uikon unbranch related changes to Series 60
* code.
*/
#define RD_UIKON_UNBRANCH

/*
* R&D Flag to handle migration from old insecure Pinboard API to new one.
*/
#undef RD_PINB_SRV_CHANGE

/*
* R&D Flag to remove HTML plugin from mail 3.0 implementation.
*/
#define RD_EMAIL_HTML_VIEW

/*
* In 3.1 Feature Manager will be removed from CommonEngine and new Feature
* Manager component will be introduced. Flag is needed to safely implement
* the change.
*/
#define RD_FEATURE_MANAGER_CHANGE

/*
* R&D Flag to remove Scale II (Pen and Touch) support from other than S60
* 4.0 builds.
*
* Feature not supported, this flag must be always undefined. Do not edit this !
*/
#undef RD_SCALABLE_UI_V2

/*
* R&D Flag to remove 3.1 Toolbar and Generic Buttons
*/
#define RD_TOOLBAR_SUPPORT

/*
* Meeting request feature adds meeting request utlis non-variable component
* to platfrom.
*/
#define RD_MEETING_REQUEST_UTILS

/*
* Device allows a video file to be set as a ringing tone.
*/
#define RD_VIDEO_AS_RINGING_TONE

/*
* General Settings Application Renovation
*/
#define RD_GS_RENOVATION

/*
* Unified SMS and MMS Editor,  targetted for release 3.1U
*/
#define RD_UNIFIED_EDITOR

/*
* Bluetooth user interface renovation.
*/
#define RD_BTUI_RENOVATION

/*
* This flag enables ScaleII component "Preview Popup".
*/
#define RD_PREVIEW_POPUP

/*
* This flag enables the flip (clamshell) and grip (slider) event handling.
* Devices without this functionality can leave the TelephonyDeviceMode.DLL
* component out of their builds.
*/
#define RD_TELEPHONY_DEVICE_MODE

/*
* R&D Flag to enable smooth development & integration of customazable Active
* Idle.
*/
#define RD_CUSTOMIZABLE_AI

/*
* R&D Flag to remove video mailbox support from older than S60 3.1 builds.
*/
#define RD_VIDEO_MAILBOX_SUPPORT

/*
* This flag enables early development of Bluetooth OPP/BIP features (3.1u).
*/
#define RD_BT_MSG_RENOVATION

/*
* This flag enables early development of  AIW Help consumer integration
* feature.
*/
#define RD_HELP_AIW_INTEGRATION

/*
* R&D Flag to control inclusion of ScaleII feature: Stretch two-lined list
* automatically as one-lined.
*/
#define RD_LIST_STRETCH

/*
* RD flag to flag out implementation of Enhanced CBA
*/
#undef RD_ENHANCED_CBA

/*
* RD flag to flag out implementation of Split view.
*/
#undef RD_SPLIT_VIEW

/*
* Support for Browser Plugin. Used in deciding whether the browser video
* plugin is taken in.
*/
#define RD_BROWSER_VIDEO_PLUGIN

/*
* This flag enables 3GP Write Extention feature in Record Utility.
*/
#undef RD_3GP_WRITE_EXTENTION

/*
* Feature flag enables the usage of the Virtual Phonebook APIs.
*/
#define RD_VIRTUAL_PHONEBOOK

/*
* Media Gallery updated features for 3.1
*/
#define RD_MEDIA_GALLERY_UPDATED_FEATURES

/*
* This R&D flag is needed for safely incorporating Gif animation support for
* screensaver Animation Plugin
*/
#define RD_SCREENSAVER_GIFANIMATION

/*
* This flag allows to choose from either built-in Display Post
* implementation or an external Display Post module.
*/
#undef RD_DISPLAY_POST

/*
* Phonebook application supports multiple contact stores. It enables users
* to manage contacts from multiple repositories in one application.
*/
#define RD_PHONEBOOK2

/*
* A flag to control one of the sub-features in OMA DRM v2 implementation.
*/
#define RD_DRM_IMSI_BINDING

/*
* A flag to control one of the sub-features in OMA DRM v2 implementation.
*/
#define RD_DRM_BUY_NEW_RIGHTS_BEFORE_EXPIRATION

/*
* A flag to control one of the sub-features in OMA DRM v2 implementation.
*/
#define RD_DRM_DROPPED_30_FEATURES

/*
* A flag to control one of the sub-features in OMA DRM v2 implementation.
*/
#undef RD_DRM_DETAILS_VIEW_RENOVATION

/*
* A flag to control one of the sub-features in OMA DRM v2 implementation.
*/
#define RD_DRM_RINGTONE_BLOCKING

/*
* All signature connector development is done behind this R&D feature flag.
*/
#define RD_S60_SIGNATURE_CONNECTOR

/*
* Trackster is a generic component, which can be used for various purposes
* in various applications. The basic idea and the innovation behind the work
* is to build the behavior based on Bezier curves, which define how the
* control appears.
*/
#define RD_TRACKSTER_MENU

/*
* This flag allowes early development of new General Settings features.
*/
#define RD_GS_RENOVATION_PHASE2

/*
* This flag allowes early development of new Flash as Screensaver features.
*/
#define RD_FLASHLITE_SCREENSAVER

/*
* This flag controls the messaging virtual phonebook migration independently
* from RD_VIRTUAL_PHONEBOOK
*/
#define RD_MESSAGING_VIRTUAL_PHONEBOOK

/*
* This R&D flag is needed for incorporating "Multiple Alarms"  in ClockApp.
*/
#define RD_MULTI_ALARMS

/*
* This flag controls major changes in File Manager and memory card
* applications that are implemented in CCB.
* Changes include memory card application removal and MCAppEngine.dll move
* to file manager app with code and resource modifications.
*/
#undef RD_FILE_MANAGER_MMC_MERGE

/*
* This flag controls configurability features to System Application
* (referred as "SysAp") and HwResourceManager (referred as HWRM) components.
* SysAp needs this flag for moving part of its key event handling
* functionality to a plug-in that can be variated by product programs.
* HWRM needs this flag for moving part of its light controlling
* functionality to a plug-in that can be variated by product programs.
*/
#undef RD_DEVICE_MODE_CONFIGURABILITY

/*
* This flag is used to determine whether the automatic keyguard features in
* Autolock are compiled.
*/
#define RD_AUTO_KEYGUARD

/*
*  When enabled, Music Collection server monitors USB and memory card events
* and performs a database refresh when new card is inserted or USB cable is
* disconnected. It will also perform the refresh after startup. The refresh
* is handled as a low priority task in the background.
*/
#define RD_MUSIC_COLLECTION_AUTO_REFRESH

/*
* R&D Flag to control inclusion of the feature "animation effects".
*/
#define RD_ANIMATION_EFFECTS

/*
* R&D Flag to exclude dialog sliding from other "animation effects".
*/
#undef RD_SLIDING_ANIMATION_EFFECTS

/*
* R&D Flag to separate XML UI framework phase 2 development work from phase
* 1.
*/
#undef RD_XMLUI_2

/*
* R&D Flag to enable smooth integration of customizable to device bootup.
* The flag is used variate out current Idle + Active Idle solution and
* replace it new customizable AI.
*/
#undef RD_BOOT_CUSTOMIZABLE_AI

/*
* In order to enable safe development of  OMA DRM v2 Silent rights object
* acquisition
*/
#define RD_DRM_SILENT_RIGHTS_ACQUISITION

/*
* R&D flag that enables the Streaming Source supports for  Audio
* Controllers.
*/
#define RD_AUDIOCONTROLLER_STREAMINGSOURCE_SUPPORT

/*
* This R&D flag is needed to safely integrate changes needed to remove
* hard-coded dialog borders in S60 UI framework.
*/
#undef RD_NO_DIALOG_BORDERS

/*
* Defines whether a set of images can be set as wallpaper. Wallpaper is
* shown based on user defined value and then changed to a new image in the
* image set.
*/
#undef RD_SLIDESHOW_WALLPAPER

/*
* Defines whether a set of images can be set as wallpaper. Wallpaper is
* shown based on user defined value and then changed to a new image in the
* image set.
*/
#undef RD_SLIDESHOW_SCREENSAVER

/*
* Enables Application and Network Level Roaming.
*/
#define RD_ALR_AND_NLR_ENABLERS

/*
* ImageViewer's ImagePreview API and DLL are available in release.
*/
#define RD_IMAGEPREVIEW

/*
* This Helix engine flag is needed to variate S60 Video engine solution
* between all ARM MicroPlayer (ROP) and Helix engines.
*/
#define RD_ARM_MDF_HELIX_ENGINE

/*
* This flag enables new UI concept and plugin framework for regional
* calendar enhancements. The flag disables old Chinese Lunar Calendar
* implementation (without plugin framework) and enables new Lunar Calendar
* plugin (using framework).
*/
#define RD_CALENDAR_PLUGIN_FW

/*
* RD Feature flag for implementing new Browser 3.2 features prior to
* branching 3.1
*/
#define RD_32_BROWSER

/*
* RD Feature flag for implementing new  WOW:Gallery/Image Viewer Evolution
* 3.2 features prior to branching 3.1.
*/
#undef RD_WOW_GALLERY_EVOLUTION

/*
* RD Feature flag for splitting Messaging UI Utilities API into domain and
* internal parts.
*/
#undef RD_MUIU_SPLIT

/*
* RD feature flag for implementing audio playback support in SVG-T engine.
*/
#undef RD_SVGT_AUDIO_SUPPORT

/*
* RD feature flag for implementing additional backup improvements for File
* Manager.
*/
#undef RD_FILE_MANAGER_BACKUP

/*
* RD feature flag for enabling full screen wallpaper development.
*/
#undef RD_FULLSCREEN_WALLPAPER

/*
* RD feature flag for new fastswap tasklist development.
*/
#define RD_FSW_V2

/*
* RD feature flag for file manager - memory card merge changes.
*/
#define RD_FILE_MANAGER_MMC_MERGE

/*
* RD feature flag for development of new Phone architecture.
*/
#undef RD_PHONE_NG

/*
* Device allows a video file to be set as a ringing tone.
*/
#define RD_VIDEO_AS_RINGING_TONE

/*
* Enable enhanced view sorting in Gallery
*/
#undef RD_WOW_GALLERY_SORTING_VIEWS

/*
* Enable video thumbnail support in Gallery
*/
#undef RD_WOW_GALLERY_VIDEO_THUMBNAILS

/*
* Image Handling Library utilized Extended ICL JPEG API
*/
#undef RD_IHL_EXTJPEGAPI

/*
* Image Viewer uses transparent custom UI controls
*/
#undef RD_IV_TRANSPARENT_UI

/*
* Java architecture renewal, phase 1. S60 implementation replaces Symbian
* implementation of Java Installer, Java Registry and Java Backup
* components.
*/
#define RD_JAVA_ARCHITECTURE_RENEWAL_PHASE1

/*
* Attach vCards to MMS in MMS editor
*/
#undef RD_MMS_VCARD

/*
* Zooming in message lists
*/
#undef RD_MESSAGE_LIST_ZOOMING

/*
* Zooming support in message viewers and editors
*/
#undef RD_MESSAGE_VIEWER_ZOOMING

/*
* MMS Read Receipt handling
*/
#undef RD_MMS_READ_RECEIPT

/*
* MMS Postcard extra charge notification
*/
#undef RD_MMS_POSTCARD_CHARGE

/*
* Client-Server model implementation for SendUI
*/
#undef RD_SENDUI_SERVER

/*
* SVG-T rendering support in messaging applications
*/
#undef RD_SVGT_IN_MESSAGING

/*
* S60 support for configuring soft notifications
*/
#undef RD_CONFIGURING_SOFT_NOTIFICATIONS

/*
* EP integration: Streamlined e-mail deletion
*/
#undef RD_STREAMLINED_EMAIL_DELETION

/*
* EP integration: Matching sender address to Contacts in e-mail
*/
#undef RD_MATCHING_SENDER_IN_EMAIL

/*
* Ability to integrate licensee's settings application with Email app
*/
#undef RD_LICENCEE_WIZARD

/*
* Video conversion API for Messaging
*/
#undef RD_MESSAGING_VIDEO_CONVERSION_API

/*
* OMA DS mail improvements
*/
#undef RD_OMA_DS_EMAIL_IMPROVEMENTS

/*
* EP integration: E-mail priority flag support
*/
#undef RD_EMAIL_PRIORITY

/*
* EP integration: Reply-to support in SMTP e-mail
*/
#undef RD_REPLY_TO_IN_SMTP

/*
* RD flag for development of RemoteLock feature.
*/
#undef RD_REMOTELOCK

/*
* RD flag for development of new XML Engine APIs.
*/
#define RD_XML_ENGINE_API_CHANGE

/*
* RD flag for development of new AIW Dial Data APIs.
*/
#undef RD_AIW_DIAL_DATA_API

/*
* RD flag for development of Client certificates and private key handling
* feature.
*/
#undef RD_CLIENT_CERTIFICATES

/*
* RD flag for development of Symbian version of S60 SyncML engine
*/
#undef RD_USE_SYMBIAN_SYNCML_CONVERGENCE

/*
* RD flag for development of multimedia ringing tones in Cover UI
*/
#undef RD_MULTIMEDIA_RINGING_TONES_FOR_COVER_UI

/*
* RD flag for development of metadata performance improvements
*/
#undef RD_METADATA_UTILITY_32

/*
* RD flag for development of IM UI facelift
*/
#undef RD_IM_UI_FACELIFT

/*
* Feature enables flexible memory usage for storing update files on c-drive.
* RnD flag will be used temporarily for increment 15 development time only
* to flag changes made on component fotaserver and SyncMLNotifier.
*/
#undef RD_FOTA_FLEXIBLE_MEMORY_USAGE

/*
* RD flag for development of new, combined AudioVideoPlugin
*/
#undef RD_BROWSER_USE_AUDIOVIDEOPLUGIN

/*
* Feature enables the blocking the SyncML Device Management session (Either
* for Device settings like MMS settings or for FOTA downloads) when user in
* roaming networks. This RnD flag will be used temporarily for increment 15
* development time only to flag changes made on component SyncMLNotifier.
*/
#undef RD_DM_ROAMING_BLOCKING_SUPPORT

/*
* Feature enables the Device Manager UI evolution feature. This RnD flag
* will be used temporarily for increment 15 development time only to flag
* changes made on components OmaDmAppUi, SyncMLNotifier and fotaserver.
*/
#undef RD_OMADMAPPUI_UI_EVOLUTION

/*
* Feature enables the Device Management Internet Access Adapter
* implementation which supports Application Level Roaming and Networking
* Level Romaing feature in S60 platform. This RnD flag will be used
* temporarily for increment 15 development time only to flag changes made on
* component OmaDmExtensions.
*/
#undef RD_DM_APPLICATION_LEVEL_ROAMING_SUPPORT

/*
* RD flag for development of Toolbar in Video Telephony.
*/
#undef RD_VT_TOOLBAR

/*
* RD flag for development of video preferences (brightness/contrast/color
* tone/white balance) in video telephony.
*/
#undef RD_VT_VIDEO_PREFERENCES

/*
* RD flag for development of ActiveSync
*/
#define RD_ACTIVESYNC_UI_INTEGRATION

/*
* RD flag for development of new Data Sync UI
*/
#undef RD_DS_UI_EVOLUTION

/*
* RD flag for development of new Widgets implementation
*/
#undef RD_BROWSER_WIDGETS

/*
* RD flag for development of Catalogs client v3
*/
#undef RD_CATALOGS_CLIENT

/*
* Flag is used to remove SAE component.
*/
#undef RD_REMOVE_SAE

/*
* RD flag for development of Read Audio support in Music Player.
*/
#undef RD_RA_SUPPORT_FOR_MUSIC_PLAYER

/*
* RD flag to enable/disable the progressive download functionality for
* certain types of browser-downloadable content.
*/
#undef RD_BROWSER_PROGRESSIVE_DOWNLOAD

/*
* RD flag to enable/disable the Extended ICL JPEG API.
*/
#undef RD_EXTENDED_ICL_JPEG_API

/*
* RD flag for Sensor FW development
*/
#undef RD_SENSOR_FW

/*
* RD-flag for early development of light control customizability features to
* System Application.
*/
#undef RD_LIGHT_CONTROL_CHANGE

/*
* Enable/disable Grid view in Gallery
*/
#define RD_GALLERY_GRID

/*
* Enable disable Preview Popup in Gallery
*/
#undef RD_GALLERY_PREVIEW_POPUP

//-----------------------------------
//IBY flags
//-----------------------------------
/*
* This flags controls whether Jerusalem or Tel Aviv appears in the common
* city list. E.g. in Startup, GS or Clock application.
*/
#undef __ROM_HIDE_JERUSALEM

/*
* Device contains Series 60 FM Radio application components.
*/
#undef __S60_FM_RADIO_APPLICATION
#define KFeatureIdS60FmRadioApplication KOtherFeatureFirst+539

/*
* Indicates whether a device has a pen support.
*/
#define __PEN_SUPPORT
#define KFeatureIdPenSupport KCommonFeatureFirst+409

/*
* Indicates whether a device has a vibra support.
*/
#define __VIBRA
#define KFeatureIdVibra KCommonFeatureFirst+410

/*
* TV-Out Settings UI
*/
#undef __TV_OUT
#define KFeatureIdTvOut KOtherFeatureFirst+540

/*
* Device does not have dedicated key for power management, but the
* functionality is combined to some other hard key.
*/
#undef __NO_POWERKEY
#define KFeatureIdNoPowerkey KOtherFeatureFirst+639

/*
* Touch Screen Calibration application.
*/
#undef __PEN_SUPPORT_CALIBRATION
#define KFeatureIdPenSupportCalibration KOtherFeatureFirst+658

/*
* HWRM Target Modifier Plug-in (TMP) is responsible for device specific
* target modifications according to target activation status. Customers
* desiring custom functionality can simply replace the entire plug-in by
* udefining the flag and implementing own plug-in.
*/
#undef __HWRM_TARGET_MODIFIER_PLUGIN
#define KFeatureIdHwrmTargetModifierPlugin KOtherFeatureFirst+665

/*
*/
#undef __FLASH_LITE_VIEWER
#define KFeatureIdFlashLiteViewer KOtherFeatureFirst+145

/*
*/
#undef __FLASH_LITE_BROWSER_PLUGIN
#define KFeatureIdFlashLiteBrowserPlugin KOtherFeatureFirst+146

/*
* This flag enables I-Cal syncronization.
*/
#undef __I_CAL_SUPPORT
#define KFeatureIdICalSupport KOtherFeatureFirst+588

/*
* Device supports Virtual keyboard input ( on-screen keyboard).
*/
#define __VIRTUAL_KEYBOARD_INPUT
#define KFeatureIdVirtualKeyboardInput KOtherFeatureFirst+603

/*
* Device supports handwriting recognition input.
*/
#define __HANDWRITING_RECOGNITION_INPUT
#define KFeatureIdHandwritingRecognitionInput KOtherFeatureFirst+604

/*
* Device has a software implementation of OpenVG API. If no hardware support
* is present, this flag should be enabled.
*/
#define __OPENVG_SW_IMPLEMENTATION
#define KFeatureIdOpenvgSwImplementation KOtherFeatureFirst+605

/*
* Enables a subset of call barring options to be displayed in GS.
*/
#undef __RESTRICTED_CALL_BARRING
#define KFeatureIdRestrictedCallBarring KOtherFeatureFirst+608

/*
* Enables alternative call divert view and handling in GS.
*/
#undef __RESTRICTED_CALL_DIVERT
#define KFeatureIdRestrictedCallDivert KOtherFeatureFirst+609

/*
* Mediator is a server that extends mechanisms of inter-process
* communication. It supports creation of indirect interfaces for passing
* commands and events between clients and easy transfer of large amounts of
* data.
*/
#define __MEDIATOR
#define KFeatureIdMediator KOtherFeatureFirst+614

/*
* The Manner Mode can SET/CANCEL the following settings at one time by
* simply depressing the Manner Key.
*     ·Mute Ring tone
*     ·Vibration Ringer
*     ·Mute Key Confirmation Tone
*     ·Boost Mic Sensitivity
*     ·Mute Low Power Alarm
*     -Shutter sound must not be mute
*/
#undef __MANNER_MODE
#define KFeatureIdMannerMode KOtherFeatureFirst+629

/*
* This feature activates the zooming support in Series 60 UI.
*/
#define __UI_ZOOM
#define KFeatureIdUiZoom KOtherFeatureFirst+631

/*
* This feature activates the Exchange Active Sync UI.
*/
#define __MOBILE_ACTIVE_SYNC
#define KFeatureIdMobileActiveSync KOtherFeatureFirst+651

/*
* Component enables service provider specific branding in applications.
*/
#undef __BRANDING_SERVER
#define KFeatureIdBrandingServer KOtherFeatureFirst+657

/*
* MRT libraries: Open C, SSL, GLIB and RGA.
*/
#undef __MRT_SDK_LIBRARIES
#define KFeatureIdMrtSdkLibraries KOtherFeatureFirst+663

/*
* Device supports USB device lock functionality.
*/
#define __USB_DEVICE_LOCK
#define KFeatureIdUsbDeviceLock KOtherFeatureFirst+140

/*
* Includes and excludes components used in PictBridge printing.
*/
#undef __USB_PICTBRIDGE
#define KFeatureIdUsbPictbridge KOtherFeatureFirst+531

/*
* Includes and excludes PTP (Picture Transfer Protocol) components.
*/
#undef __USB_PTP
#define KFeatureIdUsbPtp KOtherFeatureFirst+532

/*
* Enables multipersonality support in USB
*/
#define __USB_MULTIPERSONALITY
#define KFeatureIdUsbMultiPersonality KOtherFeatureFirst+534

/*
* Includes and excludes UI components used in PictBridge printing
*/
#undef __USB_PICTBRIDGE_UI
#define KFeatureIdUsbPictbridgeUi KOtherFeatureFirst+566

/*
* Device supports Bluetooth stereo audio.
*/
#define __BT_STEREO_AUDIO
#define KFeatureIdBtStereoAudio KOtherFeatureFirst+580

/*
* The feature enables device to support Dial-up Networking service
* (Bluetooth, IrDA or USB).
*/
#define __DIALUP_NETWORKING
#define KFeatureIdDialupNetworking KOtherFeatureFirst+660

/*
* Device supports Plug and Play Mobile Services.
*/
#undef __PLUG_AND_PLAY_MOBILE_SERVICES
#define KFeatureIdPlugAndPlayMobileServices KOtherFeatureFirst+659

/*
* Presence Framework provides protocol agnostic presence handling services
* to S60 applications and subsystems. Concrete presence protocols are
* implemented as plug-ins to Presence Framework. In long run protocol
* agnostic Presence Framework replaces purely Wireless Village specific
* presence suppor controlled with __PRESENCE flag.
*/
#define __PRESENCE_FRAMEWORK
#define KFeatureIdPresenceFramework KOtherFeatureFirst+637

/*
* The new IM UI Application (called IM UI NG, NG = New Generation)
*/
#define __CHATNG
#define KFeatureIdChatNG KOtherFeatureFirst+650

/*
* Flag is used to incorporate MMS upload feature into the release.
*/
#undef __SENDUI_MMS_UPLOAD
#define KFeatureIdSenduiMmsUpload KOtherFeatureFirst+135

/*
* Flag is used ro incorporate Postcard application into the release.
*/
#undef __MMS_POSTCARD
#define KFeatureIdMmsPostcard KOtherFeatureFirst+509

/*
* Enables inclusion of custom http header on Mms Http Post and Get requests
* for subscriber identification.
*/
#undef __MMS_XID_HEADER_HTTP_FILTER
#define KFeatureIdMmsXidHeaderHttpFilter KOtherFeatureFirst+520

//-----------------------------------
//Messaging
//-----------------------------------
/*
* Flag is used to include always on PDP context plugin binaries to the
* build.
*/
#undef __ALWAYS_ONLINE_PDPCONTEXT
#define KFeatureIdAlwaysOnlinePDPContext KOtherFeatureFirst+144

/*
* Flag is used to include always on PDP context plugin binaries, version 2,
* to the build.
*/
#undef __ALWAYS_ONLINE_PDPCONTEXT2
#define KFeatureIdAlwaysOnlinePDPContext2 KOtherFeatureFirst+662

/*
* Flag for Xpress Audio Messaging feature. Device supports recording and
* sending a sound clip as a MMS message.
*/
#define __AUDIO_MESSAGING
#define KFeatureIdAudioMessaging KOtherFeatureFirst+565

/*
* The flag is used for image time variation of the OMA EMN watcher plugin
* that receives the incoming OMA email notifications. Additionally,
* it would be used for hiding the EMN functionality from the email settings.
*/
#define __OMA_EMAIL_NOTIFICATIONS
#define KFeatureIdOmaEmailNotifications KOtherFeatureFirst+633

/*
* Device supports data synchronization over HTTP.
*/
#define __SYNCML_DS_OVER_HTTP
#define KFeatureIdSyncMlDsOverHttp KOtherFeatureFirst+414

/*
* SyncML AIW provider provides menu items and commands for starting and
* editing the settings of synchronization directly from PIM applications.
*/
#define __SYNCML_DS_AIW_PROVIDER
#define KFeatureIdSyncMlDsAiwProvider KOtherFeatureFirst+516

/*
* Device supports configuring VoIP settings using SyncML.
*/
#define __SYNCML_DM_VOIP
#define KFeatureIdSyncMlDmVoIP KCommonFeatureFirst+58

/*
* Device supports configuring SIP settings using SyncML.
*/
#define __SYNCML_DM_SIP
#define KFeatureIdSyncMlDmSIP KCommonFeatureFirst+59

/*
* Feature flag for Sync and Provisioning/Embedded Link adapter
*/
#undef __SAP_EMBEDDED_LINK_ADAPTER
#define KFeatureIdSapEmbeddedLinkAdapter KOtherFeatureFirst+569

/*
* Feature flag for Sync and Provisioning/Idle Softkey adapter
*/
#undef __SAP_IDLE_SOFTKEY_ADAPTER
#define KFeatureIdSapIdleSoftkeyAdapter KOtherFeatureFirst+570

/*
* Feature flag for Sync and Provisioning/Operator logo adapter
*/
#undef __SAP_OPERATOR_LOGO_ADAPTER
#define KFeatureIdSapOperatorLogoAdapter KOtherFeatureFirst+571

/*
* Feature flag for Sync and Provisioning/Screensaver adapter
*/
#undef __SAP_SCREENSAVER_ADAPTER
#define KFeatureIdSapScreensaverAdapter KOtherFeatureFirst+572

/*
* Feature flag for Sync and Provisioning/Startup adapter
*/
#undef __SAP_STARTUP_ADAPTER
#define KFeatureIdSapStartupAdapter KOtherFeatureFirst+573

/*
* Feature flag for Sync and Provisioning/Themes adapter
*/
#undef __SAP_THEMES_ADAPTER
#define KFeatureIdSapThemesAdapter KOtherFeatureFirst+574

/*
* Feature flag for Sync and Provisioning/Wallpaper adapter
*/
#undef __SAP_WALLPAPER_ADAPTER
#define KFeatureIdSapWallpaperAdapter KOtherFeatureFirst+575

/*
* Feature flag for Sync and Provisioning/Application management
*/
#undef __SAP_APPLICATION_MANAGEMENT
#define KFeatureIdSapApplicationManagement KOtherFeatureFirst+576

/*
* Feature flag for Sync and Provisioning/Terminal control
*/
#undef __SAP_TERMINAL_CONTROL_FW
#define KFeatureIdSapTerminalControlFw KOtherFeatureFirst+577

/*
* Feature flag for Sync and Provisioning/Policy management
*/
#undef __SAP_POLICY_MANAGEMENT
#define KFeatureIdSapPolicyManagement KOtherFeatureFirst+578

/*
* Feature flag for Sync and Provisioning/UI settins server
*/
#undef __SAP_UI_SETTING_SERVER
#define KFeatureIdSapUiSettingServer KOtherFeatureFirst+579

/*
* Device supports SMS synchronisation using the SyncML.
*/
#define __SYNCML_DS_SMS
#define KFeatureIdSyncMlDsSms KOtherFeatureFirst+599

/*
* Feature flag for Sync and Provisioning/Device Lock Enhancements
*/
#undef __SAP_DEVICE_LOCK_ENHANCEMENTS
#define KFeatureIdSapDeviceLockEnhancements KOtherFeatureFirst+611

/*
* SVG-T viewer is included in the build.
*/
#define __SVGT_VIEWER
#define KFeatureIdSvgtViewer KOtherFeatureFirst+139

/*
* Device supports all-ARM AAC encoding capabilities.
*/
#define __AAC_ENCODER_PLUGIN
#define KFeatureIdAacEncoderPlugin KOtherFeatureFirst+141

/*
* Device supports all-ARM AAC+ and Enhanced AAC+ decoding capabilities
*/
#define __AAC_PLUS_DECODER_PLUGIN
#define KFeatureIdAacPlusDecoderPlugin KOtherFeatureFirst+143

/*
* Device supports equalizer.
*/
#define __EQUALIZER
#define KFeatureIdEqualizer KOtherFeatureFirst+502

/*
* Device supports Media Transfer Protocol.
*/
#define __MTP_PROTOCOL_SUPPORT
#define KFeatureIdMtpProtocolSupport KCommonFeatureFirst+503

/*
* Device supports H.264/MPEG4 AVC decoder
*
* Feature not supported, this flag must be always undefined. Do not edit this !
*/
#undef __AVC_DECODER
#define KFeatureIdAvcDecoder KOtherFeatureFirst+567

/*
* Device supports H.264/MPEG4 AVC encoder
*/
#undef __AVC_ENCODER
#define KFeatureIdAvcEncoder KOtherFeatureFirst+568

/*
* Device supports RTP.
*/
#define __RTP_STACK
#define KFeatureIdRtpStack KOtherFeatureFirst+589

/*
* Device supports Audio Controller Streaming feature.
*/
#define __AUDIO_CONTROLLER_STREAMING
#define KFeatureIdAudioControllerStreaming KOtherFeatureFirst+591

/*
* The flag allows to choose between built-in Display Post implementation or
* an external Display Post module.
*/
#undef __DISPLAY_POST
#define KFeatureIdDisplayPost KOtherFeatureFirst+610

/*
* This feature flag will enable/disable the ability of RealPlayer to
* playback AVC (H.264) video by including/excluding the AVC codec DLL and
* AVC Depacketizer DLL in the rom image.
*/
#define __ARM_AVC
#define KFeatureIdArmAvc KOtherFeatureFirst+630

/*
* Beatnik Audio engine is the standard, default engine in S60 platform. With
* this flag, it is possible to variate out Beatnik Audio Engine and uses
* another midi audio engines.
*/
#define __BEATNIK_AUDIOENGINE
#define KFeatureIdBeatnikAudioengine KOtherFeatureFirst+640

/*
* Support for MDF H264 decoder. This decoder is used by MediaPlayer via new
* helix engine and MDF. Excluded if hardware accelerated decoder is used
* instead.
*/
#define __ARM_MDF_H264_DEC
#define KFeatureIdArmMdfH264Dec KOtherFeatureFirst+642

/*
* Support for MDF Realvideo decoder. This decoder is used by MediaPlayer via
* new helix engine and MDF. Excluded if hardware accelerated decoder is used
* instead.
*/
#define __ARM_MDF_REALVIDEO_DEC
#define KFeatureIdArmMdfRealvideoDec KOtherFeatureFirst+643

/*
* Support for MDF H263 MPEG4 decoder. This decoder is used by MediaPlayer
* via new helix engine and MDF. Excluded if hardware accelerated decoder is
* used instead.
*/
#define __ARM_MDF_H263MPEG4_DEC
#define KFeatureIdArmMdfH263mpeg4Dec KOtherFeatureFirst+644

/*
* Support for MDF Post processor. Excluded if hardware accelerated
* post-processing is used instead.
*/
#define __ARM_MDF_POSTPROCESSOR
#define KFeatureIdArmMdfPostprocessor KOtherFeatureFirst+645

/*
* SVG-T ScreenSaver is a ECOM plugin DLL based on the Netscape plugin API.
* This is used by the screensaver application to support SVG Screensavers.
*/
#define __SVGT_SCREENSAVER_PLUGIN
#define KFeatureIdSvgtScreensaverPlugin KOtherFeatureFirst+647

/*
* Device supports Windows Media. In other words it indicates whether
* WM-related components such as ASF-parser and codecs are in place.
*/
#undef __WINDOWS_MEDIA
#define KFeatureIdWindowsMedia KOtherFeatureFirst+653

/*
* Device supports Windows Media DRM. In other words it indicates whether
* WMDRM related components such as WMDRM MTP plugin and WMDRM PK are in
* place.
*/
#undef __WINDOWS_MEDIA_DRM
#define KFeatureIdWindowsMediaDrm KOtherFeatureFirst+654

/*
* Multimedia Sharing application.
*/
#define __MULTIMEDIA_SHARING
#define KFeatureIdMultimediaSharing KOtherFeatureFirst+656

/*
* This flag is used when telephony service provides its functionality also
* to external subsystems.
*
* Feature not supported, this flag must be always undefined. Do not edit this !
*/
#undef __TELEPHONY_SERVICE
#define KFeatureIdTelephonyService KOtherFeatureFirst+137

/*
* Device supports showing an image, animated GIF or text for an incoming
* call.
*/
#define __CALL_IMAGETEXT
#define KFeatureIdCallImagetext KOtherFeatureFirst+503

/*
* This flag moves video call menus to upper layer for better visibility and
* usability.
*/
#undef __VIDEOCALL_MENU_VISIBILITY
#define KFeatureIdVideocallMenuVisibility KOtherFeatureFirst+519

/*
* This flag is used to control the existance of the OMA XDM feature
*/
#define __XDM
#define KFeatureIdXdm KOtherFeatureFirst+523

/*
* This flag is used to control the existance of the XCAP protocol
* implementation of XDM
*/
#define __XDM_XCAP
#define KFeatureIdXdmXcap KOtherFeatureFirst+524

/*
* This flag is used to control the existence of the Local Storage protocol
* implementation of XDM
*/
#define __XDM_LOCALSTORAGE
#define KFeatureIdXdmLocalStorage KOtherFeatureFirst+525

/*
* OMA Push-to-talk over Cellular.
*/
#define __OMA_POC
#define KFeatureIdOmaPoc KOtherFeatureFirst+538

/*
* When this flag is enabled and call control service is activated by the
* SIM, all dialled digit strings, supplementary service (SS) control strings
* and unstructured supplementary data (USSD) strings are first passed to the
* SIM before the ME sets up the call, the supplementary service operation or
* the USSD operation.
*/
#define __SAT_CALL_CONTROL
#define KFeatureIdSatCallControl KOtherFeatureFirst+541

/*
* This flag constitutes of five SAT commands: Open Channel, Close Channel,
* Send Data, Receive Data, Channel Status. They implement the "e" class of
* SAT commands and are related to Bearer Independent Protocol. When this
* flag is enabled, these SAT commands are supported.
*/
#define __SAT_BIP
#define KFeatureIdSatBip KOtherFeatureFirst+542

/*
* If this flag is enabled, SIM can request ME to display a text message,
* and/or an icon.
*/
#define __SAT_DISPLAY_TEXT
#define KFeatureIdSatDisplayText KOtherFeatureFirst+543

/*
* If this flag is enabled, SAT Get Inkey command instructs the ME to display
* text and/or an icon and to expect the user to enter a single character.
*/
#define __SAT_GET_INKEY
#define KFeatureIdSatGetInkey KOtherFeatureFirst+544

/*
* If this flag is enabled, SAT Get Input command instructs the ME to display
* text and/or an icon and that any response string entered by the user shall
* be passed transparently by the ME to the SIM and shall not be stored in
* the ME.
*/
#define __SAT_GET_INPUT
#define KFeatureIdSatGetInput KOtherFeatureFirst+545

/*
* If this flag is enabled, the SIM shall use SAT Language Notification
* command to notify the ME about the language currently used for any text
* string within proactive commands or envelope command responses.
*/
#define __SAT_LANGUAGE_NOTIFICATION
#define KFeatureIdSatLanguageNotification KOtherFeatureFirst+546

/*
* If this flag is enabled, upon receiving SAT Launch Browser command, the ME
* shall decide if it is able to execute the command. See details from 3GPP
* specifications.
*/
#define __SAT_LAUNCH_BROWSER
#define KFeatureIdSatLaunchBrowser KOtherFeatureFirst+547

/*
* When this flag is enabled, mobile originated short messages are controlled
* by SIM.
*/
#define __SAT_MO_SM_CONTROL
#define KFeatureIdSatMoSmControl KOtherFeatureFirst+548

/*
* When this flag is enabled, SIM can instruct the ME to play an audio tone.
*/
#define __SAT_PLAY_TONE
#define KFeatureIdSatPlayTone KOtherFeatureFirst+549

/*
* If this flag is enabled, SIM can request ME to provide current local
* information to the SIM.
*/
#define __SAT_PROVIDE_LOCAL_INFO
#define KFeatureIdSatProvideLocalInfo KOtherFeatureFirst+550

/*
* When this flag is enabled, clients of SAT Refresh API are enabled to be
* notified of the changes to the SIM configuration that have occurred as the
* result of a SIM application activity.
*/
#define __SAT_REFRESH
#define KFeatureIdSatRefresh KOtherFeatureFirst+551

/*
* If this flag is enabled, the SIM shall supply a set of items to the ME
* from which the user may choose one.
*/
#define __SAT_SELECT_ITEM
#define KFeatureIdSatSelectItem KOtherFeatureFirst+552

/*
* When this flag is enabled, SAT Send DTMF command requests the ME to send a
* Dual Tone Multiple Frequency (DTMF) string after a call has been
* successfully established either by the proactive command SET UP CALL or
* the user.
*/
#define __SAT_SEND_DTMF
#define KFeatureIdSatSendDtfm KOtherFeatureFirst+553

/*
* When this flag is enabled, SMS commands may be sent by the SIM. See
* details from 3GPP specification.
*/
#define __SAT_SEND_SM
#define KFeatureIdSatSendSm KOtherFeatureFirst+554

/*
* When this flag is enabled and SIM requests ME to send supplementary
* service (SS) command, the ME shall decide if it is able to execute the
* command. See details from 3GPP specification.
*/
#define __SAT_SEND_SS
#define KFeatureIdSatSendSs KOtherFeatureFirst+555

/*
* When this flag is enabled and SIM requests ME to send unstructured
* supplementary service data (USSD), the ME shall decide if it is able to
* execute the command. See details from 3GPP specification.
*/
#define __SAT_SEND_USSD
#define KFeatureIdSatSendUssd KOtherFeatureFirst+556

/*
* When this flag is enabled and SIM requests ME to set up a call, the ME
* shall decide if it able to execute the command.
*/
#define __SAT_SETUP_CALL
#define KFeatureIdSatSetupCall KOtherFeatureFirst+557

/*
* If this flag is enabled, the SIM shall supply a set of events.
*/
#define __SAT_SET_UP_EVENT_LIST
#define KFeatureIdSatSetUpEventList KOtherFeatureFirst+558

/*
* If this flag is enabled, the SIM shall supply a text string, which shall
* be displayed by the ME as an idle mode text if the ME is able to do it.
*/
#define __SAT_SET_UP_IDLE_MODE_TEXT
#define KFeatureIdSatSetUpIdleModeText KOtherFeatureFirst+559

/*
* When this flag is enabled, the SIM shall supply a set of menu items, which
* shall be integrated with the menu system in order to give the user the
* opportunity to choose one of these menu items at his own discretion.
*/
#define __SAT_SET_UP_MENU
#define KFeatureIdSatSetUpMenu KOtherFeatureFirst+560

/*
* Device has component that performs integrity check of SWI certificate
* store in c: drive during boot.
*/
#define __BTIC_ENABLED
#define KFeatureIdBticEnabled KOtherFeatureFirst+600

/*
* In addition to the SWI certificate store check (defined by
* __BTIC_ENABLED), also binaries (having TCB or DRM capability) in c: drive
* are integrity checked during boot.
*/
#undef __BTIC_BINARIES_CHECK_ENABLED
#define KFeatureIdBticBinariesCheckEnabled KOtherFeatureFirst+601

/*
* Enables UPIN functionality.
*/
#define __UPIN
#define KFeatureIdUpin KOtherFeatureFirst+612

/*
* Device supports remote locking.
*/
#define __REMOTE_LOCK
#define KFeatureIdRemoteLock KOtherFeatureFirst+652

/*
* Device supports IP Push feature.
*/
#undef __IP_PUSH
#define KFeatureIdIpPush KOtherFeatureFirst+409

/*
* This feature enables controlling and accessing other deveices via UPnP
* protocol.
*/
#define __UPNP_STACK
#define KFeatureIdUpnpStack KOtherFeatureFirst+528

/*
* WLAN hardware supports 256 bit WEP encryption
*/
#define __WLAN_WEP256_ENABLED
#define KFeatureIdWlanWep256Enabled KOtherFeatureFirst+530

/*
* Flag enables support of Media Server in UPnP stack.
*/
#define __UPNP_MEDIASERVER
#define KFeatureIdUpnpMediaserver KOtherFeatureFirst+661

/*
* Flag enables support of Audio&Video in UPnP stack.
*/
#define __UPNP_AVCP
#define KFeatureIdUpnpAvcp KOtherFeatureFirst+533

/*
* Flag enables support of printing in UPnP stack.
*/
#define __UPNP_PRINT_FRAMEWORK
#define KFeatureIdUpnpPrintFramework KOtherFeatureFirst+535

/*
* Flag that enables support of remotestorage support and mapping of drives.
*/
#undef __UPNP_REMOTE_STORAGE
#define KFeatureIdUpnpRemoteStorage KOtherFeatureFirst+536

/*
* Flag enable RemoteStorage feature, access to shared file systems like file
* shared and web servers.
*/
#undef __REMOTE_STORAGE_FW
#define KFeatureIdRemoteStorageFw KOtherFeatureFirst+581

/*
* This flag is used to control the existance of SIP/SIMPLE feature in S60.
*/
#define __SIP_SIMPLE_PRESENCE_PROTOCOL
#define KFeatureIdSipSimplePresenceProtocol KOtherFeatureFirst+635

/*
* When the feature flag is set, HSDPA setting item is visible for the user.
*/
#undef __HSXPA_SUPPORT
#define KFeatureIdHsxpaSupport KOtherFeatureFirst+666

/*
* Device has a location verifier module.
*/
#undef __LOCATIONVERIFIER
#define KFeatureIdLocationVerifier KOtherFeatureFirst+136

/*
* Device has internal GPS hardware.
*/
#undef __LOCATIONGPSHW
#define KFeatureIdLocationGpsHw KOtherFeatureFirst+138

/*
* Device has basic location info display.
*/
#define __BASIC_LOCATION_INFO_DISPLAY
#define KFeatureIdBasicLocationInfoDisplay KOtherFeatureFirst+513

/*
* Device has Secure User Plane Location (SUPL) Framework.
*/
#define __SUPL_FRAMEWORK
#define KFeatureIdSuplFramework KOtherFeatureFirst+583

/*
* Device has OMA SUPL variant of SUPL Protocol Plug-in for Common SUPL
* Framework.
*/
#define __OMA_SUPL_PLUGINS
#define KFeatureIdOmaSuplPlugins KOtherFeatureFirst+584

/*
* Support for network based positioning methods. All PSYs that implement
* network based positioning technology shall be hidden behind Network
* Positioning Proxy.
*/
#define __NP_PROXY
#define KFeatureIdNpProxy KOtherFeatureFirst+598

/*
* This flag is intended to toggle presence of Map and Navigation AIW
* provider in ROM.
*/
#define __MAP_AND_NAVIGATION_AIW_PROVIDER
#define KFeatureIdMapAndNavigationAiwProvider KOtherFeatureFirst+602

/*
* Flag enables full screen mode in camera application. Full screen is
* supported only in landscape mode.
* If hardware is not supporting landscape mode this flag should be set off.
*/
#undef __CAMERA_FULLSCREEN_VIEWFINDER
#define KFeatureIdCameraFullscreenViewfinder KOtherFeatureFirst+607

/*
* Device has Java MIDP2.0.
*/
#define __JAVA_MIDP20
#define KFeatureIdJavaMIDP20 KOtherFeatureFirst+413

/*
* Device supports JSR 205, WMA 2.0 specification.
*/
#define __JAVA_JSR205_WMA_2_0_SUPPORT
#define KFeatureIdJavaJsr205Wma20Support KOtherFeatureFirst+415

/*
* Device supports JSR 234, Advanced Multimedia Supplements
*/
#define __JAVA_JSR_234_3D_AUDIO_AND_MUSIC_CAPABILITIES
#define KFeatureIdJavaJsr2343DAudioAndMusicCapabilities KOtherFeatureFirst+416

/*
* Device supports JSR 180, SIP API for J2ME
*/
#define __JAVA_JSR_180_SIP_API
#define KFeatureIdJavaJsr180SipAPI KOtherFeatureFirst+417

/*
* Device supports JSR 226, Scalable 2D Vector Graphics API for J2ME
*/
#define __JAVA_JSR_226_2D_SVG_API
#define KFeatureIdJavaJsr2262DSvgAPI KOtherFeatureFirst+418

/*
* Device supports JSR 177, Security and Trust Services API for J2ME
*/
#define __JAVA_JSR_177_SECURITY_AND_TRUST_SERVICES
#define KFeatureIdJavaJsr177SecurityAndTrustServices KOtherFeatureFirst+419

/*
* Support  for VSCL 2.0 specifications. VSCL 2.0 specification includes the
* following functions:
*    - Bar Code
*    - Device Control Support
*    - Listener Functions
*    - Low Level Infrared API
*    - SVG Support
*    - Save Picture Feature
*    - Resident MIDlet support
*/
#undef __JAVA_VSCL
#define KFeatureIdJavaVscl KOtherFeatureFirst+562

/*
* Flag enables full Java Bar Code API support. This feature requires camera
* lens hardware that supports macro mode and autofocus, and is capable of
* decent close-up images.
*/
#undef __JAVA_BAR_CODE_FULL
#define KFeatureIdJavaBarCodeFull KOtherFeatureFirst+563

/*
* Flag enables the optional APDU part of Java Adaptation of the Security and
* Trust Services API JSR 177 implementation.
*/
#define __JAVA_JSR177_SECURITY_AND_TRUST_SERVICES_APDU
#define KFeatureIdJavaJsr177SecurityAndTrustServicesApdu KOtherFeatureFirst+585

/*
* Flag enables the optional PKI part of Java Adaptation of the Security and
* Trust Services API JSR 177 implementation.
*/
#define __JAVA_JSR177_SECURITY_AND_TRUST_SERVICES_PKI
#define KFeatureIdJavaJsr177SecurityAndTrustServicesPki KOtherFeatureFirst+586

/*
* Flag enables the optional Crypto part of Java Adaptation of the Security
* and Trust Services API JSR 177 implementation.
*/
#define __JAVA_JSR177_SECURITY_AND_TRUST_SERVICES_CRYPTO
#define KFeatureIdJavaJsr177SecurityAndTrustServicesCrypto KOtherFeatureFirst+587

/*
* Support for Embedded Standard Widget Toolkit.
*/
#undef __JAVA_ESWT
#define KFeatureIdJavaESWT KOtherFeatureFirst+664

/*
* Device supports Feeds (RSS) functionality.
*/
#define __RSS_FEEDS
#define KFeatureIdRssFeeds KCommonFeatureFirst+166

/*
* Device includes standard Series 60 browser.
*/
#define __SERIES60_NATIVE_BROWSER
#define KFeatureIdSeries60NativeBrowser KCommonFeatureFirst+167

/*
* Support for Browser Plugin. Used in deciding whether the browser video
* plugin is taken in.
*/
#define __BROWSER_VIDEO_PLUGIN
#define KFeatureIdBrowserVideoPlugin KOtherFeatureFirst+606

/*
* Support for Video services application. Used in deciding whether the video
* services application  is taken in.
*/
#define __VIDEO_MENU
#define KFeatureIdVideoMenu KOtherFeatureFirst+634

//-----------------------------------
//Misc
//-----------------------------------
/*
* Device application UIs use Europe Look And Feel (LAF).
*/
#define __AVKON_ELAF__
#define KFeatureIdAvkonELaf KOtherFeatureFirst+10

/*
* Device application UIs use Asia Pacific Look And Feel (LAF).
*/
#undef __AVKON_APAC__
#define KFeatureIdAvkonApac KOtherFeatureFirst+15

/*
* Device supports Musical Instrument Digital Interface (MIDI) sounds.
*/
#define __SERIES60_MIDI
#define KFeatureIdMidi KOtherFeatureFirst+11

/*
* Device support context helps in applications.
*/
#define __SERIES60_HELP
#define KFeatureIdHelp KOtherFeatureFirst+12

/*
* Device does not have a keyboard slider to activate keyboard.
*/
#define __SERIES60_KEYPAD_NO_SLIDER
#define KFeatureIdKeypadNoSlider KOtherFeatureFirst+13

/*
* Device does not have a separate voice key to activate voice command
* functionality.
*/
#undef __SERIES60_KEYPAD_NO_VOICE_KEY
#define KFeatureIdKeypadNoVoiceKey KOtherFeatureFirst+14

/*
* Device has Ambient Light Sensor feature.
*/
#define __SERIES60_AMBIENT_LIGHT_SENSOR
#define KFeatureIdAmbientLightSensor KOtherFeatureFirst+529

/*
* Calendar application uses Lunar calendar. Used in Asia Pacific (APAC)
* area.
*/
#define __SERIES60_LUNAR_CALENDAR
#define KFeatureIdLunarCalendar KOtherFeatureFirst+17

/*
* Device supports Calling Name Presentation (CNAP) as defined in GSM 2.96. B
* subscriber is able to see A subscriber's number and name even the caller's
* ID is not stored in the phone. The name of the subscriber comes from
* network.
*/
#undef __SERIES60_PHONE_CNAP
#define KFeatureIdPhoneCnap KOtherFeatureFirst+31

/*
* Device supports Tele Type (TTY) functionality.  TTY is also referred to as
* TDD (Telecommunication Device for the Deaf). Applicable to devices
* targeted to United States (US) markets.
*/
#define __SERIES60_PHONE_TTY
#define KFeatureIdPhoneTty KOtherFeatureFirst+32

/*
* Phone application supports 2 digit call number for dialing customer
* service number. Applicable to devices targeted to United States (US)
* markets
*/
#undef __SERIES60_PHONE_2DIGIT_DIAL
#define KFeatureIdPhone2DigitDial KOtherFeatureFirst+33

/*
* Device has Real One Player application available
*/
#define __SERIES60_REAL_PLAYER
#define KFeatureIdRealPlayer KOtherFeatureFirst+40

/*
* Devices protects certain SW settings, like Internet access points.
* Operators can preset the phones already in the factory so that later user
* is not able to modify settings.
*/
#define __SERIES60_SETTINGS_PROTECTION
#define KFeatureIdSettingsProtection KOtherFeatureFirst+50

/*
* Device does NOT support old OTA configuration which has been replaced by
* new OMA Provisioning.  To keep compatibility with old mechanism you should
* set this off  (#undef).
*/
#undef __NO_OTA_CONFIGURATION
#define KFeatureIdNoOtaConfig KOtherFeatureFirst+51

/*
* Device supports WAP Push Service Loading (SL). When receiving the SL
* message the terminal will automatically load content to client without
* user confirmation. The SL together with SI (Service Indication) offer
* standard way of receiving notifications of services in the Internet e.g
* news.
*/
#define __SERIES60_PUSH_SL
#define KFeatureIdPushSL KOtherFeatureFirst+54

/*
* Device support WAP Simple Push (SP).  The SP is a standard way of pushing
* content into device e.g ringing tones.
*/
#undef __SERIES60_PUSH_SP
#define KFeatureIdPushSP KOtherFeatureFirst+55

/*
* Profiles application supports user to add new / delete old profiles.
*/
#define __DYNAMIC_PROFILES
#define KFeatureIdDynamicProfiles KOtherFeatureFirst+56

/*
* Device boot framework supports starting also 3rd party applications upon
* the boot. By default only native applications can be started.
*/
#define __EXTENDED_STARTUP
#define KFeatureIdExtendedStartup KOtherFeatureFirst+57

/*
* Device contains Operator menu application.  It is a wrapper to Browser
* application and allows using operator specific application icon (and
* label), and allows opening wanted URL initially.
*/
#define __OPERATOR_MENU
#define KFeatureIdOperatorMenu KOtherFeatureFirst+58

/*
* Device supports Multiple OMA Provisioning contexts. The feature allows the
* user to choose which configuration context is currently "active" in order
* to improve usability by reducing the number of detailed connectivity
* decisions and processes involved with utilizing services.
*/
#define __MULTIPLE_PROV_CTX
#define KFeatureIdMultipleProvCtx KOtherFeatureFirst+59

/*
* Browser application supports Narrow screen rendering. That enables user to
* read HTML content more easily without a need to scroll horizontally.
*/
#define __BROWSER_NARROW_SCREEN
#define KFeatureIdBrowserNarrowScreen KOtherFeatureFirst+60

/*
* Application installer accepts only installation of digitally signed SW 
* (having corresponding certificate installed on terminal). See dependencies
* to flag __INSTALL_SECURITY_UI.
*/
#undef __INSTALL_SECURITY
#define KFeatureIdInstallSecurity KOtherFeatureFirst+61

/*
* Deprecated feature flag for Advanced Audio Coding (AAC) codec. Use __AAC 
* feature instead.
*/
#define __AUDIO_AAC
#define KFeatureIdAudioAac KOtherFeatureFirst+62

/*
* Media Gallery & Player applications support audio file playlist (M3U media
* queue format).
*/
#define __AUDIO_PLAYLIST
#define KFeatureIdAudioPlaylist KOtherFeatureFirst+63

/*
* Browser application supports more detailed information of download
* progress (in addition to "spinning globe")
*/
#define __BROWSER_PROGRESS_IND
#define KFeatureIdBrowserProgressInd KOtherFeatureFirst+64

/*
* Browser application supports expanding the amount of screen space used for
* browser display.
*/
#define __BROWSER_FULLSCREEN
#define KFeatureIdBrowserFullScr KOtherFeatureFirst+66

/*
* Browser aplication support HTML <frame> tags.
*/
#define __BROWSER_FRAMES
#define KFeatureIdBrowserFrames KOtherFeatureFirst+69

/*
* Browser application supports persistent cache in addition to default
* volatile cache.  Contents of this cache will remain from one browser
* session to the next (also through power cycles of the phone.)
*/
#define __OPERATOR_CACHE
#define KFeatureIdOperatorCache KOtherFeatureFirst+71

/*
* General settings application supports controlling display brightness.
*/
#undef __BRIGHTNESS_CONTROL
#define KFeatureIdBrightnessControl KOtherFeatureFirst+72

/*
* MMS editor supports slide set creation (MMS Conformant Document version
* 2.0.0 [2]). That allows end user to create a ?slide show? as a Multimedia
* Message (MM) using a slide template.
*/
#define __SMIL_EDITOR
#define KFeatureIdSmilEditor KOtherFeatureFirst+73

/*
* Device support seamless links, i.e. application offer direct browser links
* to download services applicable to the application.
*/
#define __SEAMLESS_LINKS
#define KFeatureIdSeamlessLinks KOtherFeatureFirst+74

/*
* Device shows SW panic note when an application panic (unexpected error)
* occurs. Disabling this feature in a final product is recommended.
*/
#define __SHOW_PANICS
#define KFeatureIdShowPanics KOtherFeatureFirst+75

/*
* Device supports MMC hotswap. A MMC card can be inserted and removed from
* device without removing battery or rebooting the device
*/
#define __MMC_HOTSWAP
#define KFeatureIdMmcHotswap KOtherFeatureFirst+76

/*
* Devices supports Always On-line framework which enables various
* always-online plug-ins, e.g. Email.
*/
#define __ALWAYS_ONLINE
#define KFeatureIdAlwaysOnLine KOtherFeatureFirst+78

/*
* Device supports Japanese pictograhps
*/
#undef __JAPANESE_PICTOGRAPHS
#define KFeatureIdJapanesePicto KOtherFeatureFirst+79

/*
* Device uses Japanese language variant.
*/
#undef __JAPANESE
#define KFeatureIdJapanese KOtherFeatureFirst+80

/*
* Device uses Thai language variant.
*/
#undef __THAI
#define KFeatureIdThai KOtherFeatureFirst+81

/*
* HTTP digest authentication
*/
#define __HTTP_DIGEST_AUTH
#define KFeatureIdHttpDigestAuth KOtherFeatureFirst+84

/*
* Device supports Image Upload feature.
*
* Feature not supported, this flag must be always undefined. Do not edit this !
*/
#undef __IMAGE_UPLOAD
#define KFeatureIdImageUpload KOtherFeatureFirst+86

/*
* Device supports sending a file to active call number.
*/
#define __SEND_FILE_IN_CALL
#define KFeatureIdSendFileInCall KOtherFeatureFirst+87

/*
* Device application Uis support IPV6.
*/
#define __IPV6
#define KFeatureIdIPv6 KOtherFeatureFirst+88

/*
* Device uses only "simple" logs (call logs only)
*/
#undef __SIMPLE_LOGS
#define KFeatureIdSimpleLogs KOtherFeatureFirst+89

/*
* Device supports Cell Broadcast feature (CBS).
*/
#define __CELL_BROADCAST
#define KFeatureIdCellBroadcast KOtherFeatureFirst+90

/*
* Device supports Unstructured Suppelementary Service Data (USSB).
*/
#define __USSD
#define KFeatureIdUSSD KOtherFeatureFirst+91

/*
* Device supports sending email messages using SMS as the bearer transport.
*/
#undef __EMAIL_OVER_SMS
#define KFeatureIdEmailOverSms KOtherFeatureFirst+92

/*
* Device supports RealVideo9.
*/
#define __RV9
#define KFeatureIdRV9 KOtherFeatureFirst+94

/*
* Device uses Chinese language variant.
*/
#undef __CHINESE
#define KFeatureIdChinese KOtherFeatureFirst+96

/*
* Clock application supports World clock and City/country views
*/
#define __WORLD_CLOCK
#define KFeatureIdWorldClock KOtherFeatureFirst+98

/*
* Browser application supports posting a file from the file system to Web
* server, in addition to "normal" user input.
*/
#define __BROWSER_FILE_UPLOAD
#define KFeatureIdBrowserFileUpload KOtherFeatureFirst+99

/*
* Device supports keeping mailbox always connected and up to date.
*/
#define __ALWAYS_ONLINE_EMAIL
#define KFeatureIdAlwaysOnLineEmail KOtherFeatureFirst+101

/*
* Browser application supports Netscape plug-in API.
*/
#define __BROWSER_NETSCAPE_API
#define KFeatureIdBrowserNetscapeAPI KOtherFeatureFirst+103

/*
* Device supports Install security UI.
* Dependencies:
* INSTALL_SECURITY  "ON"  -> allowed values for __INSTALL_SECURITY_UI are as
* follows:
*   "\0"  : forced OFF, means install security is forced,  so no UI and user
* cannot control security.
* INSTALL_SECURITY  "OFF"  -> allowed values for __INSTALL_SECURITY_UI are
* as follows:
*   "0" : OFF, means no install security whatsoever, and no user control.
*   "1" : ON, means user has an UI that he can use to control install
* security.
*/
#define __INSTALL_SECURITY_UI
#define KFeatureIdInstallSecurityUI KOtherFeatureFirst+104

/*
* Device supports connection monitoring UI.
*/
#define __CONNMON_UI
#define KFeatureIdConnMonUI KOtherFeatureFirst+105

/*
* Device supports the specified fine-tuning of Smart Messaging over SMS.
*/
#define __SMARTMSG_SMS_BOOKMARK_RECEIVING
#define KFeatureIdSmartmsgSMSBookmarkReceiving KOtherFeatureFirst+106

/*
* Device supports the specified fine-tuning of Smart Messaging over SMS.
*/
#undef __SMARTMSG_SMS_WAP_AP_RECEIVING
#define KFeatureIdSmartmsgSMSWapApReceiving KOtherFeatureFirst+107

/*
* Device supports the specified fine-tuning of Smart Messaging over SMS.
*/
#undef __SMARTMSG_SMS_IAP_SETTINGS_RECEIVING
#define KFeatureIdSmartmsgSMSIapSettingsReceiving KOtherFeatureFirst+108

/*
* Device supports the specified fine-tuning of Smart Messaging over SMS.
*/
#undef __SMARTMSG_SMS_WV_SETTINGS_RECEIVING
#define KFeatureIdSmartmsgSMSWvSettingsReceiving KOtherFeatureFirst+109

/*
* Device supports the specified fine-tuning of Smart Messaging over SMS.
*/
#define __SMARTMSG_SMS_OPERATOR_LOGO_RECEIVING
#define KFeatureIdSmartmsgSMSOperatorLogoReceiving KOtherFeatureFirst+110

/*
* Device supports the specified fine-tuning of Smart Messaging over SMS.
*/
#define __SMARTMSG_SMS_RINGING_TONE_RECEIVING
#define KFeatureIdSmartmsgSMSRingingToneReceiving KOtherFeatureFirst+111

/*
* Device supports the specified fine-tuning of Smart Messaging over SMS.
*/
#define __SMARTMSG_SMS_GMS_MESSAGE_RECEIVING
#define KFeatureIdSmartmsgSMSGmsMessageReceiving KOtherFeatureFirst+112

/*
* Device supports the specified fine-tuning of Smart Messaging over SMS.
*/
#undef __SMARTMSG_SMS_GMS_MESSAGE_SENDING_SUPPORTED 
#define KFeatureIdSmartmsgSMSGmsMessageSendingSupported KOtherFeatureFirst+113

/*
* Device supports the specified fine-tuning of Smart Messaging over SMS.
*/
#define __SMARTMSG_SMS_VCAL_RECEIVING
#define KFeatureIdSmartmsgSMSVcalReceiving KOtherFeatureFirst+114

/*
* Device supports the specified fine-tuning of Smart Messaging over SMS.
*/
#define __SMARTMSG_SMS_VCARD_RECEIVING
#define KFeatureIdSmartmsgSMSVcardReceiving KOtherFeatureFirst+115

/*
* Device supports the specified fine-tuning of Smart Messaging over SMS.
*/
#define __SMARTMSG_SMS_VCAL_SENDING
#define KFeatureIdSmartmsgSMSVcalSending KOtherFeatureFirst+116

/*
* Device supports the specified fine-tuning of Smart Messaging over SMS.
*/
#define __SMARTMSG_SMS_VCARD_SENDING
#define KFeatureIdSmartmsgSMSVcardSending KOtherFeatureFirst+117

/*
* ENPolicy provides emergency number policy APIs and is used by phoneserver
* component.
* DOS emergency number policy checks emergency number by using ETel custom
* API.
* SOS emergency number policy checks emergency number by using ETel
* multimode API and System agent.
*/
#define __EN_POLICY_DOS
#define KFeatureIdEnPolicyDos KOtherFeatureFirst+118

/*
* The Active Idle includes several plugins to display different content.
* Additional feature flags for them will be requested separately as the
* necessity for them to be optional arises.
* At the moment this flag will cover all Active Idle mandatory features.
*/
#define __ACTIVE_IDLE
#define KFeatureIdActiveIdle KOtherFeatureFirst+119

/*
* The flag tells whether the palette index address is defined with #define
* in palette.cpp or calculated dynamically in run-time, which is slower.
*/
#undef __PALETTE_INDEX_ADDRESS_FIXED
#define KFeatureIdPaletteIndexAddressFixed KOtherFeatureFirst+120

/*
* Media player supports Channel Listing Mode.
*
* Channel Listing  is a method of content presentation. Content will be
* displayed as a list of channels the user can choose from. The device will
* make a request for the channel listing each time the multimedia
* application is invoked.
*
* Feature not supported, this flag must be always undefined. Do not edit this !
*/
#undef __CDMA_CHANNEL_LISTING
#define KFeatureIdCdmaChannelListing KOtherFeatureFirst+121

/*
* Support for Browser Plugin. Used in deciding whether the browser audio
* pugin is taken into builds.
*/
#define __BROWSER_AUDIO_PLUGIN
#define KFeatureIdBrowserAudioPlugin KOtherFeatureFirst+122

/*
* Device supports 176x208 resolution
*
* Feature not supported, this flag must be always undefined. Do not edit this !
*/
#undef __LAYOUT176_208
#define KFeatureIdLayout176_208 KOtherFeatureFirst+123

/*
* Device supports 208x176 resolution
*
* Feature not supported, this flag must be always undefined. Do not edit this !
*/
#undef __LAYOUT208_176
#define KFeatureIdLayout208_176 KOtherFeatureFirst+582

/*
* Device supports 208x208 resolution (square)
*/
#undef __LAYOUT208_208
#define KFeatureIdLayout208_208 KOtherFeatureFirst+124

/*
* Device supports 240x320 resolution (QVGA)
*/
#define __LAYOUT_240_320
#define KFeatureIdLayout240_320 KOtherFeatureFirst+125

/*
* Device supports 320x240 resolution (QVGA landscape)
*/
#define __LAYOUT_320_240
#define KFeatureIdLayout320_240 KOtherFeatureFirst+126

/*
* Device supports 352x416 resolution (double)
*
* Feature not supported, this flag must be always undefined. Do not edit this !
*/
#undef __LAYOUT_352_416
#define KFeatureIdLayout352_416 KOtherFeatureFirst+127

/*
* Device supports 416x352 resolution (double landscape)
*
* Feature not supported, this flag must be always undefined. Do not edit this !
*/
#undef __LAYOUT_416_352
#define KFeatureIdLayout416_352 KOtherFeatureFirst+128

/*
* Device supports 480x640 resolution (VGA portrait)
*/
#undef __LAYOUT_480_640
#define KFeatureIdLayout480_640 KOtherFeatureFirst+615

/*
* Device supports 640x480 resolution (VGA landscape)
*/
#undef __LAYOUT_640_480
#define KFeatureIdLayout640_480 KOtherFeatureFirst+616

/*
* Device supports 320x480 resolution (HVGA portrait)
*/
#undef __LAYOUT_320_480
#define KFeatureIdLayout320_480 KOtherFeatureFirst+617

/*
* Device supports 480x320 resolution (HVGA landscape)
*/
#undef __LAYOUT_480_320
#define KFeatureIdLayout480_320 KOtherFeatureFirst+618

/*
* Device supports 800x352 resolution (WVGA landscape)
*/
#undef __LAYOUT_800_352
#define KFeatureIdLayout800_352 KOtherFeatureFirst+619

/*
* Device supports 352x800 resolution (WVGA portrait)
*/
#undef __LAYOUT_352_800
#define KFeatureIdLayout352_800 KOtherFeatureFirst+620

/*
* Device supports 240x320 resolution (QVGA2 for larger screens, portrait)
*/
#define __LAYOUT_240_320_LARGE_SCREEN
#define KFeatureIdLayout240_320_LargeScreen KOtherFeatureFirst+621

/*
* Device supports 320x240 resolution (QVGA2 for larger screens, landscape)
*/
#define __LAYOUT_320_240_LARGE_SCREEN
#define KFeatureIdLayout320_240_LargeScreen KOtherFeatureFirst+622

/*
* Device supports 480x640 resolution (VGA portrait, touch screen)
*/
#undef __LAYOUT_480_640_TOUCH
#define KFeatureIdLayout480_640_Touch KOtherFeatureFirst+623

/*
* Device supports 640x480 resolution (VGA landscape, touch screen)
*/
#undef __LAYOUT_640_480_TOUCH
#define KFeatureIdLayout640_480_Touch KOtherFeatureFirst+624

/*
* Device supports 240x320 resolution (QVGA, touch screen)
*/
#undef __LAYOUT_240_320_TOUCH
#define KFeatureIdLayout240_320_Touch KOtherFeatureFirst+625

/*
* Device supports 320x240 resolution (QVGA landscape, touch screen)
*/
#undef __LAYOUT_320_240_TOUCH
#define KFeatureIdLayout320_240_Touch KOtherFeatureFirst+626

/*
* Device supports 320x480 resolution (HVGA portrait, touch screen)
*/
#undef __LAYOUT_320_480_TOUCH
#define KFeatureIdLayout320_480_Touch KOtherFeatureFirst+627

/*
* Device supports 480x320 resolution (HVGA landscape, touch screen)
*/
#undef __LAYOUT_480_320_TOUCH
#define KFeatureIdLayout480_320_Touch KOtherFeatureFirst+628

/*
* Flag defines whether icons are taken from scalable icons directory or from
* bitmap icon directory. In a 176*208 device it is better to use bitmap
* icons instead of SVGT icons, for both performance and memory consumption
* reasons.
* And also, avkon's bitmap icons are still needed in release 2.8 for
* compatibility mode. (SDK applications may have loaded them directly via
* CFbsBitmap::Load).
*/
#define __SCALABLE_ICONS
#define KFeatureIdScalableIcons KOtherFeatureFirst+129

/*
* Java implementation supports advanced features of Java Mobile Media API
* (JSR135) version 1.1, implemented in release 2.6 onwards. This flag must
* always be enabled when __JAVA_MMAPI11 is enabled.
*/
#define JSR_135_SUPPORT
#define KFeatureIdJsr135Support KOtherFeatureFirst+130

/*
* International call prefix feature for Japan to make it easier for end
* users to handle complicated Japanese international call prefixes.
*/
#undef __JAPAN_PREFIX_CHANGE
#define KFeatureIdJapanPrefixChange KOtherFeatureFirst+131

/*
* MMBox (MMS Notifications) View can be opened from the message centre. It
* shows the multimedia messages stored in the MMS Center as a MMS
* notifications.
*/
#undef __MMS_NOTIFICATIONS_VIEW
#define KFeatureIdMMSNotificationsView KOtherFeatureFirst+132

/*
* Device has PRC China variant. This feature flag should be defined only if
* __CHINESE feature flag is defined.
*/
#undef __CHINESE_PRC_FONTS
#define KFeatureIdChinesePrcFonts KOtherFeatureFirst+133

/*
* Device has Taiwan and/or Hong Kong China variant. This feature flag should
* be defined only if __CHINESE feature flag is defined.
*/
#undef __CHINESE_TAIWAN_HK_FONTS
#define KFeatureIdChineseTaiwanHkFonts KOtherFeatureFirst+134

/*
* Browser uses OSS WebEngine.
*/
#define __BROWSER_OSS_ENGINE
#define KFeatureIdBrowserOssEngine KOtherFeatureFirst+142

/*
* Device has email UI components.
*/
#define __EMAIL_UI
#define KFeatureIdEmailUi KOtherFeatureFirst+410

/*
* Device supports native Symbian OS installation packages.
*/
#define __INSTALLER_SISX
#define KFeatureIdInstallerSisx KOtherFeatureFirst+411

/*
* This flag enables drive mode profile. The profile is silent and
* unmodifiable. In this profile the phone refuses to receive calls.
*/
#undef __DRIVE_MODE
#define KFeatureIdDriveMode KOtherFeatureFirst+412

/*
* Applications are not allowed to be started from MMC, when this flag is
* enabled.
*/
#undef __EXE_PROTECTION
#define KFeatureIdExeProtection KOtherFeatureFirst+499

/*
* Activates alternative grouping of Japanese pictographs. This feature is
* effective only if __JAPANESE_PICTOGRAPHS is also defined.
*/
#undef __JAPANESE_PICTOGRAPHS_GROUPING
#define KFeatureIdJapanesePictographsGrouping KOtherFeatureFirst+500

/*
* Device supports user-configurable USSD menu.
*/
#undef __USER_CONFIGURABLE_USSD_MENU
#define KFeatureIdUserConfigurableUssdMenu KOtherFeatureFirst+501

/*
* Device supports OMA content download.
*/
#define __CONTENT_DOWNLOAD
#define KFeatureIdContentDownload KOtherFeatureFirst+504

/*
* Device has restricted voice mail functionality (no voice mail number
* setting).
*/
#undef __RESTRICTED_VOICE_MAIL
#define KFeatureIdRestrictedVoiceMail KOtherFeatureFirst+505

/*
* Device prevents transferring DRM protected content out of the phone.
*/
#undef __KEEP_DRM_CONTENT_ON_PHONE
#define KFeatureIdKeepDRMContentOnPhone KOtherFeatureFirst+506

/*
* Device prevents transferring CommDb outside of the phone.
*/
#undef __COMMDB_PROTECTION
#define KFeatureIdCommDBProtection KOtherFeatureFirst+507

/*
* Email and calendar support meeting request.
*/
#undef __MEETING_REQUEST_SUPPORT
#define KFeatureIdMeetingRequestSupport KOtherFeatureFirst+508

/*
* 3D Menu feature enhances Application Shell with animating 3D icons.
*/
#define __3D_MENU
#define KFeatureId3DMenu KOtherFeatureFirst+511

/*
* Device supports bearer management for seamless application level roaming.
*/
#define __BEARER_MGNT
#define  KFeatureIdBearerMgnt KOtherFeatureFirst+512

/*
* Device supports Cisco Compatible eXtensions in WLAN settings.
*/
#undef __WLAN_CCX
#define KFeatureIdWlanCcx KOtherFeatureFirst+515

/*
* Enlarged Japanese library for predictive text entry. This feature has no
* effect if the feature __JAPANESE is not defined.
*/
#define __JAPANESE_LARGER_DICTIONARY
#define KFeatureIdJapaneseLargerDictionary KOtherFeatureFirst+517

/*
* This flag is used to indicate that the eAAC+ soft codec should be included
* in ROM.
*/
#define __INCLUDE_EAACPLUS_CMMFCODEC
#define KFeatureIdIncludeEaacplusCmmfcodec KOtherFeatureFirst+521

/*
* This flag is used to configure the AudioControllerPluginsVariant to use
* the either the soft codec (if #defined)  or the HW codec (if #undefed).
*/
#define __USE_EAACPLUS_CMMFCODEC
#define KFeatureIdUseEaacplusCmmfCodec KOtherFeatureFirst+522

/*
* This flag allows 3rd parties to implement their own meeting request
* solutions.
*/
#define __MEETING_REQUEST_ENABLER
#define KFeatureIdMeetingRequestEnabler KOtherFeatureFirst+590

/*
* This flag indicates that the 3GP Extention feature is supported in
* MetadataUtility.
*/
#define __3GP_EXTENTION
#define KFeatureId3GpExtension KOtherFeatureFirst+592

/*
* Device supports Optical Character Recognizer feature (OCR).
*/
#undef __OCR
#define KFeatureIdOcr KOtherFeatureFirst+593

/*
* Support for OCR engine from Hanwang Technology Co. Ltd.
*/
#undef __OCR_HANWANG
#define KFeatureIdOcrHanwang KOtherFeatureFirst+594

/*
* This flag controls OCR database storage location. If the flag is on, all
* OCR databases are put to ROM image.
*/
#undef __OCR_ROMDB
#define KFeatureIdOcrRomdb KOtherFeatureFirst+595

/*
* Device uses alternative QVGA layout with smaller fonts, designed for
* devices having larger physical screen size.
*/
#undef __QVGA2_LAYOUT_IN_USE
#define KFeatureIdQvga2LayoutInUse KOtherFeatureFirst+596

/*
* This flag defines if Application Shell should use Avkon architecture in UI
* implementation instead of XML UI framework (XUIKON). It affects only to
* Application Shell component.
*/
#undef __APPSHELL_AVKON_UI
#define KFeatureIdAppshellAvkonUi KOtherFeatureFirst+613

/*
* Device supports Hindi fonts. Flag may be used only in IBY files.
*/
#undef __HINDI_ROM_CONTENT
#define KFeatureIdHindiRomContent KOtherFeatureFirst+636

/*
* Defines whether transition effects are used in UI. Also controls whether
* the effect engine is included in ROM or not.
*/
#undef __UI_TRANSITION_EFFECTS
#define KFeatureIdUiTransitionEffects KOtherFeatureFirst+638

/*
* Defines whether RealOne Player is system default player for certain MIME
* types. Disabling this flag enables use of another media player.
*/
#define __REAL_PLAYER_AS_DEFAULT
#define KFeatureIdRealPlayerAsDefault KOtherFeatureFirst+641

/*
* This flag controls if Thai Regional Calendar plugin is delivered to ROM
* Image.
* Plugin enhances S60 Calendar application views with Thai specific
* information (e.g. Thai year).
*/
#undef __THAI_CALENDAR
#define KFeatureIdThaiCalendar KOtherFeatureFirst+646

/*
* This feature finds keywords in application data files, databases, services
* and locations available in mobile environment. This flag controls the
* framework (engine) part of the search feature.
*/
#define __GENERAL_SEARCH_FRAMEWORK
#define KFeatureIdGeneralSearchFramework KOtherFeatureFirst+648

/*
* This feature finds keywords in application data files, databases, services
* and locations available in mobile environment. This flag controls the UI
* part of the search feature.
*/
#define __GENERAL_SEARCH_UI
#define KFeatureIdGeneralSearchUi KOtherFeatureFirst+649


#include "..\..\..\epoc32\include\oem\ProductVariant.hrh"

#endif
