Module flash_config :: Class FlashConfigurationWriter |
[hide private]
[frames] | no frames]

# Class FlashConfigurationWriter

source code
Builder that creates the flash configuration files

Instance Methods | [hide private]
__init__(self, configs, product) FlashConfigurationWriter init | source code
_get_all_languagepacks(self) Collect all language packs and store them internally | source code
_get_compatible_languagepacks(self, config) Get language packs compatible with a customer variant | source code
_get_all_udas(self) Collect all udas and store them internally | source code
_get_all_mms(self) Collect all mm's and store them internally | source code
_get_all_mcs(self) Collect all mc's and store them internally | source code
_get_compatible_udas(self, config) Get uda's compatible with a customer variant | source code
_get_compatible_mms(self, config) Get mm's compatible with a customer variant | source code
_get_compatible_mcs(self, config) Get mc's compatible with a customer variant | source code
_write_file(self, config, romtype, uda, mm, mc) Write an xml flash configuration file | source code
_append_to_makefile(self, config, romtype) | source code
write(self) Go throught the config and creates the flash configuration files | source code