{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Main","Key values"],"not_rendered":{"macros":1,"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Main","index":0,"n_rows":13,"n_cols":6,"rows_kept":13,"flags":["formulas_cached_only"]}
[{"$nulls":5},"DO NOT DELETE THIS SHEET. THE FUTURE CONVERSION SCRIPTS NEED THE TEMPLATE VERSION INFORMATION"]
[null,"Template version","2.0"]
[null,"Purpose"]
[null,"CenRep keys "]
[]
[null,"Entity"]
[null,"Owner"]
[null,"Version",0.02]
[]
[null,"Version History"]
[null,"Date","Version","Type","Author","Comments"]
[null,"2005-03-23",0.01,"draft",null,"First draft, Client initiated firmware update key"]
[null,"2005-05-02",0.02,"draft",null,"Update UID name to include work \"Internal\" so that other private and public keys can be added later"]

{"sheet":"Key values","index":1,"n_rows":23,"n_cols":59,"rows_kept":23,"flags":["formulas_cached_only"]}
["Uid Name","Uid Value","Range From","Range To","Key Name","Key Int","Shared Data Name","Purpose","Removed","Platform Release","Variant Name","Def Value","Read  Only","Key Type","Backup","RFS","Cust Config","Owner","Related Features","AlwaysPass","NetworkServices","LocalServices","ReadUserData","WriteUserData","Location","ReadDeviceData","WriteDeviceData","ProtServ","DRM","SwEvent","PowerMgmt","AllFiles","DiskAdmin","NetworkControl","MultiMediaDD","CommDD","TCB","TrustedUI","UserEnvironment","SurroundingsDD","SID Read","SID Write","Yes","No","Must","Int","Real","Str","Bin","R","W","RW","elaf","apac","thai","japan","gsm","low_cost","Do not delete AN1 -> BC1, since they are used in the multichoise column validation"]
["KCRUidDeviceManagementInternalKeys","0x101F9A0A",{"$nulls":5},"OMA Device Management Internal CR keys"]
[{"$nulls":9},"S60 3.1",{"$nulls":4},"Yes","Yes",null,"0x101F99FB",null,"R",{"$nulls":6},"W"]
[{"$nulls":4},"KDevManClientInitiatedFwUpdateId","0x00000001",null,"Indicates whether device should send firmware update request to device management server. Value is device management profile id. -1 indicates no request (default value).",{"$nulls":4},"No","Int"]
[{"$nulls":9},"S60 3.1",null,-1,null,null,"No","Yes","No",null,"__SYNCML_DM_FOTA","R",{"$nulls":6},"W"]
[{"$nulls":4},"KDevManSessionType","0x00000002",null,"Indicates whether the session is Generic or Fota or other type(future purpose) . 0 Indicates a generic session , 1 Indicates a Fota session ,2 Indicates other session types.",{"$nulls":4},"No","Int"]
[{"$nulls":9},"S60 3.2",null,0,null,null,"No","Yes","No",null,"__SYNCML_DM","R",{"$nulls":6},"W"]
[{"$nulls":4},"KDevManSANUIBitVariation","0x00000003",null,"Indicates whether the following features should be ON or OFF in the package 0 message.\nBit 0 -  UI mode bits processing feature should be ON or OFF. If this bit is \"0\" its OFF , if 1 then its ON.\nBit 1(since S60 5.0)  - Package 0 enhancement feature, which interprets the Vendor specific Information is on or off.\n If this bit 0 its OFF , if 1 then its ON.",{"$nulls":4},"No","Int"]
[{"$nulls":9},"S60 3.1",null,0,null,null,"No","Yes","Yes",null,"__SYNCML_DM","R",{"$nulls":6},"W"]
[{"$nulls":9},"S60 5.0",null,2,null,null,"No","Yes","Yes",null,"__SYNCML_DM","R",{"$nulls":6},"W"]
[{"$nulls":4},"KDevManServerAlertTimeout","0x00000004",null,"Indicates whether the timeout for server alert message variation.\n0 - No timeout. \nNumeric value - In Minutes ",{"$nulls":4},"No","Int"]
[{"$nulls":9},"S60 3.1",null,0,null,null,"No","Yes","Yes",null,"__SYNCML_DM","R",{"$nulls":6},"W"]
[{"$nulls":4},"KDevManUserInteractionAlerts","0x00000005",null,"Indicates whether the user interaction alerts feature is ON or OFF.\nValue : If value is 0 then all alerts are ON.\nRequired alert can be switched OFF  by making the corresponding bit to 1.\nBit 0 - Display Alert (1100) \nBit 1 - Confirmation Alert ( 1101) \nBit 2 - User Input alert ( 1102)\nBit 3 - Single Choice alert ( 1103)\nBit 4 - Multiple Choice alert ( 1104)",{"$nulls":4},"No","Int"]
[{"$nulls":9},"S60 3.2",null,0,null,null,"No","Yes","Yes",null,"__SYNCML_DM","R",{"$nulls":6},"W"]
[{"$nulls":4},"KDevManProfilesXMLFile","0x00000006",null,"ABSOLUTE path of XML file along with filename where DM profiles are stored.",{"$nulls":4},"No","Str"]
[{"$nulls":9},"S60 3.2",null,"Z:\\\\private\\\\101F99FB\\\\factorydmprofiles.xml",null,null,"No","Yes","Yes",null,"__SYNCML_DM","R",{"$nulls":6},"W"]
[{"$nulls":4},"KDevManFUMOPredefinedNodes","0x00000007",null,"Specifies the names of the predefined Dynamic nodes under the FUMO object, ./FUMO/<X>.\nThis is comma separated values upto maximum 4 strings .\nDefault value of X is FWPkg1,FWPkg2,FWPkg3,FWPkg4",{"$nulls":4},"No","Str"]
[{"$nulls":9},"S60 3.1",null,"FWPkg",null,null,"No","Yes","Yes",null,"__SYNCML_DM_FOTA","R",{"$nulls":6},"W"]
[{"$nulls":9},"S60 5.0",null,"FWPkg1,FWPkg2,FWPkg3,FWPkg4",null,null,"No","Yes","Yes",null,"__SYNCML_DM_FOTA","R",{"$nulls":6},"W"]
[{"$nulls":4},"KDevManUINotesCustomization","0x00000008",null,"This flag defines if the feature to enable  the customized UI notes for Package 0 informative , interacttrive and note between firware install and update.\nThis UI notes are requested from CMCC .",{"$nulls":4},"Yes","Int"]
[{"$nulls":9},"S60 3.2",null,0,null,null,"No","Yes","Yes",null,"__SYNCML_DM","R",{"$nulls":6},"W"]
[{"$nulls":4},"KDevManDMSessionTimeout","0x00000009",null,"This key is used to enable DM session time out feature.\nDefault value : -1 \nAllowed values.\n1 - 30 .\nThis unit is in minutes .\nIf value is -1 or any other value  then this feature OFF. And default behavior.\nValue :  1-30, session times out withthin this time E.g If value is 5 min, then a call comes which gets high priorioty than GPRS , Dm session waits for 5 min and times out if Call doesn't end. ",{"$nulls":4},"No","Int"]
[{"$nulls":9},"S60 3.2",null,-1,null,null,"No","Yes","Yes",null,"__SYNCML_DM","R",{"$nulls":6},"W"]