// Copyright (c) 1997-2009 Nokia Corporation and/or its subsidiary(-ies).
// All rights reserved.
// This component and the accompanying materials are made available
// under the terms of the License "Eclipse Public License v1.0"
// which accompanies this distribution, and is available
// at the URL "http://www.eclipse.org/legal/epl-v10.html".
//
// Initial Contributors:
// Nokia Corporation - initial contribution.
//
// Contributors:
//
// Description:
// e32\klib\arm\cumem.cia
// 
//

#include <kernel/klib.h>
#include <e32cia.h>
#include <arm.h>
#if defined(__REPLACE_GENERIC_UTILS)
#include "replacement_utils.h"
#endif

extern "C" {

#ifdef _DEBUG
#define CUMEM_FAULT(cc, reason) asm("mov"#cc" r0, #%a0 " : : "i" (reason)); \
                                asm("b"#cc" " CSM_ZN2KL5PanicENS_13TKernLibPanicE)	
#endif


__NAKED__ void kumemget_no_paging_assert(TAny* /*aKernAddr*/, const TAny* /*aAddr*/, TInt /*aLength*/)
	{
	asm("mrs r3, spsr ");			// r3=spsr_svc
	asm("tst r3, #0x0f ");			// test for user mode
	asm("bne memcpy ");				// if not, just do memcpy
#ifndef USE_REPLACEMENT_UMEMGET
	asm("b umemget_no_paging_assert");
#else
	asm("b umemget");
#endif
	}


#ifndef USE_REPLACEMENT_UMEMGET
	
#ifdef __CPU_ARMV6
// Conditional returns are not predicted on ARMv6
__NAKED__ void dummy_umemget32_exit()
	{
	asm("_umemget32_exit: ");
	asm("ldmfd sp!, {r4, pc} ");	
	}
#define UMEMGET32_EXIT(cc)	asm("b"#cc" _umemget32_exit")
#else
#define UMEMGET32_EXIT(cc)	asm("ldm"#cc"fd sp!, {r4, pc}")
#endif

	
EXPORT_C __NAKED__ void kumemget32(TAny* /*aKernAddr*/, const TAny* /*aAddr*/, TInt /*aLength*/)
	{
	asm("mrs r3, spsr ");			// r3=spsr_svc
	asm("tst r3, #0x0f ");			// test for user mode
	asm("bne wordmove ");			// if not, just do wordmove
	// otherwise fall through to umemget32
	}


EXPORT_C __NAKED__ void umemget32(TAny* /*aKernAddr*/, const TAny* /*aUserAddr*/, TInt /*aLength*/)
	{
	ASM_ASSERT_PAGING_SAFE
#ifdef __USER_MEMORY_GUARDS_ENABLED__
	asm("stmfd sp!, {r11, lr} ");
	asm("subs r12, r2, #1");
	asm("ldrhsb r11, [r0]"); // test access to first byte of kernel memory
	asm("ldrhsb r11, [r0,r12]"); // test access to last byte of kernel memory
	USER_MEMORY_GUARD_OFF(,r11,r12);
	asm("bl 1f");
	USER_MEMORY_GUARD_RESTORE(r11,r12);
	asm("ldmfd sp!, {r11, pc} ");	
	asm("1:");
#endif
	PLD(1);
#ifdef _DEBUG
	asm("tst r2, #3 ");						// check length is a whole number of words
	CUMEM_FAULT(ne, KL::EWordMoveLengthNotMultipleOf4);
#endif
	asm("_umemget_word_aligned: ");	
	asm("stmfd sp!, {r4, lr} ");
	asm("subs ip, r2, #32 ");
	asm("blo _umemget32_small_copy ");
	PLD_ioff(1, 32);
	asm("beq _umemget32_32_byte_case ");	// 32 byte case is common - don't bother to align

	asm("rsb lr, r0, #32 ");				// align destination: 0 - 28 byte copy
	asm("movs lr, lr, lsl #27 ");
	asm("beq _umemget32_large_copy ");
	asm("sub r2, r2, lr, lsr #27 ");
	asm("msr cpsr_f, lr ");					// put length bits 4, 3, 2 into N, Z, C
	asm("ldrmit r3, [r1], #4 ");
	asm("ldrmit r4, [r1], #4 ");
	asm("ldrmit ip, [r1], #4 ");
	asm("ldrmit lr, [r1], #4 ");
	asm("stmmiia r0!, {r3, r4, ip, lr} ");
	asm("ldreqt r3, [r1], #4 ");
	asm("ldreqt r4, [r1], #4 ");
	asm("ldrcst ip, [r1], #4 ");
	asm("stmeqia r0!, {r3, r4} ");
	asm("strcs ip, [r0], #4 ");
	asm("subs ip, r2, #32 ");
	asm("blo _umemget32_small_copy ");

	asm("_umemget32_large_copy: ");			// copy 32 byte blocks
	PLD_ioff(1, 64);
	asm("_umemget32_32_byte_case: ");
	asm("ldrt r2, [r1], #4 ");
	asm("ldrt r3, [r1], #4 ");
	asm("ldrt r4, [r1], #4 ");
	asm("ldrt lr, [r1], #4 ");
	asm("subs ip, ip, #32 ");
	asm("stmia r0!, {r2, r3, r4, lr} ");
	asm("ldrt r2, [r1], #4 ");
	asm("ldrt r3, [r1], #4 ");
	asm("ldrt r4, [r1], #4 ");
	asm("ldrt lr, [r1], #4 ");
	asm("stmia r0!, {r2, r3, r4, lr} ");
	asm("bhs _umemget32_large_copy ");
		
	asm("_umemget32_small_copy: ");			// 0 - 31 byte copy, length in ip bits 0-4
	asm("movs r2, ip, lsl #27 ");
	UMEMGET32_EXIT(eq);
	asm("msr cpsr_f, r2 ");					// put length bits 4, 3, 2 into N, Z, C
	asm("ldrmit r3, [r1], #4 ");
	asm("ldrmit r4, [r1], #4 ");
	asm("ldrmit ip, [r1], #4 ");
	asm("ldrmit lr, [r1], #4 ");
	asm("stmmiia r0!, {r3, r4, ip, lr} ");
	asm("ldreqt r3, [r1], #4 ");
	asm("ldreqt r4, [r1], #4 ");
	asm("ldrcst ip, [r1], #4 ");
	asm("stmeqia r0!, {r3, r4} ");
	asm("strcs ip, [r0], #4 ");	
	asm("movs r2, r2, lsl #3 ");
	UMEMGET32_EXIT(eq);
	asm("msr cpsr_f, r2 ");					// put length bits 1, 0 into N, Z	
	asm("ldrmibt r3, [r1], #1 ");
	asm("ldrmibt r4, [r1], #1 ");	
	asm("ldreqbt ip, [r1], #1 ");
	asm("strmib r3, [r0], #1 ");
	asm("strmib r4, [r0], #1 ");
	asm("streqb ip, [r0], #1 ");
	asm("ldmfd sp!, {r4, pc} ");	
	}


EXPORT_C __NAKED__ void kumemget(TAny* /*aKernAddr*/, const TAny* /*aAddr*/, TInt /*aLength*/)
	{
	asm("mrs r3, spsr ");			// r3=spsr_svc
	asm("tst r3, #0x0f ");			// test for user mode
	asm("bne memcpy ");				// if not, just do memcpy
	// otherwise fall through to umemget
	}


EXPORT_C __NAKED__ void umemget(TAny* /*aKernAddr*/, const TAny* /*aUserAddr*/, TInt /*aLength*/)
	{
	// Optimised for aligned transfers, as unaligned are very rare in practice

	ASM_ASSERT_PAGING_SAFE
	asm("umemget_no_paging_assert:");
#ifdef __USER_MEMORY_GUARDS_ENABLED__
	asm("stmfd sp!, {r11, lr} ");
	asm("subs r12, r2, #1");
	asm("ldrhsb r11, [r0]"); // test access to first byte of kernel memory
	asm("ldrhsb r11, [r0,r12]"); // test access to last byte of kernel memory
	USER_MEMORY_GUARD_OFF(,r11,r12);
	asm("bl 1f");
	USER_MEMORY_GUARD_RESTORE(r11,r12);
	asm("ldmfd sp!, {r11, pc} ");	
	asm("1:");
#endif
	PLD(1);
	asm("tst r0, #3 ");
	asm("tsteq r1, #3 ");
	asm("beq _umemget_word_aligned ");
	asm("cmp r2, #8 ");
	asm("bhs 1f ");

	asm("2: ");
	asm("subs r2, r2, #1 ");
 	asm("ldrplbt r3, [r1], #1 ");
	asm("strplb r3, [r0], #1 ");
	asm("bgt 2b ");
	__JUMP(,lr);

	asm("1: ");						// Attempt to word align
	asm("movs r3, r0, lsl #30 ");
	asm("beq 5f ");
	asm("rsbs r3, r3, #0 ");		// 01->c0000000 (MI,VC) 10->80000000 (MI,VS) 11->40000000 (PL,VC)
	asm("sub r2, r2, r3, lsr #30 ");
	asm("ldrmibt r3, [r1], #1 ");
	asm("strmib r3, [r0], #1 ");
	asm("ldrmibt r3, [r1], #1 ");
	asm("strmib r3, [r0], #1 ");
	asm("ldrvcbt r3, [r1], #1 ");
	asm("strvcb r3, [r0], #1 ");	// r0 now word aligned
	asm("5: ");
	asm("movs r3, r1, lsl #31 ");
	asm("bic r1, r1, #3 ");
	asm("bcs 3f ");					// branch if src mod 4 = 2 or 3
	asm("bpl _umemget_word_aligned ");	// branch if src mod 4 = 0

	asm("4: ");						// src mod 4 = 1
	asm("subs r2, r2, #4 ");
	asm("ldrget r3, [r1], #4 ");
	asm("ldrget ip, [r1] ");
	asm("movge r3, r3, lsr #8 ");
	asm("orrge r3, r3, ip, lsl #24 ");
	asm("strge r3, [r0], #4 ");
	asm("bgt 4b ");
	asm("add r1, r1, #1 ");
	asm("b umemget_do_end ");
	
	asm("3: ");						
	asm("bmi 5f ");
	asm("2: ");						// src mod 4 = 2
	asm("subs r2, r2, #4 ");
	asm("ldrget r3, [r1], #4 ");
	asm("ldrget ip, [r1] ");
	asm("movge r3, r3, lsr #16 ");
	asm("orrge r3, r3, ip, lsl #16 ");
	asm("strge r3, [r0], #4 ");
	asm("bgt 2b ");
	asm("add r1, r1, #2 ");
	asm("b umemget_do_end ");
	
	asm("5: ");						// src mod 4 = 3
	asm("subs r2, r2, #4 ");
	asm("ldrget r3, [r1], #4 ");
	asm("ldrget ip, [r1] ");
	asm("movge r3, r3, lsr #24 ");
	asm("orrge r3, r3, ip, lsl #8 ");
	asm("strge r3, [r0], #4 ");
	asm("bgt 5b ");
	asm("add r1, r1, #3 ");

	asm("umemget_do_end: ");
	__JUMP(eq,lr);
	asm("adds r2, r2, #2 ");		// -1 if 1 left, 0 if 2 left, +1 if 3 left
	asm("ldrplbt r3, [r1], #1 ");
	asm("strplb r3, [r0], #1 ");
	asm("ldrplbt r3, [r1], #1 ");
	asm("strplb r3, [r0], #1 ");
	asm("ldrnebt r3, [r1], #1 ");
	asm("strneb r3, [r0], #1 ");
	__JUMP(,lr);
	}

#endif  // USE_REPLACEMENT_UMEMGET

__NAKED__ void kumemput_no_paging_assert(TAny* /*aAddr*/, const TAny* /*aKernAddr*/, TInt /*aLength*/)
	{
	asm("mrs r3, spsr ");			// r3=spsr_svc
	asm("tst r3, #0x0f ");			// test for user mode
	asm("bne memcpy ");				// if not, just do memcpy
#ifndef USE_REPLACEMENT_UMEMPUT
	asm("b umemput_no_paging_assert");
#else
	asm("b umemput");
#endif
	}


#ifndef USE_REPLACEMENT_UMEMPUT
	
#ifdef __CPU_ARMV6
// Conditional returns are not predicted on ARMv6
__NAKED__ void dummy_umemput32_exit()
	{
	asm("_umemput32_exit: ");
	asm("ldmfd sp!, {r4, pc} ");	
	}
#define UMEMPUT32_EXIT(cc)	asm("b"#cc" _umemput32_exit")
#else
#define UMEMPUT32_EXIT(cc)	asm("ldm"#cc"fd sp!, {r4, pc}")
#endif

	
EXPORT_C __NAKED__ void kumemput32(TAny* /*aAddr*/, const TAny* /*aKernAddr*/, TInt /*aLength*/)
	{
	asm("mrs r3, spsr ");			// r3=spsr_svc
	asm("tst r3, #0x0f ");			// test for user mode
	asm("bne wordmove ");			// if not, just do wordmove
	// otherwise fall through to umemput32
	}

	
EXPORT_C __NAKED__ void umemput32(TAny* /*aUserAddr*/, const TAny* /*aKernAddr*/, TInt /*aLength*/)
	{
	ASM_ASSERT_DATA_PAGING_SAFE
#ifdef __USER_MEMORY_GUARDS_ENABLED__
	asm("stmfd sp!, {r11, lr} ");
	asm("subs r12, r2, #1");
	asm("ldrhsb r11, [r1]"); // test access to first byte of kernel memory
	asm("ldrhsb r11, [r1,r12]"); // test access to last byte of kernel memory
	USER_MEMORY_GUARD_OFF(,r11,r12);
	asm("bl 1f");
	USER_MEMORY_GUARD_RESTORE(r11,r12);
	asm("ldmfd sp!, {r11, pc} ");	
	asm("1:");
#endif
	PLD(1);
#ifdef _DEBUG
	asm("tst r2, #3 ");						// check length is a whole number of words
	CUMEM_FAULT(ne, KL::EWordMoveLengthNotMultipleOf4);
#endif
	asm("cmp r2, #4 ");						// special case for 4 byte copy which is common
	asm("ldrhs r3, [r1], #4 ");
	asm("subhs r2, r2, #4 ");
	asm("strhst r3, [r0], #4 ");
	__JUMP(ls,lr);
	
	asm("_umemput_word_aligned: ");
	asm("stmfd sp!, {r4, lr} ");
	asm("subs r2, r2, #32 ");
	asm("bhs _umemput32_align_source ");

	asm("_umemput32_small_copy: ");			// copy 1 - 31 bytes
	asm("mov r2, r2, lsl #27 ");
	asm("msr cpsr_f, r2 ");					// put length bits 4, 3, 2 into N, Z, C
	asm("ldmmiia r1!, {r3, r4, ip, lr} ");
	asm("strmit r3, [r0], #4 ");
	asm("strmit r4, [r0], #4 ");
	asm("ldmeqia r1!, {r3, r4} ");
	asm("strmit ip, [r0], #4 ");
	asm("ldrcs ip, [r1], #4 ");
	asm("strmit lr, [r0], #4 ");
	asm("streqt r3, [r0], #4 ");
	asm("streqt r4, [r0], #4 ");
	asm("strcst ip, [r0], #4 ");
	asm("movs r2, r2, lsl #3 ");
	UMEMPUT32_EXIT(eq);
	asm("msr cpsr_f, r2 ");					// put length bits 1, 0 into N, Z
	asm("ldrmih r3, [r1], #2 ");
	asm("ldreqb r4, [r1], #1 ");
	asm("strmibt r3, [r0], #1 ");
	asm("movmi r3, r3, lsr #8 ");
	asm("strmibt r3, [r0], #1 ");
	asm("streqbt r4, [r0], #1 ");
	asm("ldmfd sp!, {r4, pc} ");
	
	asm("_umemput32_align_source: ");
	PLD_ioff(1, 32);
	asm("cmp r2, #32 ");
	asm("bls _umemput32_large_copy ");		// don't bother if length <= 64
	asm("rsb ip, r1, #32 ");
	asm("movs ip, ip, lsl #27 ");
	asm("beq _umemput32_large_copy ");
	asm("msr cpsr_f, ip ");					// put length bits 4, 3, 2 into N, Z, C
	asm("sub r2, r2, ip, lsr #27 ");
	asm("ldmmiia r1!, {r3, r4, ip, lr} ");
	asm("strmit r3, [r0], #4 ");
	asm("strmit r4, [r0], #4 ");
	asm("ldmeqia r1!, {r3, r4} ");
	asm("strmit ip, [r0], #4 ");
	asm("ldrcs ip, [r1], #4 ");
	asm("strmit lr, [r0], #4 ");
	asm("streqt r3, [r0], #4 ");
	asm("streqt r4, [r0], #4 ");
	asm("strcst ip, [r0], #4 ");

	asm("_umemput32_large_copy: ");			// copy 32 byte blocks
	PLD_ioff(1, 64);
	asm("ldmia r1!, {r3, r4, ip, lr} ");
	asm("strt r3, [r0], #4 ");
	asm("strt r4, [r0], #4 ");
	asm("strt ip, [r0], #4 ");
	asm("strt lr, [r0], #4 ");
	asm("ldmia r1!, {r3, r4, ip, lr} ");
	asm("strt r3, [r0], #4 ");
	asm("strt r4, [r0], #4 ");
	asm("strt ip, [r0], #4 ");
	asm("strt lr, [r0], #4 ");
	asm("subs r2, r2, #32 ");
	asm("bhs _umemput32_large_copy ");
	asm("adds r2, r2, #32 ");
	asm("bne _umemput32_small_copy ");
	asm("ldmfd sp!, {r4, pc} ");
	}


__NAKED__ void uumemcpy32(TAny* /*aUserDst*/, const TAny* /*aUserSrc*/, TInt /*aLength*/)
	{
	ASM_ASSERT_PAGING_SAFE
#ifdef __USER_MEMORY_GUARDS_ENABLED__
	asm("stmfd sp!, {r11, lr} ");
	USER_MEMORY_GUARD_OFF(,r11,r12);
	asm("bl 1f");
	USER_MEMORY_GUARD_RESTORE(r11,r12);
	asm("ldmfd sp!, {r11, pc} ");	
	asm("1:");
#endif
	asm("1: ");
	asm("subs r2, r2, #4 ");
	asm("ldrplt r3, [r1], #4 ");
	asm("strplt r3, [r0], #4 ");
	asm("bpl 1b ");
	__JUMP(,lr);
	}


__NAKED__ void uumemcpy(TAny* /*aUserDst*/, const TAny* /*aUserSrc*/, TInt /*aLength*/)
	{
	ASM_ASSERT_PAGING_SAFE
#ifdef __USER_MEMORY_GUARDS_ENABLED__
	asm("stmfd sp!, {r11, lr} ");
	USER_MEMORY_GUARD_OFF(,r11,r12);
	asm("bl 1f");
	USER_MEMORY_GUARD_RESTORE(r11,r12);
	asm("ldmfd sp!, {r11, pc} ");	
	asm("1:");
#endif
	asm("cmp r2, #8 ");
	asm("bcs 1f ");
	asm("2: ");
	asm("subs r2, r2, #1 ");
	asm("ldrplbt r3, [r1], #1 ");
	asm("strplbt r3, [r0], #1 ");
	asm("bgt 2b ");
	__JUMP(,lr);
	asm("1: ");
	asm("movs r3, r0, lsl #30 ");
	asm("beq 5f ");
	asm("rsbs r3, r3, #0 ");		// 01->c0000000 (MI,VC) 10->80000000 (MI,VS) 11->40000000 (PL,VC)
	asm("sub r2, r2, r3, lsr #30 ");
	asm("ldrmibt r3, [r1], #1 ");
	asm("strmibt r3, [r0], #1 ");
	asm("ldrmibt r3, [r1], #1 ");
	asm("strmibt r3, [r0], #1 ");
	asm("ldrvcbt r3, [r1], #1 ");
	asm("strvcbt r3, [r0], #1 ");	// r0 now word aligned
	asm("5: ");
	asm("movs r3, r1, lsl #31 ");
	asm("bic r1, r1, #3 ");
	asm("bcs 3f ");					// branch if src mod 4 = 2 or 3
	asm("bmi 4f ");					// branch if src mod 4 = 1
	asm("2: ");
	asm("subs r2, r2, #4 ");
	asm("ldrget r3, [r1], #4 ");
	asm("strget r3, [r0], #4 ");
	asm("bgt 2b ");
	asm("uumemcpy_do_end: ");
	__JUMP(eq,lr);
	asm("adds r2, r2, #2 ");		// -1 if 1 left, 0 if 2 left, +1 if 3 left
	asm("ldrplbt r3, [r1], #1 ");
	asm("strplbt r3, [r0], #1 ");
	asm("ldrplbt r3, [r1], #1 ");
	asm("strplbt r3, [r0], #1 ");
	asm("ldrnebt r3, [r1], #1 ");
	asm("strnebt r3, [r0], #1 ");
	__JUMP(,lr);
	asm("3: ");						// get here if src mod 4 = 2 or 3
	asm("bmi 5f ");					// branch if 3
	asm("2: ");
	asm("subs r2, r2, #4 ");
	asm("ldrget r3, [r1], #4 ");
	asm("ldrget ip, [r1] ");
	asm("movge r3, r3, lsr #16 ");
	asm("orrge r3, r3, ip, lsl #16 ");
	asm("strget r3, [r0], #4 ");
	asm("bgt 2b ");
	asm("add r1, r1, #2 ");
	asm("b uumemcpy_do_end ");
	asm("5: ");
	asm("subs r2, r2, #4 ");
	asm("ldrget r3, [r1], #4 ");
	asm("ldrget ip, [r1] ");
	asm("movge r3, r3, lsr #24 ");
	asm("orrge r3, r3, ip, lsl #8 ");
	asm("strget r3, [r0], #4 ");
	asm("bgt 5b ");
	asm("add r1, r1, #3 ");
	asm("b uumemcpy_do_end ");
	asm("4: ");
	asm("subs r2, r2, #4 ");
	asm("ldrget r3, [r1], #4 ");
	asm("ldrget ip, [r1] ");
	asm("movge r3, r3, lsr #8 ");
	asm("orrge r3, r3, ip, lsl #24 ");
	asm("strget r3, [r0], #4 ");
	asm("bgt 4b ");
	asm("add r1, r1, #1 ");
	asm("b uumemcpy_do_end ");
	}


EXPORT_C __NAKED__ void kumemput(TAny* /*aAddr*/, const TAny* /*aKernAddr*/, TInt /*aLength*/)
	{
	asm("mrs r3, spsr ");			// r3=spsr_svc
	asm("tst r3, #0x0f ");			// test for user mode
	asm("bne memcpy ");				// if not, just do memcpy
	// otherwise fall through to umemput
	}


EXPORT_C __NAKED__ void umemput(TAny* /*aUserAddr*/, const TAny* /*aKernAddr*/, TInt /*aLength*/)
	{
	// Optimised for word-aligned transfers, as unaligned are very rare in practice	

	ASM_ASSERT_DATA_PAGING_SAFE
	asm("umemput_no_paging_assert:");
#ifdef __USER_MEMORY_GUARDS_ENABLED__
	asm("stmfd sp!, {r11, lr} ");
	asm("subs r12, r2, #1");
	asm("ldrhsb r11, [r1]"); // test access to first byte of kernel memory
	asm("ldrhsb r11, [r1,r12]"); // test access to last byte of kernel memory
	USER_MEMORY_GUARD_OFF(,r11,r12);
	asm("bl 1f");
	USER_MEMORY_GUARD_RESTORE(r11,r12);
	asm("ldmfd sp!, {r11, pc} ");	
	asm("1:");
#endif
	PLD(1);
	asm("tst r0, #3 ");
	asm("tsteq r1, #3 ");
	asm("beq _umemput_word_aligned ");
	
	asm("cmp r2, #8 ");
	asm("bcs 1f ");
	asm("2: ");						// Copy 0 - 7 bytes
	asm("subs r2, r2, #1 ");
	asm("ldrplb r3, [r1], #1 ");
	asm("strplbt r3, [r0], #1 ");
	asm("bgt 2b ");
	__JUMP(,lr);
	
	asm("1: ");						// Word-align dest
	asm("movs r3, r0, lsl #30 ");
	asm("beq 5f ");
	asm("rsbs r3, r3, #0 ");		// 01->c0000000 (MI,VC) 10->80000000 (MI,VS) 11->40000000 (PL,VC)
	asm("sub r2, r2, r3, lsr #30 ");
	asm("ldrmib r3, [r1], #1 ");
	asm("strmibt r3, [r0], #1 ");
	asm("ldrmib r3, [r1], #1 ");
	asm("strmibt r3, [r0], #1 ");
	asm("ldrvcb r3, [r1], #1 ");
	asm("strvcbt r3, [r0], #1 ");	// r0 now word aligned
	asm("5: ");
	asm("movs r3, r1, lsl #31 ");
	asm("bic r1, r1, #3 ");
	asm("bcs 3f ");					// branch if src mod 4 = 2 or 3
	asm("bpl _umemput_word_aligned "); // branch if src mod 4 = 0

	asm("4: ");						// get here if src mod 4 = 1
	asm("subs r2, r2, #4 ");
	asm("ldrge r3, [r1], #4 ");
	asm("ldrge ip, [r1] ");
	asm("movge r3, r3, lsr #8 ");
	asm("orrge r3, r3, ip, lsl #24 ");
	asm("strget r3, [r0], #4 ");
	asm("bgt 4b ");
	asm("add r1, r1, #1 ");
	asm("b _umemput_do_end ");
	
	asm("3: ");						// get here if src mod 4 = 2 or 3
	asm("bmi 5f ");					// branch if 3
	asm("2: ");
	asm("subs r2, r2, #4 ");
	asm("ldrge r3, [r1], #4 ");
	asm("ldrge ip, [r1] ");
	asm("movge r3, r3, lsr #16 ");
	asm("orrge r3, r3, ip, lsl #16 ");
	asm("strget r3, [r0], #4 ");
	asm("bgt 2b ");
	asm("add r1, r1, #2 ");
	asm("b _umemput_do_end ");
	
	asm("5: ");						// get here if src mod 4 = 3
	asm("subs r2, r2, #4 ");
	asm("ldrge r3, [r1], #4 ");
	asm("ldrge ip, [r1] ");
	asm("movge r3, r3, lsr #24 ");
	asm("orrge r3, r3, ip, lsl #8 ");
	asm("strget r3, [r0], #4 ");
	asm("bgt 5b ");
	asm("add r1, r1, #3 ");

	asm("_umemput_do_end: ");		// z set if done, else r2 == length remaining - 4
	__JUMP(eq,lr);
	asm("adds r2, r2, #2 ");		// r2 = -1 if 1 left, 0 if 2 left, +1 if 3 left
	asm("ldrplb r3, [r1], #1 ");
	asm("strplbt r3, [r0], #1 ");
	asm("ldrplb r3, [r1], #1 ");
	asm("strplbt r3, [r0], #1 ");
	asm("ldrneb r3, [r1], #1 ");
	asm("strnebt r3, [r0], #1 ");
	__JUMP(,lr);
	}

#endif  // USE_REPLACEMENT_UMEMPUT
	
	
EXPORT_C __NAKED__ void kumemset(TAny* /*aAddr*/, const TUint8 /*aValue*/, TInt /*aLength*/)
	{
	asm("mrs r3, spsr ");			// r3=spsr_svc
	asm("tst r3, #0x0f ");			// test for user mode
	asm("bne memset ");				// if not, just do memset
	// otherwise fall through to umemset
	}


EXPORT_C __NAKED__ void umemset(TAny* /*aUserAddr*/, const TUint8 /*aValue*/, TInt /*aLength*/)
	{
	ASM_ASSERT_DATA_PAGING_SAFE
#ifdef __USER_MEMORY_GUARDS_ENABLED__
	asm("stmfd sp!, {r11, lr} ");
	USER_MEMORY_GUARD_OFF(,r11,r12);
	asm("bl 1f");
	USER_MEMORY_GUARD_RESTORE(r11,r12);
	asm("ldmfd sp!, {r11, pc} ");	
	asm("1:");
#endif
	asm("cmp r2, #7 ");
	asm("bhi 2f ");
	asm("1: ");
	asm("subs r2, r2, #1 ");
	asm("strplbt r1, [r0], #1 ");
	asm("bgt 1b ");
	__JUMP(,lr);	
	asm("2: ");
	asm("and r1, r1, #0xff ");
	asm("orr r1, r1, r1, lsl #8 ");
	asm("orr r1, r1, r1, lsl #16 ");
	asm("movs r3, r0, lsl #30 ");
	asm("beq 3f ");
	asm("rsbs r3, r3, #0 ");		// 01->c0000000 (MI,VC) 10->80000000 (MI,VS) 11->40000000 (PL,VC)
	asm("strmibt r1, [r0], #1 ");	// if 01 or 10 do 2 byte stores
	asm("strmibt r1, [r0], #1 ");
	asm("strvcbt r1, [r0], #1 ");	// if 01 or 11 do 1 byte store
	asm("sub r2, r2, r3, lsr #30 ");
	asm("3: ");						// r0 now word aligned
	asm("subs r2, r2, #4 ");
	asm("strplt r1, [r0], #4 ");
	asm("bgt 3b ");
	__JUMP(eq,lr);					// return if finished
	asm("adds r2, r2, #2 ");		// -1 if 1 left, 0 if 2 left, +1 if 3 left
	asm("strplbt r1, [r0], #1 ");
	asm("strplbt r1, [r0], #1 ");
	asm("strnebt r1, [r0], #1 ");
	__JUMP(,lr);
	}
	
}
