/*
* Copyright (c) 2009 Nokia Corporation and/or its subsidiary(-ies).
* All rights reserved.
* This component and the accompanying materials are made available
* under the terms of the License "Eclipse Public License v1.0"
* which accompanies this distribution, and is available
* at the URL "http://www.eclipse.org/legal/epl-v10.html".
*
* Initial Contributors:
* Nokia Corporation - initial contribution.
*
* Contributors:
*
* Description:
*
*/
//#NAME: autotest MMC, MmmcLoader component
// loads images from drive d: into "internal" mmc on E: and then boots from MMC

#define BASE_ROM
#define REBOOT_DRIVER

#include <rom\##VARIANT##\header.iby>

#undef WITH_EXTENSION
#undef WITH_ROFS
#undef WITH_COMP
#undef MMC_DUAL_SLOT
#undef USE_SDIO_SD_MMC
#undef _NAND2

// enable slot 2, so we can write to "internal" MMC...
#define MMC_DUAL_SLOT
#define USE_SDIO_SD_MMC

files=

#include <rom\##VARIANT##\kernel.iby>
#include "user.iby"
#include <rom\hal\hal.iby>
#include <rom\f32\f32.iby>

data=\epoc32\rom\##VARIANT##\mmctest_load_rel_autoexec.bat	\autoexec.bat

file=\Epoc32\Release\##MAIN##\##BUILD##\MMCLOADER.EXE		\sys\bin\MMCLOADER.EXE
