{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Main","Key values"],"not_rendered":{"macros":1,"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Main","index":0,"n_rows":12,"n_cols":6,"rows_kept":12,"flags":["formulas_cached_only"]}
[{"$nulls":5},"DO NOT DELETE THIS SHEET. THE FUTURE CONVERSION SCRIPTS NEED THE TEMPLATE VERSION INFORMATION"]
[null,"Template version","2.1"]
[null,"Purpose"]
[null,"CenRep keys "]
[]
[]
[]
[null,"Version",0.01]
[]
[null,"Version History"]
[null,"Date","Version","Type",null,"Comments"]
[null,"02.04.2007",0.01,"Draft",null,"Draft version of the document defining the Keys for defining the display order of Location based Applications and Contents/Services in Location Centre"]

{"sheet":"Key values","index":1,"n_rows":11,"n_cols":59,"rows_kept":11,"flags":["formulas_cached_only"]}
["Uid Name","Uid Value","Range From","Range To","Key Name","Key Int","Shared Data Name","Purpose","Removed","Platform Release","Variant Name","Def Value","Read  Only","Key Type","Backup","RFS","Cust Config","Owner","Related Features","AlwaysPass","NetworkServices","LocalServices","ReadUserData","WriteUserData","Location","ReadDeviceData","WriteDeviceData","ProtServ","DRM","SwEvent","PowerMgmt","AllFiles","DiskAdmin","NetworkControl","MultiMediaDD","CommDD","TCB","TrustedUI","UserEnvironment","SurroundingsDD","SID Read","SID Write","Yes","No","Must","Int","Real","Str","Bin","R","W","RW","elaf","apac","thai","japan","gsm","low_cost","Do not delete AN1 -> BC1, since they are used in the multichoise column validation"]
["KCRUidLocationCentre","0x10283137",{"$nulls":5},"UID of the Location Centre Central Repository Key. This key defines the position of the Location based Applications and Contents/Services in Location Centre and the value for Location Centre Server Shutdown timer value."]
[{"$nulls":9},"S60 5.0",{"$nulls":4},"No","No",null,"0x10283137"]
[{"$nulls":4},"ELcTop","0x00000001",null,"Top Key for list of Location based Applications and Contents/Services which are shown at the top of Location Centre list. This key is a Read only key and the default values for the Keys is configured by the device manufacturer while flashing the device. They cannot be dynamically configured. The keys contains a string which contains a list of Unique Identifers for Location based Application and Contents/Services in the order in which the device manufacturer wants these Applications and Contents/Services to be displayed.\nThe maximum length of this string is 1024 characters\nThe format of this Key is defined as\n| Count | Length(1) | UID(1) | Length(2) | UID(2) | ... | Length( Count ) | UID( Count ) |\nwhere,\nCount ( 4 digits ) - The number of Location based Applications or Contents / Services which are predefined to be displayed at the top of Location Centre in the Decimal format. The number of digits are restricted to 4. Even if the no. of significant digits is less than 4 ( for eg. 2, say 10 ), the key item should be packed as 0010.\nLength(n) ( 4 digits ) - Length of the UID for the Location based Application or Content/Service encoded as as a string format. This field contains the length in the in the Decimal format. The number of digits are restricted to 4. Even if the no. of significant digits is less than 4 ( for eg. 2, say 10), the key item should be packed as 0010.\nString(n) - UID of the Location based Application or Content/Service encoded as a string.",{"$nulls":4},"Yes","Str"]
[{"$nulls":9},"S60 5.0",null,"00020008101F85A20008101F85A0",null,null,"No","No","Yes",null,null,"R"]
[{"$nulls":4},"ELcMiddle","0x00000002",null,"Middle Key for list of Location based Applications and Contents/Services which are shown at the middle of Location Centre list.\nThis key takes a Boolean value indicating whether there are any Location based Applications or Contents/Services which have been dynamically installed or not. The values which this key can take are\nETrue, If there are certain Location based Applications or Contents/Service which have been dynamically installed on the terminal.\nEFalse, If there are no Location based Applications or Contents/Service which have been dynamically installed on the terminal.\nThe default value for this Key is EFalse.\nIncase there are any dynamically installed Applications or Contents/Services then these components would be displayed in the middle of Location Centre in the order of their registration.",{"$nulls":4},"No","Int"]
[{"$nulls":9},"S60 5.0",null,0,null,null,"Yes","Yes","No",null,null,"R",{"$nulls":6},"W"]
[{"$nulls":4},"ELcBottom","0x00000003",null,"Bottom Key for list of Location based Applications and Contents/Services which are shown at the top of Location Centre list. This key is a Read only key and the default values for the Keys is configured by the device manufacturer while flashing the device. They cannot be dynamically configured. The keys contains a string which contains a list of Unique Identifers for Location based Application and Contents/Services in the order in which the device manufacturer wants these Applications and Contents/Services to be displayed.\nThe maximum length of this string is 1024 characters\nThe format of this Key is defined as\n| Count | Length(1) | UID(1) | Length(2) | UID(2) | ... | Length( Count ) | UID( Count ) |\nwhere,\nCount ( 4 digits ) - The number of Location based Applications or Contents / Services which are predefined to be displayed at the bottom of Location Centre in the Decimal format. The number of digits are restricted to 4. Even if the no. of significant digits is less than 4 ( for eg. 2, say 10 ), the key item should be packed as 0010.\nLength(n) ( 4 digits ) - Length of the UID for the Location based Application or Content/Service encoded as as a string format. This field contains the length in the in the Decimal format. The number of digits are restricted to 4. Even if the no. of significant digits is less than 4 ( for eg. 2, say 10), the key item should be packed as 0010.\nString(n) - UID of the Location based Application or Content/Service encoded as a string.",{"$nulls":4},"Yes","Str"]
[{"$nulls":9},"S60 5.0",null,"000100081028313B",null,null,"No","No","Yes",null,null,"R"]
[{"$nulls":4},"KLcShutdownTimerValue","0x00000004",null,"Value for Location Centre shutdown timer in milliseconds.",{"$nulls":4},"Yes","Int"]
[{"$nulls":9},"S60 5.0",null,5000,null,null,"No","No","Yes",null,null,"R",{"$nulls":6},"W"]