{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Main","Key values"],"not_rendered":{"macros":1,"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Main","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"flags":["formulas_cached_only"]}
[{"$nulls":5},"DO NOT DELETE THIS SHEET. THE FUTURE CONVERSION SCRIPTS NEED THE TEMPLATE VERSION INFORMATION"]
[null,"Template version","2.0"]
[null,"Purpose"]
[null,"CenRep keys "]
[]
[null,"Entity"]
[null,"Owner"]
[null,"Version",{"v":0.8,"d":"0.80"}]
[]
[null,"Version History"]
[null,"Date","Version","Type","Author","Comments"]
[null,"2004-10-19",{"v":0.2,"d":"0.20"},"Draft",null,"Update, templates etc"]
[null,"2004-10-29",{"v":0.3,"d":"0.30"},"Draft",null,"Updates, corrections"]
[null,"2005-01-20",{"v":0.4,"d":"0.40"},"Draft",null,"Template update"]
[null,"2005-05-23",{"v":0.5,"d":"0.50"},"Draft",null,"Capabilities changed to WriteDeviceData"]
[null,"2005-06-06",{"v":0.6,"d":"0.60"},"Draft",null,"Added capability \"read\" to AlwaysPass"]
[null,"2006-05-18",{"v":0.7,"d":"0.70"},"Draft",null,"Removed keys KCbsLimitedReception and KCbsCleanupTime"]
[null,"2007-10-12",{"v":0.8,"d":"0.80"},"Draft",null,"Added KCRUidCbsVariation UID and KCbsVariationFlags key"]

{"sheet":"Key values","index":1,"n_rows":14,"n_cols":59,"rows_kept":14,"flags":["formulas_cached_only"]}
["Uid Name","Uid Value","Range From","Range To","Key Name","Key Int","Shared Data Name","Purpose","Removed","Platform Release","Variant Name","Def Value","Read  Only","Key Type","Backup","RFS","Cust Config","Owner","Related Features","AlwaysPass","NetworkServices","LocalServices","ReadUserData","WriteUserData","Location","ReadDeviceData","WriteDeviceData","ProtServ","DRM","SwEvent","PowerMgmt","AllFiles","DiskAdmin","NetworkControl","MultiMediaDD","CommDD","TCB","TrustedUI","UserEnvironment","SurroundingsDD","SID Read","SID Write","Yes","No","Must","Int","Real","Str","Bin","R","W","RW","elaf","apac","thai","japan","gsm","low_cost","Do not delete AN1 -> BC1, since they are used in the multichoise column validation"]
["KCRUidCellBroadcast","0x1020298F",{"$nulls":5},"CBS Server specific keys"]
[{"$nulls":9},"S60 3.0",{"$nulls":4},"Yes","Yes",null,"0x1000A859",null,"R",{"$nulls":6},"W"]
[{"$nulls":4},"KCbsReception","0x00000001","KCbsReception","This key setting enables CBS messages reception if it is turned on. Only for CBS Server internal usage.",{"$nulls":4},"No","Int"]
[{"$nulls":9},"S60 3.0",null,0,null,null,"Yes","Yes","No","0x1000A859",null,"R",{"$nulls":6},"W"]
[{"$nulls":4},"KCbsTopicDetection","0x00000002","KCbsTopicDetection","If this key value is set on and the topic of received message is not in the topic list, the topic is added to the topic list. Only for CBS Server internal usage.",{"$nulls":4},"No","Int"]
[{"$nulls":9},"S60 3.0",null,0,null,null,"Yes","Yes","No","0x1000A859",null,"R",{"$nulls":6},"W"]
[{"$nulls":4},"KCbsLanguages","0x00000003","KCbsLanguages","This key holds information of message languages that are allowed to be received. Default value means that all messages with all languages are allowed to be received. Only for CBS Server internal usage.",{"$nulls":4},"No","Str"]
[{"$nulls":9},"S60 3.0",null,"0000000000000000000001",null,null,"Yes","Yes","No","0x1000A859",null,"R",{"$nulls":6},"W"]
[]
["KCRUidCbsVariation","0x102078EE",{"$nulls":5},"CBS local variation API"]
[{"$nulls":9},"S60 5.0",{"$nulls":4},"No","No",null,"0x1000A859",null,"R"]
[{"$nulls":4},"KCbsVariationFlags","0x00000001",null,"The key is used to set if the CBS topics are subscribed automatically (SIM topics and manually added topics). If enabled, also reception setting is set on. 0 = automatic subscription disabled, 1 = automatic subscription enabled",{"$nulls":4},"Yes","Int"]
[{"$nulls":9},"S60 5.0",null,1,null,null,"No","No","Yes",null,null,"R"]