: public note

Created: | 4/17/2008 10:42:09 AM
Modified: | 4/17/2008 10:45:15 AM
Project: |
Author: | Symbian
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Advanced: |
UUID: | {D15FA9CB-37F7-4f6f-9B4A-C93825EB6FB2}
Appears In: | SUPL-MTLR-Standard

<p>Because the SUPL Protocol Module injects a Location Request immediately after a Privacy Request, it is possible that an accurate GPS Position is generated before the delivery of a Reference Location.<br/></p><p><br/></p><p>For simplicity this scenario is not shown.<br/></p>