: public note

Created: | 11/12/2008 3:54:50 PM
Modified: | 11/12/2008 3:56:20 PM
Project: |
Author: | Symbian
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Advanced: |
UUID: | {385082E4-5765-4567-8F56-D9DF1EE4E8AA}
Appears In: | Generic - MOLR - EPOS LS - Dual PSY positioning - Interleaving Consecutive Request - PREQ2501

<p>There is no new session requested because the ongoing session is TB, but the new request from the Location Server is A. The ongoing TB positioning has priority over A positioning. TB positioning will provide a location update satisfying both clients.<br/></p><p>For details see the "AGPS Location Manager" section of the Architectural Specification document.<br/></p>