: public <<subsystem extension>> component instance

Created: | 1/3/2008 11:53:56 AM
Modified: | 1/3/2008 11:53:56 AM
Project: |
Author: | Symbian
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Advanced: |
UUID: | {1DAA9650-BD04-4491-AE47-70725CCC73BD}
Appears In: | SUPL-MOLR-TA-Standard

- Messages To
- Messages From
- Custom Properties

Element | Message | Details
«executable» : Network Gateway | GetCurrentCapabilities(aCapabilities :TLbsNetPosCapabilities&) | Type: Sequence Asynchronous Call
«executable» : Network Gateway | ProcessStatusUpdate(aActiveServiceMask :TLbsNetProtocolServiceMask) | Type: Sequence Asynchronous Call
«executable» : Network Gateway | ProcessStatusUpdate(aActiveServiceMask :TLbsNetProtocolServiceMask) | Type: Sequence Asynchronous Call
: SUPL Server | SUPL_START(aCapab : , aLocId : , aQoP : ) | Type: Sequence Asynchronous Call
: SUPL Server | SUPL_POS_INIT(aCapab : , aAD : , aLocId : , aPos : , aSUPLPos : , aVer : ) | Type: Sequence Asynchronous Call
: SUPL Server | SUPL_POS() | Type: Sequence Asynchronous Call
: SUPL Server | SUPL_POS() | Type: Sequence Asynchronous Call

Element | Message | Details
: SUPL Server | SUPL_RESPONSE(aPosMethod : , aSLPAddr : , aAuthKey : , aKeyIdent4 : ) | Type: Sequence Asynchronous Call
: SUPL Server | SUPL_POS() | Type: Sequence Asynchronous Call
: SUPL Server | SUPL_END(aPos : , aStatusCode : , aVer : ) | Type: Sequence Asynchronous Call
: SUPL Server | SUPL_POS() | Type: Sequence Asynchronous Call

Property | Value
isIndirectlyInstantiated: | true