: public note

Created: | 1/4/2008 2:18:46 PM
Modified: | 3/5/2008 6:47:27 PM
Project: |
Author: | Symbian
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Advanced: |
UUID: | {CEEFC84B-5FD2-49d9-8759-841353A63B4B}
Appears In: | Common - Network Location Request

<p>As a result of the Location Request the AGPS Module MUST generate the Assistance Data Request.<br/></p><p>Normally the Module requests the default assistance data set required to perform positioning<br/></p><p>It may also indicate that no assistance data is needed by setting the aDataRequestmask to 0, what is usually the case if the module has already received all the required Assistance Data.<br/></p>