Note : public note

Created: | 8/11/2008 4:42:36 PM
Modified: | 10/9/2008 3:51:15 PM
Project: |
Author: | Symbian
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Advanced: |
UUID: | {0A2996BA-C712-4d3e-890E-AF8502CCD8AA}
Appears In: | Generic - MOLR - Get Last Known Position Area

<p>During a typical MO-LR location can arrive from two different sources<br/></p><p> - AGPS Manager - GPS position (Terminal Based positioning only)<br/></p><p> - Network - Reference Position (both Terminal Based and Terminal Assisted positioning) <br/></p><p> and Final Network Position (Terminal Assisted positioning only)<br/></p><p><br/></p><p>Every time the Location Monitor receives a location it takes the following actions:<br/></p><p>- schedules the position to be stored in a permanent storage (to improve performance the permanent store should not be updated more frequently than every couple of seconds).<br/></p><p><br/></p><p>When updating the permanent store the Location Monitor requests/uses Mobile Network Information from Etel and searches the store to check for network information match (Cell Id, MCC, MNC, LAC). <br/></p><p>If no match was found the location is added to the store. If a mach has been found the stored position is replaced.<br/></p>