{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Main","Key values"],"not_rendered":{"macros":1,"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Main","index":0,"n_rows":14,"n_cols":6,"rows_kept":14,"flags":["formulas_cached_only"]}
[{"$nulls":5},"DO NOT DELETE THIS SHEET. THE FUTURE CONVERSION SCRIPTS NEED THE TEMPLATE VERSION INFORMATION"]
[null,"Template version","2.0"]
[null,"Purpose"]
[null,"CenRep keys "]
[]
[null,"Entity","Networking CF"]
[null,"Owner","sirpa.h.kemppainen@nokia.com"]
[null,"Version",0.03]
[]
[null,"Version History"]
[null,"Date","Version","Type","Author","Comments"]
[null,"2004-11-11",0.01,"draft","Tero Mäkelä","First version"]
[null,"2005-01-31",0.02,"draft","Tero Mäkelä","New template taken into use."]
[null,"2005-02-14",0.03,"draft","Tero Mäkelä","Uid name changed"]

{"sheet":"Key values","index":1,"n_rows":27,"n_cols":59,"rows_kept":27,"flags":["formulas_cached_only"]}
["Uid Name","Uid Value","Range From","Range To","Key Name","Key Int","Shared Data Name","Purpose","Removed","Platform Release","Variant Name","Def Value","Read  Only","Key Type","Backup","RFS","Cust Config","Owner","Related Features","AlwaysPass","NetworkServices","LocalServices","ReadUserData","WriteUserData","Location","ReadDeviceData","WriteDeviceData","ProtServ","DRM","SwEvent","PowerMgmt","AllFiles","DiskAdmin","NetworkControl","MultiMediaDD","CommDD","TCB","TrustedUI","UserEnvironment","SurroundingsDD","SID Read","SID Write","Yes","No","Must","Int","Real","Str","Bin","R","W","RW","elaf","apac","thai","japan","gsm","low_cost","Do not delete AN1 -> BC1, since they are used in the multichoise column validation"]
["KCRUidDCL","0x101F6CFE",{"$nulls":5},"Keys for configuring the logging frequency of Data Connection Logger"]
[{"$nulls":9},"S60 3.0",{"$nulls":4},"No","No",null,"0x101F6CFE",null,"R"]
[{"$nulls":4},"KDCLGprsThreshold","0x00000001","KDCLGprsThreshold","GPRS data volume threshold used in volume mode.",{"$nulls":4},"Yes","Int"]
[{"$nulls":9},"S60 3.0",null,20480,null,null,"No","No","Yes",null,null,"R"]
[{"$nulls":4},"KDCLWcdmaThreshold","0x00000002","KDCLWcdmaThreshold","WCDMA data volume threshold used in volume mode.",{"$nulls":4},"Yes","Int"]
[{"$nulls":9},"S60 3.0",null,51200,null,null,"No","No","Yes",null,null,"R"]
[{"$nulls":4},"KDCLWlanThreshold","0x00000003","KDCLWlanThreshold","WLAN data volume threshold used in volume mode.",{"$nulls":4},"Yes","Int"]
[{"$nulls":9},"S60 3.0",null,102400,null,null,"No","No","Yes",null,null,"R"]
[{"$nulls":4},"KDCLLanThreshold","0x00000004","KDCLLanThreshold","LAN data volume threshold used in volume mode",{"$nulls":4},"Yes","Int"]
[{"$nulls":9},"S60 3.0",null,102400,null,null,"No","No","Yes",null,null,"R"]
[{"$nulls":4},"KDCLTimerInterval","0x00000005","KDCLTimerInterval","Timer interval used in timer mode.",{"$nulls":4},"Yes","Int"]
[{"$nulls":9},"S60 3.0",null,10,null,null,"No","No","Yes",null,null,"R"]
[{"$nulls":4},"KDCLForceTimerMode","0x00000006","KDCLForceTimerMode","Force timer mode.",{"$nulls":4},"Yes","Int"]
[{"$nulls":9},"S60 3.0",null,0,null,null,"No","No","Yes",null,null,"R"]
[]
[]
["KCRUidDCLLogs","0x101F4CD5",{"$nulls":5},"Keys for data counter loggings"]
[{"$nulls":9},"S60 3.0",{"$nulls":4},"No","No",null,"0x101F6CFE",null,"R",{"$nulls":6},"W"]
[{"$nulls":4},"KLogsGPRSSentCounter","0x0000000C","KLogsGPRSSentCounter","Amount of total sent bytes using gprs connection.",{"$nulls":4},"No","Str"]
[{"$nulls":9},"S60 3.0",null,0,null,null,"No","No","No",null,null,"R",{"$nulls":6},"W"]
[{"$nulls":4},"KLogsGPRSReceivedCounter","0x0000000D","KLogsGPRSReceivedCounter","Amount of total received bytes using gprs connection.",{"$nulls":4},"No","Str"]
[{"$nulls":9},"S60 3.0",null,0,null,null,"No","No","No",null,null,"R",{"$nulls":6},"W"]
[{"$nulls":4},"KLogsWLANSentCounter","0x00000014","KLogsWLANSentCounter","Amount of total sent bytes using WLAN connection.",{"$nulls":4},"No","Str"]
[{"$nulls":9},"S60 3.0",null,0,null,null,"No","No","No",null,null,"R",{"$nulls":6},"W"]
[{"$nulls":4},"KLogsWLANReceivedCounter","0x00000015","KLogsWLANReceivedCounter","Amount of total received bytes using WLAN connection.",{"$nulls":4},"No","Str"]
[{"$nulls":9},"S60 3.0",null,0,null,null,"No","No","No",null,null,"R",{"$nulls":6},"W"]