overview | deprecated | properties-table | index | help
| Helium API
prev next | frames no frames

# Properties table(Sortable)

Property | Description | Edit Status | Type
--- | --- | --- | ---
absolute.prep.root.dir | This will convert absolute path for prep.root.dir if anybody use relative path. | never | string
ado.mapping.file | Path to a INI file that contains the mapping between the ADO from Synergy WA and it's location on the BA. | never | string
ado.quality.mapping.file | Path to a INI file that contains the mapping between the ADO from Synergy WA and it's location on the BA for quality targets. | never | string
antlib.import.module.path | Path where ant XML files dynamically downloaded from jar file. | never | string
archive.max.number.of.threads | Set the maximum number of threads running for archiving (for a parallel job). | allowed | integer
archive.using.ec | Set to true to enable EC zipping | recommended | boolean
ats.aste.drop.file | Path for creation of the drop file during the build. Default is ATS3AsteDrop.zip | discouraged | string
ats.aste.email.list | The property is needed if you want to get an email from ATS server after the tests are executed. There can be one to many semicolon(s) ";" separated email addresses. | recommended | string
ats.aste.plan.name | Modify the plan name if you have understanding of test.xml file or leave it as it is. Deafault value is "plan" | recommended | string
ats.aste.testrun.name | Modify the test-run name if you have understanding of test.xml file or leave it as it is. Deafault value is a string consist of build id, product name, major and minor versions | recommended | string
ats.ctc.enabled | Should be "True" if coverage measurement and dynamic analysis (CTC) tool support is to be used by ATS. Deafault value is "False", the values are case-sensitive. | recommended | string
ats.drop.file | Path for creation of the drop file during the build. Default is ATS3Drop.zip | discouraged | string
ats.drop.location | Server location (UNC path) to save the ATS3Drop file, before sending to the ATS. For example: \\trwsem00\some_folder\. In case, ``ats.script.type`` is set to "import", ATS doesn't need to have access to ats.drop.location, its value can be any local folder on build machine, for example c:\temp (no network share needed). | must | string
ats.email.list | The property is needed if you want to get an email from ATS server after the tests are executed. There can be one to many semicolon(s) ";" separated email addresses. | recommended | string
ats.flash.images | List of flash images (.fpsx files) to install on the phone. It is not recommended to set the value manually however, it is possible. | allowed | string
ats.flashfiles.minlimit | Limit of minimum number of flash files to execute ats-test target, otherwise ATSDrop.zip will not be generated. Default value is "2" files. | recommended | string
ats.password | Password for ATS. This password might be different from NOE or HTTP/UNIX password. | must | string
ats.plan.name | Modify the plan name if you have understanding of test.xml file or leave it as it is. Deafault value is "plan" | recommended | string
ats.product.hwid | Product HardWare ID (HWID) attached to ATS. By default the value of HWID is not set. | recommended | string
ats.product.name | Name of the product to be tested. For example: "PRODUCT" | must | string
ats.report.location | Sets ATS reports store location. Default location is "${publish.dir}/${publish.subdir}" | allowed | string
ats.script.type | There are two types of ats script files to send drop to ATS server, "runx" and "import"; only difference is that with "import" ATS doesn't have to have access rights to testdrop.zip file, as it is sent to the system over http and import doesn't need network shares. If that is not needed "import" should not be used. Default value is "runx" as "import" involves heavy processing on ATS server | recommended | string
ats.server | For example: "4fio00105" or "catstresrv001.cats.noklab.net:80". Default server port is "8080", but it is not allowed between intra and Noklab. Because of this we need to define server port as 80. The host can be different depending on site and/or product. | must | string
ats.target.platform | Sets target platform for compiling test components. Default value is "armv5 urel". | recommended | string
ats.test.timeout | To set test commands execution time limit on ATS3 server, in seconds. Default value is "60". | recommended | string
ats.testrun.name | Modify the test-run name if you have understanding of test.xml file or leave it as it is. Deafault value is a string consist of build id, product name, major and minor versions | recommended | string
ats.trace.enabled | Should be "True" if tracing is needed during the tests running on ATS3. Deafault value is "False", the values are case-sensitive. | recommended | string
ats.username | Username for ATS server. This is NOT the NOE or HTTP/UNIX username. | must | string
binary.root | Defines location of binaries created in build. Used in check-capability target while generating capability scan report. | never | string
branch.name | this along with week.number used to find proper history file based on releases. | allowed | string
build.cache.dir | Directory where Helium can store files on a temporary basis for a user per build. | never | string
build.cache.log.dir | Directory where Helium can store log files on a temporary basis for a user per build. | never | string
build.drive | Substed drive where the build is performed. if not defined then helium should search next available build drive letter and subst autometically | recommended | string
build.drive.notdefined | used to track if build.drive has predefined or not | never | flag
build.duplicates.log | Default name of the build duplicates log file. | discouraged | string
build.errors.limit | Maximum allowable errors in a build. | allowed | number
build.id | A unique ID for the build. | discouraged | string
build.int.db.dir | The directory where the build integer database text files are stored. | discouraged | string
build.log | Defines name of the log file. | never | string
build.log.dir | This is where the build logs are stored. | discouraged | string
build.logging.key.stages | Defines which stages are considered as key stages and logged. | discouraged | string
build.logging.start.stage | Defines at which point logging is started. | discouraged | string
build.name | A general label for this type of build. Currently if not defined, product.name will be used to set this property, but this will likely be removed in future. | must | string
build.output.dir | This is the directory where build output is placed. | never | string
build.property.cache.file | A file where persistent properties for a build should be stored. | never | string
build.sisfiles.dir | This is the directory where sisfiles are placed. | never | string
build.summary.file | This is the file where build summary is stored. | discouraged | string
build.system | This specifies which build system is used. Default for this is ebs You can use ec for Electric Cloud.. | allowed | string
build.system.ebs | Defined if build.system is set to "ebs", which is the default. | never | string
build.system.sbs | Defined if ${build.system} is set to "sbs". | never | string
build.temp.dir | A directory for storing temporary build files. | never | string
build.type | The general type of the build. This is used for checking the tools environment. Potential values include core, ido, product. | recommended | string
build.version | Version of the build. | discouraged | string
cache.dir | Root directory where Helium can store files on a temporary basis for a user. | never | string
call.cleanup | Ensures the cleanup-all target is called when the build finishes. | allowed | string
canonical.sysdef.file | The path of the generated canonical System Definition file that contains all the input System Definition file content. | never | string
ccm.base.dir | Directory where CCM operations will be performed. | allowed | string
ccm.cache.xml | Location of the cache.xml file which enables global synergy sessions. | allowed | string
ccm.database | Name of the CCM database to use. No default value. | must | string
ccm.database.path | Path of the CCM database. No default value | discouraged | string
ccm.enabled | Defines that property if you want the ccm-get-input step to be run during the build area preparation. | allowed | string
ccm.engine.host | Engine host of CCM database. No default value. | must | string
ccm.home.dir | Home directory of CCM operations. | must | string
ccmgetinput | To check which ccmgetinput helium will be use | allowed | string
ccmtask.python.script.file | The path for the Python script to handle the ccm task bridge to the ccm.py module. | never | string
ci.min.ba.maintain | Minimal number of build area to keep. | allowed | string
ci.project.config | Location of the configuration that will be generated for the Cruise Control HLMSynergy modificationset. | allowed | string
ci.session.file | Location of the session file which will be created by Helium. | allowed | string
cmaker.component.dir | Location of the cmaker component to install it. | never | string
cmaker.config.dir | Directory where to execute cMaker. | discouraged | string
cmaker.pp.version | Version of PP(NCP) configuration to be exported | recommended | string
cmaker.s60.version | Version of S60(require cmaker.pp.version to be set) configuration to be exported | recommended | string
codescanner.config | Defines the location of a custom configuration for codescanner. | allowed | string
codescanner.format | Defines the format of Codescanner output (html|xml|std). | allowed | string
codescanner.log.unique | Defines if the folder for Codescanner output is unique (on|off). | allowed | string
common.overlay.dir | Location of the common overlay. | must | string
compile.signal.name | Name of the signal to be able to override the compile-main target. | never | string
compile.symbianos | Property must be set if the Symbian System Definition file is included in a build, in order to do full build from source. | never | string
compile.sysdef.dtd.stub | compile.sysdef.dtd.stub | never | string
core.build.version | This Defaults to the ${major.version}.${minor.version} combo and is available so that 1 number can be used (dot can be removed) | allowed | string
core.rom.output.dir | /output/release_flash_images/rnd/core | must | string
create.bom.workarea.root | Your synergy work area directory (Set as the parent of the helium dir by default) | allowed | string
ctool.china.conf | configuration for the chinese variant. | allowed | string
ctool.dir | Location of the configuration tool. | allowed | string
ctool.japan.conf | configuration for the japanese variant. | allowed | string
ctool.region.china | . | never | string
ctool.western.conf | configuration for the western variant. | allowed | string
current.env.config | Internal property used for environment setting in the beginning of the build. | never | string
customer.makefile.target | Default makefile target for running customer iMaker ROM building. | never | string
data.model.file | The data model XML file for the Ant configuration. | never | string
data.model.parsed | The data model XML file for the Ant configuration parsed. | never | string
data.model.xsl | Data Model extra content | allowed | string
database.file | Location of helium database | never | string
delta.ant.file | Temp file | never | string
delta.exclude.commasep | Comma seperated excluded directories from the zip | allowed | string
delta.zip.delete.file | Special Instructions file for SymDEC | never | string
delta.zip.file | The zip file | never | string
delta.zip.file.size | Define the file size of the zipped up released file, this is then used by delta zipping code to determine if a delta zip is required or a full zip should be created. The delta zip will only be published if it is less than 1/2 the size of this property | must | string
delta.zip.location | Output location | never | string
delta.zip.temp.location | Temp location | never | string
diamonds.build.id | The ID assigned to the build by the Diamonds server. | never | string
diamonds.build.url | The full URL to the build entry on the Diamonds server. | never | string
diamonds.compile.summary | Compilation summary file for diamonds. | never | string
diamonds.host | Diamonds server's host address. | discouraged | string
diamonds.listener.configuration.file | Diamonds Configuration file with full path used for diamonds listener. | never | string
diamonds.mail | Email address of diamonds server. | discouraged | string
diamonds.path | Diamonds server build location. | discouraged | string
diamonds.port | Diamonds server port number. | discouraged | string
diamonds.schema | Diamonds rest api schema. | discouraged | string
diamonds.target.list.to.log | List of targets that should be logged in to Diamonds. | discouraged | string
disable.analysis.tool | Set this property to disable Analysis Tool. By default Analysis Tool will run with every build and send api metrics to diamonds but Analysis Tools takes time. | allowed | string
documentation.host | The host server where the Helium documentation is stored. | never | string
documentation.path | The full path on the host server where the Helium documentation is stored. | never | string
documentation.path.root | The root of the path on the host server where the Helium documentation is stored. | never | string
documentation.url.root | Root location of the Helium release documentation. | allowed | string
drop.file.counter | Drop package file counter. Updates its value automatically when a new drop file is created for ATS. | never | integer
ec.allow.duplicates | Setting this to "1" will force xml2mak to generate only warnings (instead of errors) for duplicate components in the component list | discouraged | string
ec.build.class | Build class for Electric Cloud. No default value. | never | string
ec.emake | Location of emake tool. | discouraged | string
ec.history.dir | This specifies the directory where Electric Cloud history files are stored. Currently defined in helium.ant.xml and mapped related to publish.root.dir | discouraged | string
ec.history.option | Should be create for single node build and merge for multi node build. | never | string
ec.historyfile | Temporary location of the EC history file used by the current build. | discouraged | string
ec.makefile.file | Location of the Makefile generated to run the EC build. | discouraged | string
ec.maxagents | Maximum number of agent to be used | allowed | string
ec.mem.limit | memory limit for EC execution. See user guide for more details | never | string
ec.mode | mode is either serial / parallel - default is parallel | allowed | string
ec.scripts.dir | ec scripts location | discouraged | string
ec.sysdef2make | Location of sysdef2make.pl file, which is used to translate system definition files to make files. Internal property that normally does not require changes. | never | string
ec.tools.dir | Location of EC-tools. Passed to environment variable EC_TOOLS_DIR, when calling ecbuild_electric.cmd to execute Electric Cloud build. | discouraged | string
ee_roms.log.file | ee log file location | never | string
ee.makefile.target | Defines make target that is run when creating engineer english images. | allowed | string
ee.rom.output.dir | /output/development_flash_images/engineering_english/logs | must | string
email.ldap.rootdn | Root distinguished name of the LDAP server. | allowed | string
email.ldap.server | Network address of the LDAP server. | allowed | string
email.smtp.server | Network address of the SMTP server. | allowed | string
enabled.aste | Value must be set to execute ats-aste target. for example, 'value="1"' | must | string
enabled.ats | Value must be set to execute ats-test target. for example, 'value="1"' | must | string
epocroot | epocroot path | discouraged | string
error.email.to.list | List of email addresses where email is sent in case of build failure. No default value | never | string
eunit.prepare.zip | Name of eunit zip file. Need to unzip into build area to start eunit test | must | string
eunit.test.package | The EUnit package name to be unzipped on the environment, for executing EUnit tests." | recommended | string
eunitexerunner.flags | Flags for EUnit exerunner can be set by setting the value of this variable. The default flags are set to "/E S60AppEnv /R Off". | must | string
exclude.test.layers | Comma seperated excluded test layers. The test components (mentioned in the excluded test layers) will not be included in the ATS test drops | allowed | string
ext.java.lib.dir | External ant library path | never | string
failonerror | failonerror attribute for exec | never | boolean
file-comparison.bcomp_conf | Defines the location of Beyond Compare configuration file. | allowed | string
file-comparison.bcomp_path | Defines the location of BComp.exe. | allowed | string
file-comparison.left_name | Defines the name of the folder for the left side of comparison. | allowed | string
file-comparison.left_side | The fileset id used on the left side of comparison. | must | string
file-comparison.output | Defines the location where comparison output should be put. | allowed | string
file-comparison.regexp.from | Defines the regexp pattern (in ANT-pattern style) which to mach from given filesets. | allowed | string
file-comparison.regexp.to | Defines the regexp pattern (in ANT-pattern style) what to use in (possible) replacement. | allowed | string
file-comparison.right_name | Defines the name of the folder for the right side of comparison. | allowed | string
file-comparison.right_side | The fileset id used on the right side of comparison. | must | string
flash.config.enabled | Define that property to enable config file generation. | recommended | flag
genxml.output.file | Path for the output XML file generated by genxml used as input to EBS or EC. | never | string
genxml.output.file.suffix | Suffix used in genxml related output files. This value is added into file names to show that they are genxml related. Used in log files, genxml output files and component list for EE images. Normally does not need to be set. | never | string
getenv.tool.location | Defines the location of the getenv.pl script. | never | string
helium.build.dir | The path where Helium-specific outputs are written to. | never | string
helium.ccm.workarea.dir | The path to a Synergy work area used for updating Helium releases. | allowed | string
helium.dir | Defines the logical path to the helium directory used to start a build. | never | string
helium.doc.dir | Location of helium doc src. | never | string
helium.java.lib.dir | helium java library location | never | string
helium.svn.url | SVN URL where to find Helium. | allowed | string
helium.svn.workarea.dir | The path to a Subversion work area used for updating Helium releases. | allowed | string
helium.version | Contains Helium version information | never | string
hlm.enable.asserts | Enable helium asserts. Build will fail if this is enabled and asserts fail. | recommended | string
ido.build.filter | Property is used to define ido build filters in the configuration file. | never | string
ido.cenrep.root | Path to the cenrep root. Default value is "${build.drive}${env.EPOCROOT}/epoc32/tools/cenrep/ido/src" | never | string
ido.cenrep.target | Path to the cenrep target directory. Default value is "${build.drive}${env.EPOCROOT}/epoc32/data/z/private/10202be9" | never | string
ido.codescanner.config | Defines the location of a custom configuration for codescanner. | allowed | string
ido.codescanner.output.dir | Defines the location of Codescanner output. | recommended | string
ido.codescanner.output.type | Defines the format of Codescanner output (html|xml|std). | allowed | string
ido.keep.old | Once define this property will enable the backup of old ado before doing the copy. | allowed | string
ido.romtree | Path to the build romtree; the location contains iby files. Default value is "${build.drive}${env.EPOCROOT}/epoc32/rom/include" | never | string
ido.template.robot.ready | Location of the ready.txt FMPP template (override that property if you want to customize the content). | discouraged | string
image_creation.copyto | Path for copying the image files default is output/images | never | string
image_creation.drive | Drive (environment) to use for creating images | never | string
imagetool.cfg.xml.parsed | Locates the parsed configuration for ImageTool in the build directory. | never | string
imagetool.destination | Location where to copy ImageTool and definitions. | allowed | string
imagetool.images | Defines comma separated list of image names. | allowed | string
imagetool.log | Defines name of the ImageTool log file. | never | string
imagetool.output.dir | Defines the location of ImageTool output files. | never | string
imagetool.tooldir | Defines the location of ImageTool. | never | string
imaker.command | The path to the iMaker executable file. | never | string
imaker.engine | Defines which accelerator to use for running iMaker. (default value from build.system property) | never | string
imaker.fmpp.ant | Location of the Ant iMaker execution template. | never | string
imaker.fmpp.makefile | Location of the EC iMaker execution template. | never | string
internal.api.config | Location of the config to parse the build content. | allowed | string
internal.api.output.postbuild | Location of the postbuild ado header content. | allowed | string
internal.api.output.prebuild | Location of the prebuild ado header content. | allowed | string
is.published | The value is either true or false depending on whether the publish property is set or not. | never | string
isis_mktarget.list | Comma separated list of file names(main, what, check file names) | never | string
ivy.file | Location of ivy jar. | never | string
ivy.filename | Name of ivy jar. | never | string
last.major.helium.version | Last major helium version | never | string
loc.output.dir | The directory that will contain the zipped .loc files zip package. | never | string
loc.output.filename | The filename of the zip-loc-files target output zip file. | never | string
loc.temp.dir | The location of temporary directory used during zip-loc-files. | never | string
local.free.space | The amount of free space needed on the build machine in Mbs. | recommended | string
localisation.buildfile | begining of the localisation buildfile name | never | string
localisation.files.china | Localisation files for the China region. | recommended | string
localisation.files.japan | Localisation files for the Japan region. | recommended | string
localisation.files.western | Localisation files for the western region. | recommended | string
localisation.language.file | Defined where to find languages.xml. | never | string
localisation.makefile.target | Makefile target that is executed when creating localised rom images (target localisation-roms). | allowed | string
localisation.s60locfiles.dir | Location of Series 60 localisation input files. Internal property that does not normally needs to be set. | never | string
localisation.tool | This key defines which tool should be used to localise the build area (localisation-mcss-localiser or localisation-s60-localiser). | never | string
log.build.build_id | Diamonds logging information. | never | string
log.build.category | Diamonds logging information. | never | string
log.build.computer | Diamonds logging information. | never | string
log.build.user | Diamonds logging information. | never | string
log.target | Enables logging of the start and end of individual targets. | allowed | string
log4j.cache.dir | Log directory for log4j. | allowed | string
log4j.configuration | Defines the path to log4j configuration. | never | string
logging.output.file | Location of generated logging config. | never | string
major.version | Part of a version information that is used to differentiate a build. Major version is the part that changes less frequently. Ie. year. | allowed | string
md5.signature.file | Output location of md5 file | never | string
md5.split | Number of partial md5 files to use during creation | never | string
metadata.db.file | The path to the SQLite metadata database file. | never | string
minor.version | Part of a version information that is used to differentiate a build. Minor version is the part that changes more frequntly. Ie week or a running number. | allowed | string
network.drive | The drive letter of a substed drive that maps to the network location where the build is published. | recommended | string
network.free.space | Amount of free space in MBs needed on the network drive where the build is published. The ``network.drive`` drive property must also be defined. | allowed | string
notes.database | The Notes database to do DCT5 upload to. | recommended | string
notes.release.dir | The DCT5 Release Notes SW Release Folder (where your build is Published to, so it can be obtained from there.) | never | string
notes.server | Lotus notes server name | recommended | string
number.of.threads | how many parallel threads can run | allowed | string
old.md5.file | A previous builds md5 | allowed | string
old.md5.file.present | Is a previous builds md5 being passed manually | allowed | string
overlays.log.file | The path to the overlays output log file. | never | string
parse_abld_what.tool | Location of the parse_what_log.pl tool. | allowed | string
prep.build.dir | This is the directory where the build area is prepared. Once created it is substed to the build.drive. | never | string
prep.config.file | Defines configuration file used in prep-copy target. The file defines how files are copied and extracted into build area. | must | string
prep.delivery.file | Defines configuration file used in synergy operations (ccm-get-input for example). This file contains definition of projects that are checkouted or snapshotted. | must | string
prep.delivery.modificationset | Location where the XML modificationset file should be generated. If not defined the file is not generated. (Usefull for CI systems) | allowed | string
prep.root.dir | The directory where new build area directories are created and substed to the build drive. | recommended | string
product.family | In product builds defines the product family that the build product belong to. | must | string
product.list | In product builds defines the list of products that are build in the configuration. Property is used in rom image creation, localisation release notes creation and data packaging. | must | string
product.printname | A printable name for a product used in release notes. | must | string
product.type | Project ID in release notes. | must | string
programlevel.release.tag | Program level release tag name | allowed | string
publish | Defines whether the build content will be published to the network. | recommended | string
publish.base.dir | Directory where all builds are published. Same as publish.dir but without build.id at the end | never | string
publish.ccm.folder | Synergy folder where you want your task to be published. | allowed | string
publish.dir | Directory where the build is published (includes build.id) | must | string
publish.fileset.ids | The fileset id which will be upload | allowed | string
publish.release.dir | The directory where the release of this build is published to on the local network. | never | string
publish.release.subdir | Subdir part of the publish release dir, relative to publish.root.dir | never | string
publish.root.dir | Defines the root directory of publish feature. Should point into the root of the folder that will contain published nightly builds/releases. | recommended | string
publish.subdir | Subdir part of the publish dir, relative to publish.root.dir | allowed | string
python.modules.path | Python modules path. | allowed | string
qmake.enabled | If defined the qmake stage will be enabled during compilation. | allowed | string
qt.configure.args | The command lines argument passed to the configure tool. | allowed | string
qt.configure.log.name | The name of the Qt configure output log. | never | string
qt.dir | The location of the Qt framework to build. | recommended | string
qt.qmake.ant.template | The location of the ant template to run qmake commands. | allowed | string
qt.qmake.default.args | Setting default arguments to qMake command line, if the qmakeArgs is defined from the system definition file then those arguments are discarded. | allowed | string
read.build.int | This must be set to enable reading the build.number from a text database file located on the network. It allows automated build number incrementing. | allowed | string
release.dir.root | This is the directory which points to release-directory root. | never | string
release.images.dir | The directory where flash images of build can be found | never | string
releasenotes.logo | Defines the logo image file which will be used in release notes. | never | string
releasenotes.output | Location of output rtf file | never | string
releasenotes.output.dir | Defines the directory that will contain the output of release notes creation. | never | string
releasenotes.props | Property file with customer values | never | string
releasenotes.scan2log | Location of scan2log HTML file | never | string
releasenotes.temp.errors | Temp file | never | string
releasenotes.temp.output | Temp file | never | string
releasenotes.temp.props | Temp file | never | string
releasenotes.temp.props2 | Temp file | never | string
releasenotes.template | Defines the name of the release note template used. | never | string
relnotes.config.dir | Defines the directory that contains release notes creation configuration files. | must | string
remote.builds.config.file | The path to the configuration file for remote builds. | never | string
required.ant.version | The version of Apache Ant required by Helium. | never | string
robot.email.to | Comma seperated list of email address. | discouraged | string
rombuild.buildinfo.output | Location of the output file. | never | string
rombuild.buildinfo.template | FMPP template to generate a buildinfo makefile. | never | string
rombuild.config.file | This key defines where this parsed file will be located. | must | string
rombuild.config.file.parsed | Locates the parsed configuration for ROM builds. | never | string
rombuild.makefile.name | The filename of the output makefile generated by Helium for iMaker. | allowed | string
rombuild.using.var | Define this property if you build is using Symbian Binary Variation. | allowed | boolean
roms.spec.name | Used to select spec-section in rom image configuration for building. Used only for makefpsx. | never | string
s60.build.robot.date | This property represent the releasing interval. The syntax is as follow: day1,time1,day2,time2,projectname;day1,time1,day2,time2,projectname2
     With day and time matching the following properties: day [1, 14] time [00, 23]:[00, 59] Example: 2,10:00,3,20:00,ABS_domain
| must | string
s60.build.robot.path | Location where to publish the build robot delivery. | must | string
s60.delta.config.prefix | Define the prefix part of the configuration name that builds delta variant. | allowed | string
s60.getenv.trigger.location | Define the location of the trigger file that should be used by CI. | allowed | string
sbs.config | Configurations for which the components to be built(armv5,winscw) | allowed | string
sbs.hlm.scanlog | Enable helium scanlog for raptor. (experimental temporary solution) | allowed | boolean
sbs.implicit.tools.build | uses tools config to be built before building the actual configuration. | allowed | boolean
sbs.tools.config | tools configuration to be built | allowed | string
selge.ini.network.dir | \\\\vcfiler02\\pub\\flash_user\\Crashbin/working\\selge_ini_prep | must | string
signals.buildexception.signalname | Name of the signal configuration that is used when a signal is fired after catching a BuildException failure. | allowed | string
sis.config.file | Configuration file for SIS-file generation. | recommended | string
skip.ats.sending | Skips sending drop package file to ATS/ASTE after its creation. | allowed | boolean
skip.build.duplicates | This allow you to skip the build duplciates log generation. | allowed | boolean
skip.codescanner | Skip the codescanner target if true (true/yes/on). | allowed | boolean
skip.compile-ec-patch | If defined it skips the buildtools emake patching. | allowed | string
skip.policy-validation | Skip the policy validation target if true (true/yes/on). | allowed | boolean
sms.number | sms numbers to report error or build information. | never | string
sms.server | Server that sends SMSs | allowed | string
src | Source location for junit test class | never | string
src.classes | Java source files location for helium library | never | string
src.dir | java source directory location for helium library | never | string
subcon.build.drive | Build drive for subcon build | never | string
subcon.log.file | The path to the subcon ROMs log. | never | string
subcon.makefile.target | The name of the makefile target for making subcon ROMs. | never | string
subcon.prep.config.file | Subcon prep configuration file location | must | string
subcon.rombuild.config.file | A ROM configuration file for verifying subcon ROMS. | never | string
subcon.zips.dir | The directory where subcon zips are stored. | never | string
sysdef.clean.configurations.list | Comma-separated list of System Definition configuration names to be built in the ido-prep-clean stage. If not defined the sysdef.configurations.list will be used to generate that configuration list. | allowed | string
sysdef.configurations.list | Comma-separated list of System Definition configuration names to be built in the compile-main stage. | must | string
team | Used to specify which team configuration is being used. These configuration files are under /mc/mc_build/teams. | recommended | string
teamlevel.ci.system | Change release tag from team level to product level | allowed | boolean
teamlevel.folder.number | Folder name which contains those tasks to change the release tag | allowed | string
temp.build.dir | Directory to store temporary files generated during the process. | never | string
tools.ivy.config.file | The tools dependencies Ivy settings configuration file. | allowed | string
trace.log.file | The path to the trace ROMs log. | never | string
trace.makefile.target | The name of the makefile target for making trace ROMs. | never | string
tracing.csv.file | Path location for the memory tracing data captured by the TracingLogger. | never | string
tsrc.data.dir | The default value is "data" and refers to the 'data' directory under 'tsrc' directory. | allowed | string
tsrc.path.list | Contains list of the tsrc directories. Gets the list from system definition layer files. Assuming that the test components are defined already in te layers.sysdef.xml files to get compiled. Not recommended, but the property value can be set if there are no system definition file(s), and tsrc directories paths to set manually. | allowed | string
uda.makefile.target | The name of the makefile target for making UDA images. | never | string
unix.password | Unix password | never | string
unix.password.available | Equal 0 if the unix password if available | never | string
unix.username | Unix username. | never | string
unix.username.available | Equal 0 if the unix username if available | never | string
unsubst.after.build | Unsubsted drive after build finished. If not defined then helium should left the drive as subst. Set the value as "yes" if you want to unsubst after build finished. | allowed | string
validate.policy.csv | Location of the CSV file that defines policy IDs. | recommended | string
validate.policy.ignoreroot | Skip the validation of the given root folders. | allowed | boolean
validate.policy.log | Location validate policy xml log. | discouraged | string
validate.policy.log.xml | Location of the LogXML output file. | discouraged | string
validate.policy.pattern | Comma separated list of pattern for policy validation. Defualt value is, distribution.policy.s60,distribution.policy | allowed | string
validate.properties.at.startup | display warnings at build startup if required properties are not defined. | never | string
variant.image.targetpath | Path for copying the variant image files default is under output/variant_images | never | string
week.number | this is used to identify the history files based on releases | allowed | string
zip.config.file | Path to the the zip specification file | recommended | string
zip.config.file.parsed | Path to the parsed file of zip specification file | never | string
zip.ee.log.file | Defines log file where to record archiving of engineering english area. | never | string
zip.localised.log.file | The path to the localization zipping log file. | never | string
zip.subcon_roms.log.file | The log file name for zipping subcon_roms. | never | string
zip.subcon.log.file | Defines log file where to record archiving of subcon environment. | never | string
zip.trace_roms.log.file | The log file name for zipping trace_roms. | never | string
zip.uda_roms.log.file | The log file name for zipping uda_roms. | never | string
zip.wa.file | A unique name for the WA Sources ZIP file. | discouraged | string
zips.build.dir | This is the directory where build area is archived after the build has finished. | never | string
zips.ee.spec.name | the value should be "ee" | allowed | string
zips.flashfiles.dir | This is the directory where flash files are archived. | never | string
zips.loc.dir | This is the directory where build area is archived after the localisation. | never | string

overview | deprecated | properties-table | index | help
| Helium API
prev next | frames no frames

Copyright (c) 2009 Nokia Corporation and/or its subsidiary(-ies). All rights reserved. License: http://www.eclipse.org/legal/epl-v10.html